<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<board>
<plain>
<hole x="22.01365" y="11.9842" drill="1.9"/>
<hole x="2.01115" y="11.9842" drill="1.9"/>
<hole x="2" y="2" drill="3"/>
<hole x="22" y="2" drill="3"/>
<hole x="2" y="22" drill="3"/>
<hole x="22" y="22" drill="3"/>
<wire x1="0" y1="1.27" x2="0" y2="22.73" width="0.0762" layer="20"/>
<wire x1="0" y1="22.73" x2="1.27" y2="24" width="0.0762" layer="20" curve="-90"/>
<wire x1="1.27" y1="24" x2="22.73" y2="24" width="0.0762" layer="20"/>
<wire x1="22.73" y1="24" x2="24" y2="22.73" width="0.0762" layer="20" curve="-90"/>
<wire x1="24" y1="22.73" x2="24" y2="1.27" width="0.0762" layer="20"/>
<wire x1="24" y1="1.27" x2="22.73" y2="0" width="0.0762" layer="20" curve="-90"/>
<wire x1="22.73" y1="0" x2="1.27" y2="0" width="0.0762" layer="20"/>
<wire x1="1.27" y1="0" x2="0" y2="1.27" width="0.0762" layer="20" curve="-90"/>
<text>Robot Club KMITL
Designed in Thailand
By TinLethax (RB26)</text>
<text>ADNS5090 Optical Flow</text>
<text>+x</text>
<text>+y</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="adns_5050">
<packages>
<package name="WEIRD_DIP8">
</package>
</packages>
</library>
<library name="Wurth_Connectors_WR-PHD">
<description>&lt;BR&gt;Wurth Elektronik - Connectors - Board-to-Board Connectors - WR-PHD &lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2021a, 2021-11-04&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="61300821121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Dual Pin Header; 8 Pins</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="adns_5050" package="WEIRD_DIP8" value="ADNS5090">
<attribute name="NAME"/>
</element>
<element name="C1" library="adafruit" package="C0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="Wurth_Connectors_WR-PHD" package="61300821121" value=" 61300821121 ">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/61300821121.pdf"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="NAME"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value=" 61300821121 "/>
<attribute name="PINS" value=" 8 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Board Stacker"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="P$6"/>
<contactref element="C1" pad="2"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="SI">
<contactref element="IC1" pad="P$8"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="CLK">
<contactref element="IC1" pad="P$5"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="SO">
<contactref element="IC1" pad="P$1"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="LED_K">
<contactref element="IC1" pad="P$2"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="INT">
<contactref element="IC1" pad="P$3"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="/CS">
<contactref element="IC1" pad="P$4"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="3V3">
<contactref element="C1" pad="1"/>
<contactref element="IC1" pad="P$7"/>
<contactref element="J1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
