<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.1.0">
<drawing>
<board>
<plain>
<wire x1="30.48" y1="12.7" x2="69.85" y2="12.7" width="0" layer="20"/>
<wire x1="69.85" y1="12.7" x2="69.85" y2="54.61" width="0" layer="20"/>
<wire x1="69.85" y1="54.61" x2="30.48" y2="54.61" width="0" layer="20"/>
<wire x1="30.48" y1="54.61" x2="30.48" y2="12.7" width="0" layer="20"/>
<hole x="34.29" y="16.51" drill="3.2"/>
<hole x="66.04" y="16.51" drill="3.2"/>
<hole x="34.29" y="50.8" drill="3.2"/>
<hole x="66.04" y="50.8" drill="3.2"/>
<text>AC Relay Board</text>
</plain>
<libraries>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO41-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO18">
<description>&lt;b&gt;TO 18&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="evolviplexor">
<packages>
<package name="MOLEX4">
</package>
<package name="RELAY">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="diode" package="DO41-10" value="1N4004"/>
<element name="T1" library="transistor" package="TO18" value="2N2222">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="evolviplexor" package="MOLEX4" value="MOLEX4"/>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-12183"/>
</element>
<element name="U$2" library="evolviplexor" package="RELAY" value="RELAY"/>
</elements>
<signals>
<signal name="12V">
<contactref element="U$1" pad="P$4"/>
<contactref element="D1" pad="C"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="P$2"/>
<contactref element="U$1" pad="P$1"/>
<contactref element="T1" pad="1"/>
</signal>
<signal name="CNT">
<contactref element="U$1" pad="P$3"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$1">
<contactref element="T1" pad="3"/>
<contactref element="D1" pad="A"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="T1" pad="2"/>
<contactref element="R1" pad="P$2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
