<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="24.13" y1="52.07" x2="39.37" y2="52.07" width="0" layer="20"/>
<wire x1="39.37" y1="52.07" x2="39.37" y2="26.67" width="0" layer="20"/>
<wire x1="39.37" y1="26.67" x2="24.13" y2="26.67" width="0" layer="20"/>
<wire x1="24.13" y1="26.67" x2="24.13" y2="52.07" width="0" layer="20"/>
<text>ADP8866</text>
<text>29 Mar
2016</text>
<text>v4</text>
<text>D3</text>
<text>D2</text>
<text>D1</text>
<text>D9</text>
<text>RST</text>
<text>SCL</text>
<text>SDA</text>
<text>INT</text>
<text>C1-</text>
<text>C2-</text>
<text>C1+</text>
<text>C2+</text>
<text>Vout</text>
<text>Vin</text>
<text>GND</text>
<text>D8</text>
<text>D7</text>
<text>D6</text>
<text>D5</text>
<text>D4</text>
</plain>
<libraries>
<library name="ERIC">
<description>CDS Photoconductive Photocell.
PDV-P7002
Digikey part PDV-P7002-ND</description>
<packages>
<package name="QFN_20_4X4">
<description>20-Lead Plastic Quad Flat, No Lead Package (ML) - 4x4 mm Body [QNF]
With 0.40 mm Contact Length

page 245</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X10">
</package>
</packages>
</library>
<library name="KEMET">
<packages>
<package name="0603_B">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="ERIC" package="QFN_20_4X4" value="ADP8866"/>
<element name="C1" library="KEMET" package="0603_B" value="1u"/>
<element name="C2" library="KEMET" package="0603_B" value="1u"/>
<element name="COUT" library="KEMET" package="0603_B" value="1u"/>
<element name="CIN" library="KEMET" package="0603_B" value="1u"/>
<element name="JP1" library="SparkFun-Connectors" package="1X10" value="M10&quot;"/>
<element name="JP2" library="SparkFun-Connectors" package="1X10" value="M10&quot;"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$1" pad="12"/>
<contactref element="C2" pad="1"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="10"/>
<contactref element="C2" pad="2"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="9"/>
<contactref element="C1" pad="2"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="11"/>
<contactref element="C1" pad="1"/>
<contactref element="JP2" pad="10"/>
</signal>
<signal name="VOUT">
<contactref element="U$1" pad="13"/>
<contactref element="COUT" pad="1"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="GND">
<contactref element="COUT" pad="2"/>
<contactref element="CIN" pad="2"/>
<contactref element="U$1" pad="15"/>
<contactref element="U$1" pad="EP"/>
<contactref element="U$1" pad="15"/>
<contactref element="U$1" pad="EP"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="N$5">
<contactref element="CIN" pad="1"/>
<contactref element="U$1" pad="14"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="N$6">
<contactref element="JP1" pad="1"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="JP1" pad="2"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="JP1" pad="3"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="JP1" pad="4"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="N$10">
<contactref element="JP1" pad="5"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="N$11">
<contactref element="JP1" pad="6"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="N$12">
<contactref element="JP1" pad="7"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="N$13">
<contactref element="JP1" pad="8"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="N$14">
<contactref element="JP2" pad="5"/>
<contactref element="U$1" pad="16"/>
</signal>
<signal name="N$15">
<contactref element="JP2" pad="4"/>
<contactref element="U$1" pad="17"/>
</signal>
<signal name="N$16">
<contactref element="JP2" pad="3"/>
<contactref element="U$1" pad="18"/>
</signal>
<signal name="N$17">
<contactref element="JP2" pad="2"/>
<contactref element="U$1" pad="19"/>
</signal>
<signal name="N$18">
<contactref element="JP2" pad="1"/>
<contactref element="U$1" pad="20"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
