<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="28.57" y1="15.0875" x2="28.57" y2="29.3625" width="0" layer="20"/>
<wire x1="28.57" y1="29.3625" x2="10.8" y2="29.3625" width="0" layer="20"/>
<wire x1="10.8" y1="29.3625" x2="10.8" y2="15.0875" width="0" layer="20"/>
<wire x1="10.8" y1="15.0875" x2="28.57" y2="15.0875" width="0" layer="20"/>
<text>(C)2017 GLM REV 3b</text>
<text>-</text>
<text>LED+</text>
<text>BAT+</text>
<text>LED-</text>
<text>BAT-</text>
</plain>
<libraries>
<library name="zetex-zxld1360">
<packages>
<package name="SOT23-5L">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;&lt;p&gt;
package type OT</description>
</package>
</packages>
</library>
<library name="diode-special-packages">
<packages>
<package name="SOD123">
<description>&lt;b&gt;Diode&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="R2512">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1210">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="C0603K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0603 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1608</description>
</package>
<package name="C1210">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="inductor-power">
<packages>
<package name="DR12X">
<description>Layout for Coiltronics DR125 and 127&lt;BR&gt;
12mm sq. inductors</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="zetex-zxld1360" package="SOT23-5L" value="ZXLD1360"/>
<element name="D1" library="diode-special-packages" package="SOD123" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl" package="R1210" value="R560"/>
<element name="C2" library="rcl" package="C1210" value="4.7u 35v"/>
<element name="C3" library="rcl" package="C1206" value="1u 20v"/>
<element name="L1" library="inductor-power" package="DR12X" value="68uh DR12X"/>
<element name="LED" library="rcl" package="R2512" value="">
<attribute name="VALUE"/>
</element>
<element name="BAT" library="rcl" package="R2512" value="">
<attribute name="VALUE"/>
</element>
<element name="C1" library="rcl" package="C0603K" value="100n">
<attribute name="NAME"/>
</element>
<element name="ADJ" library="SparkFun" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND" library="SparkFun" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="+12V">
<contactref element="R1" pad="1"/>
<contactref element="IC1" pad="5"/>
<contactref element="D1" pad="K"/>
<contactref element="C2" pad="1"/>
<contactref element="BAT" pad="2"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="BAT" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="GND" pad="1"/>
</signal>
<signal name="LX">
<contactref element="IC1" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="L1" pad="P$2"/>
</signal>
<signal name="ISNS">
<contactref element="IC1" pad="4"/>
<contactref element="R1" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="LED" pad="2"/>
</signal>
<signal name="LED-">
<contactref element="C3" pad="2"/>
<contactref element="L1" pad="P$1"/>
<contactref element="LED" pad="1"/>
</signal>
<signal name="ADJ">
<contactref element="IC1" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="ADJ" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
