<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="4.1275" x2="55.5425" y2="4.1275" width="0" layer="20"/>
<wire x1="55.5425" y1="4.1275" x2="55.5425" y2="25.705" width="0" layer="20"/>
<wire x1="0" y1="25.705" x2="0" y2="4.1275" width="0" layer="20"/>
<text>Ryan Vasquez</text>
<text>PWM MOSFET Test Board
Rev. 1 5/29/14</text>
<text>PWM MOSFET 
Test Board
Rev. 1 
5/29/14</text>
<text>V+</text>
<text>V+</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>SCL</text>
<text>SCL</text>
<text>SDA</text>
<text>VCC</text>
<text>VIN</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>SCL</text>
<text>SDA</text>
<text>VIN</text>
<text>VCC</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="TSSOP28">
</package>
<package name="SOT23-W">
<description>&lt;b&gt;SOT23&lt;/b&gt; - Wave soldering</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="CPOL-RADIAL-100UF-25V">
</package>
<package name="CPOL-RADIAL-10UF-25V">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06">
</package>
<package name="1X04">
</package>
<package name="1X04_LOCK">
</package>
<package name="1X01">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="adafruit" package="TSSOP28" value=""/>
<element name="Q1" library="adafruit" package="SOT23-W" value=""/>
<element name="Q2" library="adafruit" package="SOT23-W" value=""/>
<element name="Q3" library="adafruit" package="SOT23-W" value=""/>
<element name="Q4" library="adafruit" package="SOT23-W" value=""/>
<element name="Q5" library="adafruit" package="SOT23-W" value=""/>
<element name="Q6" library="adafruit" package="SOT23-W" value=""/>
<element name="Q7" library="adafruit" package="SOT23-W" value=""/>
<element name="Q8" library="adafruit" package="SOT23-W" value=""/>
<element name="Q9" library="adafruit" package="SOT23-W" value=""/>
<element name="Q10" library="adafruit" package="SOT23-W" value=""/>
<element name="Q11" library="adafruit" package="SOT23-W" value=""/>
<element name="Q12" library="adafruit" package="SOT23-W" value=""/>
<element name="Q13" library="adafruit" package="SOT23-W" value=""/>
<element name="Q14" library="adafruit" package="SOT23-W" value=""/>
<element name="Q15" library="adafruit" package="SOT23-W" value=""/>
<element name="Q16" library="adafruit" package="SOT23-W" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="PROD_ID" value="CAP-08064"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="PROD_ID" value="CAP-08064"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="PROD_ID" value="CAP-08064"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="PROD_ID" value="CAP-08064"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="PROD_ID" value="CAP-08064"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="PROD_ID" value="CAP-08064"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="10K"/>
<element name="R3" library="SparkFun-Resistors" package="0805" value="10K"/>
<element name="R4" library="SparkFun-Resistors" package="0805" value="10K"/>
<element name="R5" library="SparkFun-Resistors" package="0805" value="10K"/>
<element name="R6" library="SparkFun-Resistors" package="0805" value="10K"/>
<element name="R7" library="SparkFun-Resistors" package="0805" value="10K"/>
<element name="C1" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value=""/>
<element name="JP3" library="SparkFun-Connectors" package="1X06" value=""/>
<element name="JP4" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0805" value="10K"/>
<element name="R9" library="SparkFun-Resistors" package="0805" value="10K"/>
<element name="JP1" library="SparkFun-Connectors" package="1X04_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X04_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="." library="SparkFun-Connectors" package="1X04_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="JP6" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="JP7" library="SparkFun-Connectors" package="1X04_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="JP8" library="SparkFun-Connectors" package="1X01" value="M01PTH"/>
<element name="C8" library="SparkFun-Capacitors" package="CPOL-RADIAL-100UF-25V" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="14"/>
<contactref element="R7" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="25"/>
<contactref element="Q9" pad="2"/>
<contactref element="Q8" pad="2"/>
<contactref element="Q7" pad="2"/>
<contactref element="Q6" pad="2"/>
<contactref element="Q5" pad="2"/>
<contactref element="Q4" pad="2"/>
<contactref element="Q11" pad="2"/>
<contactref element="Q12" pad="2"/>
<contactref element="Q13" pad="2"/>
<contactref element="Q14" pad="2"/>
<contactref element="Q15" pad="2"/>
<contactref element="Q16" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="Q10" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="JP4" pad="6"/>
<contactref element="JP3" pad="6"/>
<contactref element="Q3" pad="2"/>
<contactref element="JP4" pad="5"/>
<contactref element="JP3" pad="5"/>
<contactref element="C8" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="28"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="JP4" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="U1" pad="23"/>
</signal>
<signal name="N$2">
<contactref element="Q3" pad="3"/>
<contactref element="." pad="3"/>
</signal>
<signal name="N$5">
<contactref element="Q6" pad="3"/>
<contactref element="JP6" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="Q7" pad="3"/>
<contactref element="JP7" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="Q8" pad="3"/>
<contactref element="JP7" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="Q9" pad="3"/>
<contactref element="JP7" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="Q10" pad="3"/>
<contactref element="JP8" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="Q11" pad="3"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="Q12" pad="3"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="Q14" pad="3"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="Q15" pad="3"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="Q16" pad="3"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="N$16">
<contactref element="Q1" pad="3"/>
<contactref element="." pad="1"/>
</signal>
<signal name="N$17">
<contactref element="Q2" pad="3"/>
<contactref element="." pad="2"/>
</signal>
<signal name="PWM0">
<contactref element="U1" pad="6"/>
<contactref element="Q11" pad="1"/>
</signal>
<signal name="PWM1">
<contactref element="U1" pad="7"/>
<contactref element="Q12" pad="1"/>
</signal>
<signal name="PWM2">
<contactref element="U1" pad="8"/>
<contactref element="Q13" pad="1"/>
</signal>
<signal name="PWM3">
<contactref element="U1" pad="9"/>
<contactref element="Q14" pad="1"/>
</signal>
<signal name="PWM4">
<contactref element="U1" pad="10"/>
<contactref element="Q15" pad="1"/>
</signal>
<signal name="PWM5">
<contactref element="U1" pad="11"/>
<contactref element="Q16" pad="1"/>
</signal>
<signal name="PWM6">
<contactref element="U1" pad="12"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="PWM7">
<contactref element="U1" pad="13"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="PWM8">
<contactref element="U1" pad="15"/>
<contactref element="Q3" pad="1"/>
</signal>
<signal name="PWM9">
<contactref element="U1" pad="16"/>
<contactref element="Q4" pad="1"/>
</signal>
<signal name="PWM10">
<contactref element="U1" pad="17"/>
<contactref element="Q5" pad="1"/>
</signal>
<signal name="PWM11">
<contactref element="U1" pad="18"/>
<contactref element="Q6" pad="1"/>
</signal>
<signal name="PWM12">
<contactref element="U1" pad="19"/>
<contactref element="Q7" pad="1"/>
</signal>
<signal name="PWM13">
<contactref element="U1" pad="20"/>
<contactref element="Q8" pad="1"/>
</signal>
<signal name="PWM14">
<contactref element="U1" pad="21"/>
<contactref element="Q9" pad="1"/>
</signal>
<signal name="PWM15">
<contactref element="U1" pad="22"/>
<contactref element="Q10" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="U1" pad="27"/>
<contactref element="JP4" pad="3"/>
<contactref element="JP3" pad="3"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="U1" pad="26"/>
<contactref element="JP4" pad="4"/>
<contactref element="JP3" pad="4"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="U1" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="U1" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="U1" pad="3"/>
<contactref element="R5" pad="2"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="U1" pad="4"/>
<contactref element="R4" pad="2"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="U1" pad="5"/>
<contactref element="R3" pad="2"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="U1" pad="24"/>
<contactref element="C7" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="+12V">
<contactref element="JP4" pad="2"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP1" pad="4"/>
<contactref element="JP2" pad="4"/>
<contactref element="." pad="4"/>
<contactref element="JP6" pad="4"/>
<contactref element="JP7" pad="4"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="JP1" pad="3"/>
<contactref element="Q13" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="Q4" pad="3"/>
<contactref element="JP6" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="JP6" pad="2"/>
<contactref element="Q5" pad="3"/>
</signal>
<signal name="N$28">
</signal>
<signal name="N$30">
</signal>
<signal name="N$39">
</signal>
<signal name="N$1">
</signal>
<signal name="N$4">
</signal>
<signal name="N$12">
</signal>
<signal name="N$29">
</signal>
<signal name="N$32">
</signal>
</signals>
</board>
</drawing>
</eagle>
