<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.0">
<drawing>
<board>
<plain>
<wire x1="13.97" y1="11.43" x2="13.97" y2="66.04" width="0.1524" layer="20"/>
<wire x1="13.97" y1="66.04" x2="17.78" y2="69.85" width="0.1524" layer="20"/>
<wire x1="17.78" y1="69.85" x2="68.58" y2="69.85" width="0.1524" layer="20"/>
<wire x1="68.58" y1="69.85" x2="71.12" y2="67.31" width="0.1524" layer="20"/>
<wire x1="71.12" y1="67.31" x2="71.12" y2="11.43" width="0.1524" layer="20"/>
<wire x1="71.12" y1="11.43" x2="68.58" y2="8.89" width="0.1524" layer="20"/>
<wire x1="68.58" y1="8.89" x2="16.51" y2="8.89" width="0.1524" layer="20"/>
<wire x1="16.51" y1="8.89" x2="13.97" y2="11.43" width="0.1524" layer="20"/>
<text>GND</text>
<text>+3v</text>
<text>SIG</text>
<text>S0 S1 S2 S3</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206">
<description>&lt;h3&gt;LED 1206 SMT&lt;/h3&gt;

1206, surface mount. 

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: &lt;/li&gt;
&lt;li&gt;Area: 0.125" x 0.06"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-IC-Logic">
<description>&lt;h3&gt;SparkFun Logic ICs&lt;/h3&gt;
This library contains parts which fit into the standard logic IC families.&lt;br&gt;&lt;br&gt;
This library is special as the devices are most generalized, with manufacturer specific variants stemming from the generalized numbers.  It also uses individual gates for common parts with a power consort.  Place the gates in a schematic such that they are easy to see in the circuit, and apply power to the power symbol for multigate packages. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SSOP24">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CTRL" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
</element>
<element name="D1" library="SparkFun-LED" package="LED-1206" value="RED">
<attribute name="PROD_ID" value="DIO-09912"/>
</element>
<element name="D10" library="SparkFun-LED" package="LED-1206" value="RED">
<attribute name="PROD_ID" value="DIO-09912"/>
</element>
<element name="D11" library="SparkFun-LED" package="LED-1206" value="RED">
<attribute name="PROD_ID" value="DIO-09912"/>
</element>
<element name="D12" library="SparkFun-LED" package="LED-1206" value="RED">
<attribute name="PROD_ID" value="DIO-09912"/>
</element>
<element name="D13" library="SparkFun-LED" package="LED-1206" value="RED">
<attribute name="PROD_ID" value="DIO-09912"/>
</element>
<element name="D14" library="SparkFun-LED" package="LED-1206" value="RED">
<attribute name="PROD_ID" value="DIO-09912"/>
</element>
<element name="D15" library="SparkFun-LED" package="LED-1206" value="GREEN">
<attribute name="PROD_ID" value="DIO-00862"/>
</element>
<element name="D16" library="SparkFun-LED" package="LED-1206" value="GREEN">
<attribute name="PROD_ID" value="DIO-00862"/>
</element>
<element name="D2" library="SparkFun-LED" package="LED-1206" value="RED">
<attribute name="PROD_ID" value="DIO-09912"/>
</element>
<element name="D3" library="SparkFun-LED" package="LED-1206" value="RED">
<attribute name="PROD_ID" value="DIO-09912"/>
</element>
<element name="D4" library="SparkFun-LED" package="LED-1206" value="RED">
<attribute name="PROD_ID" value="DIO-09912"/>
</element>
<element name="D5" library="SparkFun-LED" package="LED-1206" value="RED">
<attribute name="PROD_ID" value="DIO-09912"/>
</element>
<element name="D6" library="SparkFun-LED" package="LED-1206" value="RED">
<attribute name="PROD_ID" value="DIO-09912"/>
</element>
<element name="D7" library="SparkFun-LED" package="LED-1206" value="RED">
<attribute name="PROD_ID" value="DIO-09912"/>
</element>
<element name="D8" library="SparkFun-LED" package="LED-1206" value="RED">
<attribute name="PROD_ID" value="DIO-09912"/>
</element>
<element name="D9" library="SparkFun-LED" package="LED-1206" value="RED">
<attribute name="PROD_ID" value="DIO-09912"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="200">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R10" library="SparkFun-Resistors" package="0805" value="200">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R11" library="SparkFun-Resistors" package="0805" value="200">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R12" library="SparkFun-Resistors" package="0805" value="200">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R13" library="SparkFun-Resistors" package="0805" value="200">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R14" library="SparkFun-Resistors" package="0805" value="200">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R15" library="SparkFun-Resistors" package="0805" value="200">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R16" library="SparkFun-Resistors" package="0805" value="200">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="200">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="200">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="200">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0805" value="200">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0805" value="200">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0805" value="200">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0805" value="200">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0805" value="200">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="MUX" library="SparkFun-IC-Logic" package="SSOP24" value="CD74HC4067SM96">
<attribute name="PROD_ID" value="IC-08252"/>
</element>
<element name="POWER" library="SparkFun-Connectors" package="1X03" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="D1" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="D2" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="D3" pad="A"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="D4" pad="A"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="D5" pad="A"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="D6" pad="A"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="D7" pad="A"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="D15" pad="A"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="D9" pad="A"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="D10" pad="A"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="D11" pad="A"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="D12" pad="A"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="D13" pad="A"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="D14" pad="A"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="D8" pad="A"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="D16" pad="A"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="R1" pad="2"/>
<contactref element="MUX" pad="9"/>
</signal>
<signal name="N$18">
<contactref element="MUX" pad="8"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="MUX" pad="7"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="MUX" pad="6"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="MUX" pad="5"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="MUX" pad="4"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="MUX" pad="3"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="MUX" pad="2"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="MUX" pad="23"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$26">
<contactref element="MUX" pad="16"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="MUX" pad="17"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="N$28">
<contactref element="MUX" pad="18"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="MUX" pad="19"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$30">
<contactref element="MUX" pad="20"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$31">
<contactref element="MUX" pad="21"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$32">
<contactref element="MUX" pad="22"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="GND">
<contactref element="D1" pad="C"/>
<contactref element="D2" pad="C"/>
<contactref element="D3" pad="C"/>
<contactref element="D4" pad="C"/>
<contactref element="D5" pad="C"/>
<contactref element="D6" pad="C"/>
<contactref element="D7" pad="C"/>
<contactref element="D15" pad="C"/>
<contactref element="D9" pad="C"/>
<contactref element="D10" pad="C"/>
<contactref element="D11" pad="C"/>
<contactref element="D12" pad="C"/>
<contactref element="D13" pad="C"/>
<contactref element="D14" pad="C"/>
<contactref element="D8" pad="C"/>
<contactref element="D16" pad="C"/>
<contactref element="POWER" pad="3"/>
<contactref element="MUX" pad="12"/>
</signal>
<signal name="S0">
<contactref element="CTRL" pad="1"/>
<contactref element="MUX" pad="10"/>
</signal>
<signal name="S1">
<contactref element="CTRL" pad="2"/>
<contactref element="MUX" pad="11"/>
</signal>
<signal name="S2">
<contactref element="CTRL" pad="3"/>
<contactref element="MUX" pad="14"/>
</signal>
<signal name="S3">
<contactref element="CTRL" pad="4"/>
<contactref element="MUX" pad="13"/>
</signal>
<signal name="VCC">
<contactref element="POWER" pad="1"/>
<contactref element="MUX" pad="24"/>
</signal>
<signal name="SIG">
<contactref element="POWER" pad="2"/>
<contactref element="MUX" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
