<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<board>
<plain>
<wire x1="24.13" y1="26.67" x2="44.45" y2="26.67" width="0.1524" layer="20"/>
<wire x1="44.45" y1="26.67" x2="44.45" y2="6.35" width="0.1524" layer="20"/>
<wire x1="44.45" y1="6.35" x2="24.13" y2="6.35" width="0.1524" layer="20"/>
<wire x1="24.13" y1="6.35" x2="24.13" y2="26.67" width="0.1524" layer="20"/>
<text>DAT2</text>
<text>CS</text>
<text>MOSI</text>
<text>3v3</text>
<text>SCL</text>
<text>GND</text>
<text>MISO</text>
<text>DATA1</text>
<text>GND1</text>
<text>GND2</text>
<text>GND3</text>
<text>GND4</text>
<text>SW</text>
<text>DM3CS</text>
<text>v1</text>
<text>27Mar18</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08_PIN1_NO_SILK">
</package>
</packages>
</library>
<library name="Hirose">
<packages>
<package name="DM3CS">
<description>DM3CS hinged micro sd card holder</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="1X08_PIN1_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X08_PIN1_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="Hirose" package="DM3CS" value="MICRO_SD_DM3CS"/>
</elements>
<signals>
<signal name="DAT2">
<contactref element="U$1" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="CS">
<contactref element="U$1" pad="2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="U$1" pad="3"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="3V3">
<contactref element="U$1" pad="4"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="SCL">
<contactref element="U$1" pad="5"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="6"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="MISO">
<contactref element="U$1" pad="7"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="DAT1">
<contactref element="U$1" pad="8"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="GND1">
<contactref element="U$1" pad="GND1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="GND2">
<contactref element="U$1" pad="GND2"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="GND3">
<contactref element="U$1" pad="GND3"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="GND4">
<contactref element="U$1" pad="GND4"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="SW">
<contactref element="U$1" pad="SW"/>
<contactref element="J2" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
