<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="19.05" y1="30.48" x2="31.75" y2="30.48" width="0.254" layer="20"/>
<wire x1="31.75" y1="30.48" x2="31.75" y2="20.32" width="0.254" layer="20"/>
<wire x1="31.75" y1="20.32" x2="19.05" y2="20.32" width="0.254" layer="20"/>
<wire x1="19.05" y1="20.32" x2="19.05" y2="30.48" width="0.254" layer="20"/>
<text>CAT4238</text>
<text>LED Driver</text>
<text>v1</text>
<text>24Jan19</text>
<text>VIN</text>
<text>SHDN</text>
<text>FB</text>
<text>GND</text>
<text>SW</text>
<wire x1="34.29" y1="30.48" x2="46.99" y2="30.48" width="0.254" layer="20"/>
<wire x1="46.99" y1="30.48" x2="46.99" y2="20.32" width="0.254" layer="20"/>
<wire x1="46.99" y1="20.32" x2="34.29" y2="20.32" width="0.254" layer="20"/>
<wire x1="34.29" y1="20.32" x2="34.29" y2="30.48" width="0.254" layer="20"/>
<text>CAT4238</text>
<text>LED Driver</text>
<text>v1</text>
<text>24Jan19</text>
<text>VIN</text>
<text>SHDN</text>
<text>FB</text>
<text>GND</text>
<text>SW</text>
<wire x1="19.05" y1="17.78" x2="31.75" y2="17.78" width="0.254" layer="20"/>
<wire x1="31.75" y1="17.78" x2="31.75" y2="7.62" width="0.254" layer="20"/>
<wire x1="31.75" y1="7.62" x2="19.05" y2="7.62" width="0.254" layer="20"/>
<wire x1="19.05" y1="7.62" x2="19.05" y2="17.78" width="0.254" layer="20"/>
<text>CAT4238</text>
<text>LED Driver</text>
<text>v1</text>
<text>24Jan19</text>
<text>VIN</text>
<text>SHDN</text>
<text>FB</text>
<text>GND</text>
<text>SW</text>
<wire x1="34.29" y1="17.78" x2="46.99" y2="17.78" width="0.254" layer="20"/>
<wire x1="46.99" y1="17.78" x2="46.99" y2="7.62" width="0.254" layer="20"/>
<wire x1="46.99" y1="7.62" x2="34.29" y2="7.62" width="0.254" layer="20"/>
<wire x1="34.29" y1="7.62" x2="34.29" y2="17.78" width="0.254" layer="20"/>
<text>CAT4238</text>
<text>LED Driver</text>
<text>v1</text>
<text>24Jan19</text>
<text>VIN</text>
<text>SHDN</text>
<text>FB</text>
<text>GND</text>
<text>SW</text>
<wire x1="16.51" y1="33.02" x2="49.53" y2="33.02" width="0.381" layer="20"/>
<wire x1="49.53" y1="33.02" x2="49.53" y2="5.08" width="0.381" layer="20"/>
<wire x1="49.53" y1="5.08" x2="16.51" y2="5.08" width="0.381" layer="20"/>
<wire x1="16.51" y1="5.08" x2="16.51" y2="33.02" width="0.381" layer="20"/>
<wire x1="11.43" y1="38.1" x2="54.61" y2="38.1" width="0.381" layer="20"/>
<wire x1="54.61" y1="38.1" x2="54.61" y2="0" width="0.381" layer="20"/>
<wire x1="54.61" y1="0" x2="11.43" y2="0" width="0.381" layer="20"/>
<wire x1="11.43" y1="0" x2="11.43" y2="38.1" width="0.381" layer="20"/>
</plain>
<libraries>
<library name="ONSEMI">
<packages>
<package name="SOT23(OT)">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03_NO_SILK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED1" library="ONSEMI" package="SOT23(OT)" value="CAT4238"/>
<element name="J1" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="LED4" library="ONSEMI" package="SOT23(OT)" value="CAT4238"/>
<element name="J7" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J8" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="LED3" library="ONSEMI" package="SOT23(OT)" value="CAT4238"/>
<element name="J5" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="LED6" library="ONSEMI" package="SOT23(OT)" value="CAT4238"/>
<element name="J11" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J12" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="SW">
<contactref element="J2" pad="1"/>
<contactref element="LED1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="J2" pad="2"/>
<contactref element="LED1" pad="2"/>
</signal>
<signal name="FB">
<contactref element="J2" pad="3"/>
<contactref element="LED1" pad="3"/>
</signal>
<signal name="VIN">
<contactref element="J1" pad="1"/>
<contactref element="LED1" pad="5"/>
</signal>
<signal name="SHTDN">
<contactref element="J1" pad="3"/>
<contactref element="LED1" pad="4"/>
</signal>
<signal name="SW3">
<contactref element="J8" pad="1"/>
<contactref element="LED4" pad="1"/>
</signal>
<signal name="GND3">
<contactref element="J8" pad="2"/>
<contactref element="LED4" pad="2"/>
</signal>
<signal name="FB3">
<contactref element="J8" pad="3"/>
<contactref element="LED4" pad="3"/>
</signal>
<signal name="VIN3">
<contactref element="J7" pad="1"/>
<contactref element="LED4" pad="5"/>
</signal>
<signal name="SHTDN3">
<contactref element="J7" pad="3"/>
<contactref element="LED4" pad="4"/>
</signal>
<signal name="SW2">
<contactref element="J6" pad="1"/>
<contactref element="LED3" pad="1"/>
</signal>
<signal name="GND2">
<contactref element="J6" pad="2"/>
<contactref element="LED3" pad="2"/>
</signal>
<signal name="FB2">
<contactref element="J6" pad="3"/>
<contactref element="LED3" pad="3"/>
</signal>
<signal name="VIN2">
<contactref element="J5" pad="1"/>
<contactref element="LED3" pad="5"/>
</signal>
<signal name="SHTDN2">
<contactref element="J5" pad="3"/>
<contactref element="LED3" pad="4"/>
</signal>
<signal name="SW5">
<contactref element="J12" pad="1"/>
<contactref element="LED6" pad="1"/>
</signal>
<signal name="GND5">
<contactref element="J12" pad="2"/>
<contactref element="LED6" pad="2"/>
</signal>
<signal name="FB5">
<contactref element="J12" pad="3"/>
<contactref element="LED6" pad="3"/>
</signal>
<signal name="VIN5">
<contactref element="J11" pad="1"/>
<contactref element="LED6" pad="5"/>
</signal>
<signal name="SHTDN5">
<contactref element="J11" pad="3"/>
<contactref element="LED6" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
