<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="13.3225" x2="0" y2="1.27" width="0" layer="20"/>
<wire x1="0" y1="1.27" x2="1.27" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="0" x2="27.285" y2="0" width="0" layer="20"/>
<wire x1="27.285" y1="0" x2="28.555" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="28.555" y1="1.27" x2="28.555" y2="13.3225" width="0" layer="20"/>
<wire x1="28.555" y1="13.3225" x2="27.285" y2="14.5925" width="0" layer="20" curve="90"/>
<wire x1="27.285" y1="14.5925" x2="1.27" y2="14.5925" width="0" layer="20"/>
<wire x1="1.27" y1="14.5925" x2="0" y2="13.3225" width="0" layer="20" curve="90"/>
<text>2 GND 1</text>
<text>Pin 1</text>
<text>1 VCC 2</text>
<text>Create a solder bridge across the left two
pins in each row on J3 to connect VCC to
J2 pin 1 and GND to J2 pin 2. Solder bridge
acoss the right two pins in each row of J3 to
connect GND to J2 pin 1 and VCC to J2 pin 2.</text>
<text>SCL SDA</text>
<text>J2</text>
<text>Pi OLED
Adapter v1.0</text>
<text>Pin 1</text>
<text>1 GND 2</text>
<text>2 VCC 1</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X10">
<description>&lt;h3&gt;Plated Through Hole - 2x10&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:20&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_10x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3">
<description>&lt;h3&gt;Plated Through Hole - 2x3&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J2" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="2X10" value=""/>
<element name="J3" library="SparkFun-Connectors" package="2X3" value="">
<attribute name="PROD_ID" value="CONN-11566"/>
</element>
</elements>
<signals>
<signal name="N$4">
<contactref element="J2" pad="3"/>
<contactref element="J4" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="J2" pad="4"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="J3" pad="4"/>
<contactref element="J4" pad="9"/>
</signal>
<signal name="N$2">
<contactref element="J3" pad="3"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="J3" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="J3" pad="6"/>
</signal>
<signal name="N$5">
<contactref element="J3" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="J3" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
