<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="50.47" y2="0" width="0" layer="20"/>
<wire x1="50.47" y1="0" x2="50.47" y2="50.79" width="0" layer="20"/>
<wire x1="50.47" y1="50.79" x2="0" y2="50.79" width="0" layer="20"/>
<wire x1="0" y1="50.79" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-100UF-25V">
</package>
</packages>
</library>
<library name="st-microelectronics">
<description>&lt;b&gt;ST Microelectronics Devices&lt;/b&gt;&lt;p&gt;
Microcontrollers,  I2C components, linear devices&lt;p&gt;
http://www.st.com&lt;p&gt;
&lt;i&gt;Include st-microelectronics-2.lbr, st-microelectronics-3.lbr.&lt;p&gt;&lt;/i&gt;

&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3-NS">
</package>
</packages>
</library>
<library name="special">
<description>&lt;b&gt;Special Devices&lt;/b&gt;&lt;p&gt;
7-segment displays, switches, heatsinks, crystals, transformers, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="Q">
<description>&lt;B&gt;CRYSTAL&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="PJ-102A">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="CPOL-RADIAL-100UF-25V" value=""/>
<element name="C2" library="SparkFun-Capacitors" package="CPOL-RADIAL-100UF-25V" value=""/>
<element name="IC1" library="st-microelectronics" package="DIL16" value="L293D">
<attribute name="MPN" value="L293D"/>
<attribute name="OC_NEWARK" value="56P8249"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9589619"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="2X3-NS" value="AVR_SPI_PRG_6NS"/>
<element name="Q1" library="special" package="Q" value=""/>
<element name="U$1" library="adafruit" package="PJ-102A" value="2.1MMJACKTHM"/>
<element name="U$2" library="adafruit" package="PJ-102A" value="2.1MMJACKTHM"/>
<element name="U1" library="SparkFun-DigitalIC" package="TQFP32-08" value="ATMEGA328P_TQFP">
<attribute name="PROD_ID" value="IC-09069"/>
</element>
<element name="JP2" library="pinhead" package="1X02" value=""/>
<element name="JP3" library="pinhead" package="1X02" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="5"/>
<contactref element="JP1" pad="6"/>
<contactref element="U$1" pad="RING_SW"/>
<contactref element="U$1" pad="RING"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="13"/>
<contactref element="IC1" pad="12"/>
<contactref element="U$2" pad="RING_SW"/>
<contactref element="U$2" pad="RING"/>
<contactref element="IC1" pad="5"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="TIP"/>
<contactref element="U1" pad="20"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="18"/>
<contactref element="JP1" pad="2"/>
<contactref element="IC1" pad="16"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="MISO">
<contactref element="JP1" pad="1"/>
<contactref element="U1" pad="16"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="JP1" pad="5"/>
<contactref element="U1" pad="29"/>
</signal>
<signal name="SCK">
<contactref element="JP1" pad="3"/>
<contactref element="U1" pad="17"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="JP1" pad="4"/>
<contactref element="U1" pad="15"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$3">
<contactref element="U$2" pad="TIP"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="3-4ENABLE">
<contactref element="U1" pad="14"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="3A">
<contactref element="U1" pad="13"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="4A">
<contactref element="U1" pad="12"/>
<contactref element="IC1" pad="14"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="11"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="JP3" pad="1"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="N$1">
<contactref element="JP2" pad="2"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="JP2" pad="1"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="7"/>
<contactref element="Q1" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="8"/>
<contactref element="Q1" pad="2"/>
<contactref element="C2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
