<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.7.1">
<drawing>
<board>
<plain>
<wire x1="1.27" y1="0" x2="13.97" y2="0" width="0" layer="20"/>
<wire x1="15.24" y1="1.27" x2="15.24" y2="8.89" width="0" layer="20"/>
<wire x1="13.97" y1="10.16" x2="1.27" y2="10.16" width="0" layer="20"/>
<wire x1="0" y1="8.89" x2="0" y2="1.27" width="0" layer="20"/>
<wire x1="0" y1="8.89" x2="1.27" y2="10.16" width="0" layer="20" curve="-90"/>
<wire x1="13.97" y1="10.16" x2="15.24" y2="8.89" width="0" layer="20" curve="-90"/>
<wire x1="15.24" y1="1.27" x2="13.97" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="1.27" y1="0" x2="0" y2="1.27" width="0" layer="20" curve="-90"/>
<text>1nF</text>
<text>100nF</text>
<text>MISO</text>
<text>SCL
SCK</text>
<text>MOSI
SDA</text>
<text>CS</text>
<text>RST</text>
<text>EOC</text>
<text>GND</text>
<text>+3.3V</text>
<text>Honeywell
MPR</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04_LOCK">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin Locking Footprint&lt;/h3&gt;
Pins are offset 0.005" from center to lock pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="honeywell">
<packages>
<package name="MPR-ABS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0603" value="1nF">
<attribute name="PROD_ID" value="CAP-07886"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="PROD_ID" value="CAP-08604"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X04_LOCK" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X04_LOCK" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="honeywell" package="MPR-ABS" value="MPRLS0025PA">
<attribute name="MAX_PRESSURE" value="25 psi"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="U1" pad="P$6"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="P$4"/>
</signal>
<signal name="CS">
<contactref element="J1" pad="1"/>
<contactref element="U1" pad="P$1"/>
</signal>
<signal name="MOSI/SDA">
<contactref element="U1" pad="P$2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="SCL/SCK">
<contactref element="J1" pad="3"/>
<contactref element="U1" pad="P$3"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="P$7"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="EOC">
<contactref element="U1" pad="P$8"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="RES">
<contactref element="J2" pad="4"/>
<contactref element="U1" pad="P$9"/>
</signal>
<signal name="VDD">
<contactref element="U1" pad="P$12"/>
<contactref element="C2" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="P$10"/>
<contactref element="C2" pad="2"/>
<contactref element="J2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
