<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<text>GND</text>
<text>ZZZZT</text>
<text>FadeCandy</text>
<text>There are three states of being. Not
 knowing, action and completion.
Accept that everything is a draft. It helps
 to get it done.
There is no editing stage.
Pretending you know what you're doing
 is almost the same as knowing what
 you are doing, so just accept that you
 know what you're doing even if you
 don't and do it.
Banish procrastination. If you wait more
 than a week to get an idea done,
 abandon it.
The point of being done is not to finish
 but to get other things done.
Once you're done you can throw it
 away.
Laugh at perfection. It's boring and
 keeps you from being done.
People without dirty hands are wrong.
 Doing something makes you right.
Failure counts as done. So do mistakes.
Destruction is a variant of done.
If you have an idea and publish it on the
 internet, that counts as a ghost of
 done.
Done is the engine of more.</text>
<wire x1="2.54" y1="104.14" x2="2.54" y2="-12.7" width="1.4224" layer="20"/>
<wire x1="2.54" y1="-12.7" x2="95.25" y2="-12.7" width="1.4224" layer="20"/>
<wire x1="95.25" y1="-12.7" x2="95.25" y2="104.14" width="1.4224" layer="20"/>
<wire x1="95.25" y1="104.14" x2="2.54" y2="104.14" width="1.4224" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08">
</package>
<package name="BANANA_CONN">
</package>
</packages>
</library>
<library name="OSTOQ035450">
<packages>
<package name="OSTOQ035450">
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2,8">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 2.8 mm with drill center</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="1X08" value=""/>
<element name="JP2" library="SparkFun-Connectors" package="1X08" value=""/>
<element name="U$1" library="OSTOQ035450" package="OSTOQ035450" value="OSTOQ035450"/>
<element name="U$2" library="OSTOQ035450" package="OSTOQ035450" value="OSTOQ035450"/>
<element name="U$3" library="OSTOQ035450" package="OSTOQ035450" value="OSTOQ035450"/>
<element name="U$4" library="OSTOQ035450" package="OSTOQ035450" value="OSTOQ035450"/>
<element name="U$5" library="OSTOQ035450" package="OSTOQ035450" value="OSTOQ035450"/>
<element name="U$6" library="OSTOQ035450" package="OSTOQ035450" value="OSTOQ035450"/>
<element name="U$7" library="OSTOQ035450" package="OSTOQ035450" value="OSTOQ035450"/>
<element name="U$8" library="OSTOQ035450" package="OSTOQ035450" value="OSTOQ035450"/>
<element name="FAT_VCC" library="SparkFun-Connectors" package="BANANA_CONN" value=""/>
<element name="FAT_GND" library="SparkFun-Connectors" package="BANANA_CONN" value=""/>
<element name="H1" library="holes" package="2,8" value="MOUNT-HOLE2.8"/>
<element name="H2" library="holes" package="2,8" value="MOUNT-HOLE2.8"/>
<element name="H3" library="holes" package="2,8" value="MOUNT-HOLE2.8"/>
<element name="H4" library="holes" package="2,8" value="MOUNT-HOLE2.8"/>
</elements>
<signals>
<signal name="GND">
<contactref element="JP1" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP1" pad="3"/>
<contactref element="JP1" pad="4"/>
<contactref element="JP1" pad="5"/>
<contactref element="JP1" pad="6"/>
<contactref element="JP1" pad="7"/>
<contactref element="JP1" pad="8"/>
<contactref element="FAT_GND" pad="P$1"/>
<contactref element="U$1" pad="GND"/>
<contactref element="U$2" pad="GND"/>
<contactref element="U$3" pad="GND"/>
<contactref element="U$4" pad="GND"/>
<contactref element="U$5" pad="GND"/>
<contactref element="U$6" pad="GND"/>
<contactref element="U$7" pad="GND"/>
<contactref element="U$8" pad="GND"/>
</signal>
<signal name="FAT_VCC">
<contactref element="FAT_VCC" pad="P$1"/>
<contactref element="U$1" pad="VCC"/>
<contactref element="U$2" pad="VCC"/>
<contactref element="U$3" pad="VCC"/>
<contactref element="U$4" pad="VCC"/>
<contactref element="U$5" pad="VCC"/>
<contactref element="U$6" pad="VCC"/>
<contactref element="U$7" pad="VCC"/>
<contactref element="U$8" pad="VCC"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="DATA"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$2" pad="DATA"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U$3" pad="DATA"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="U$4" pad="DATA"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="U$5" pad="DATA"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="U$6" pad="DATA"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="N$7">
<contactref element="U$7" pad="DATA"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="N$8">
<contactref element="U$8" pad="DATA"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="N$12">
</signal>
<signal name="N$13">
</signal>
<signal name="N$14">
</signal>
<signal name="N$16">
</signal>
</signals>
</board>
</drawing>
</eagle>
