<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<board>
<plain>
<wire x1="42.672" y1="7.3531625" x2="42.672" y2="20.7138375" width="0.1524" layer="20"/>
<wire x1="42.672" y1="20.7138375" x2="41.1608375" y2="22.225" width="0.1524" layer="20" curve="90"/>
<wire x1="41.1608375" y1="22.225" x2="2.2731625" y2="22.225" width="0.1524" layer="20"/>
<wire x1="2.2731625" y1="22.225" x2="0.762" y2="20.7138375" width="0.1524" layer="20" curve="90"/>
<wire x1="0.762" y1="20.7138375" x2="0.762" y2="7.553603125" width="0.1524" layer="20"/>
<wire x1="0.762" y1="7.553603125" x2="2.473603125" y2="5.842" width="0.1524" layer="20" curve="90"/>
<wire x1="2.473603125" y1="5.842" x2="41.1608375" y2="5.842" width="0.1524" layer="20"/>
<wire x1="41.1608375" y1="5.842" x2="42.672" y2="7.3531625" width="0.1524" layer="20" curve="90"/>
<text>3A Maximum</text>
<text>RV-Project.Com RGB Suppressor LSB-3A</text>
<text>+12V
</text>
<text>R</text>
<text>G</text>
<text>B</text>
<text>B</text>
<text>G</text>
<text>R</text>
<text>+12V
</text>
<text>V3.0 12-8-17</text>
<text>Pins are straight through so color order does not matter.</text>
<text>W</text>
<text>W</text>
</plain>
<libraries>
<library name="a-lib">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="BIGFOOT_SMALL">
</package>
<package name="D041-3.5MIL">
</package>
<package name="251SMALL">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X05">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LOGO1" library="a-lib" package="BIGFOOT_SMALL" value="CLIPART_LOGOBIGFOOT_SMALL"/>
<element name="LOGO2" library="a-lib" package="BIGFOOT_SMALL" value="CLIPART_LOGOBIGFOOT_SMALL"/>
<element name="D1" library="a-lib" package="D041-3.5MIL" value="TVS-SD041"/>
<element name="D2" library="a-lib" package="D041-3.5MIL" value="TVS-SD041"/>
<element name="D3" library="a-lib" package="D041-3.5MIL" value="TVS-SD041"/>
<element name="F1" library="a-lib" package="251SMALL" value="">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X05" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X05" value="">
<attribute name="VALUE"/>
</element>
<element name="D4" library="a-lib" package="D041-3.5MIL" value="TVS-SD041"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="D1" pad="C"/>
<contactref element="D3" pad="C"/>
<contactref element="F1" pad="P$2"/>
<contactref element="D4" pad="C"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="N$2">
<contactref element="F1" pad="P$1"/>
<contactref element="JP1" pad="5"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="D1" pad="A"/>
<contactref element="JP1" pad="4"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="D2" pad="A"/>
<contactref element="JP1" pad="3"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="D3" pad="A"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="GND">
</signal>
<signal name="N$6">
<contactref element="JP2" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="D4" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
