<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="54.854" x2="0" y2="-0.762" width="0" layer="20"/>
<wire x1="0" y1="-0.762" x2="1.27" y2="-2.032" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="-2.032" x2="74.854" y2="-2.032" width="0" layer="20"/>
<wire x1="74.854" y1="-2.032" x2="76.124" y2="-0.762" width="0" layer="20" curve="90"/>
<wire x1="76.124" y1="-0.762" x2="76.124" y2="55.13273125" width="0" layer="20"/>
<wire x1="76.124" y1="55.13273125" x2="74.85333125" y2="56.124" width="0" layer="20" curve="90.030171"/>
<wire x1="74.85333125" y1="56.124" x2="45.974465625" y2="56.124" width="0" layer="20"/>
<wire x1="45.974465625" y1="56.124" x2="44.704" y2="54.863534375" width="0" layer="20" curve="89.851201"/>
<wire x1="44.704" y1="54.863534375" x2="44.704" y2="48.768" width="0" layer="20"/>
<wire x1="44.704" y1="48.768" x2="43.434" y2="47.498" width="0" layer="20" curve="-90"/>
<wire x1="43.434" y1="47.498" x2="38.1" y2="47.498" width="0" layer="20"/>
<wire x1="38.1" y1="47.498" x2="36.83" y2="48.768" width="0" layer="20" curve="-90"/>
<wire x1="36.83" y1="48.768" x2="36.83" y2="54.854" width="0" layer="20"/>
<wire x1="36.83" y1="54.854" x2="35.56" y2="56.124" width="0" layer="20" curve="90"/>
<wire x1="35.56" y1="56.124" x2="1.27" y2="56.124" width="0" layer="20"/>
<wire x1="1.27" y1="56.124" x2="0" y2="54.854" width="0" layer="20" curve="90"/>
<text>GND</text>
<text>Duct LED</text>
<text>GND</text>
<text>3V3</text>
<text>D/C</text>
<text>COM</text>
<text>3</text>
<text>2</text>
<text>1</text>
<text>1</text>
<text>2</text>
<text>4</text>
<text>5VDC, 5.5mm OD
2.1mm ID Jack
Center Positive</text>
<text>Rev.1.6</text>
<text>Humidifier
Controller
CvW 2016</text>
<text>Rev. 1.6</text>
<text>GND</text>
<text>5V</text>
<text>D/C</text>
<text>4</text>
<text>3</text>
<text>Common</text>
<text>HUM4</text>
<text>HUM3</text>
<text>HUM2</text>
<text>HUM1</text>
<text>ACS711</text>
<text>VIN</text>
<text>Ultra</text>
<text>Water</text>
<text>SSR</text>
<text>GND</text>
<text>3V3</text>
<text>VIN</text>
<text>Humidifier Zone #</text>
<text>AREF</text>
<text>24VAC</text>
<text>Ultrasonic</text>
<text>Water Valve</text>
<text>LED</text>
<text>LED</text>
<text>DCS</text>
<text>DCS</text>
<text>SCK</text>
<text>SCK</text>
<text>SCK</text>
<text>SCK</text>
<text>SDO</text>
<text>SDO</text>
<text>SDO</text>
<text>SDO</text>
<text>SDI</text>
<text>SDI</text>
<text>SDI</text>
<text>SDI</text>
<text>TCS</text>
<text>TCS</text>
<text>SCK</text>
<text>SCK</text>
<text>DCS</text>
<text>DCS</text>
<text>D/C</text>
<text>D/C</text>
<text>TCS</text>
<text>TCS</text>
<text>SDO</text>
<text>SDO</text>
<text>SDI</text>
<text>SDI</text>
<text>HUM4</text>
<text>HUM3</text>
<text>HUM2</text>
<text>HUM1</text>
<text>Water</text>
<text>Ultra</text>
<text>GND</text>
<text>5V</text>
<text>ON</text>
<text>ON</text>
<text>Humidifier 
Controller
CvW 2016</text>
<text>LED</text>
<text>LED</text>
<text>SSR</text>
<text>GND</text>
<text>WATER
LEVEL</text>
<text>WATER
LEVEL</text>
<text>WATER LEVEL</text>
<text>WHT</text>
<text>BLU</text>
<text>RED</text>
<text>YLW</text>
<text>3V3</text>
<text>3V3</text>
<text>GND</text>
<text>GND</text>
<text>VIN</text>
<text>VIN</text>
<text>FAN TERMINAL</text>
<text>FAN TERMINAL</text>
<text>SSR</text>
<text>SSR</text>
<text>SSR
TERM</text>
<text>SSR
TERM</text>
<text>TX1</text>
<text>RX1</text>
<text>GND</text>
<text>TX1</text>
<text>RX1</text>
<text>GND</text>
<text>FA1</text>
<text>FA2</text>
<text>TCS</text>
<text>TCS</text>
<text>BLK</text>
<text>BLK</text>
<text>RED</text>
<text>RED</text>
</plain>
<libraries>
<library name="CvW">
<packages>
<package name="POWERJACK2.0MM">
<description>DC Power Jack, 5.5mm OD, 2.0mm ID, CUI Part Number PJ-102A</description>
</package>
<package name="WIRETERMINAL-2POS">
<description>&lt;b&gt;TE Header, Part Number 282857-2&lt;/b&gt;, 2 POS
&lt;p&gt;Good for 24A, 12-30AWG Wire. Interlocking feature.</description>
</package>
<package name="WIRETERMINAL-3POS">
</package>
<package name="ACS712">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
<package name="DIL16-ROUND">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="MINI4G4B">
<description>Mini4-G4-B Footprint</description>
</package>
<package name="MOLEX-1X4_LOCK">
</package>
</packages>
</library>
<library name=" CvW">
<packages>
<package name="SOD-123W">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
<package name="1X03">
</package>
<package name="1X14">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
<package name="B/3528-21R">
<description>&lt;b&gt;Chip Capacitor Type KEMET B / EIA 3528-21 Reflow solder&lt;/b&gt;&lt;p&gt;
KEMET T / EIA 3528-12</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="USB_Host">
<description>Generated from &lt;b&gt;USB_Host.sch&lt;/b&gt;&lt;p&gt;
by exp-project-lbr.ulp</description>
<packages>
<package name="SPARKFUN_STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
<library name="relay">
<description>&lt;b&gt;Relays&lt;/b&gt;&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;Eichhoff
&lt;li&gt;Finder
&lt;li&gt;Fujitsu
&lt;li&gt;HAMLIN
&lt;li&gt;OMRON
&lt;li&gt;Matsushita
&lt;li&gt;NAiS
&lt;li&gt;Siemens
&lt;li&gt;Schrack
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="G2REA">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x norm. open, high current, Omron</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206-BOTTOM">
</package>
</packages>
</library>
<library name="con-faston">
<description>&lt;b&gt;FASTON Connector&lt;/b&gt; Printed Circuit Board Tabs&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="62409-1">
<description>&lt;b&gt;TAB, FASTON, PC Board, 6,35 (.250) Series&lt;/b&gt;&lt;p&gt;
Distributor: Digikey - Nb.  A24742-ND&lt;br&gt;
Source: http://catalog.tycoelectronics.com .. ENG_CD_62409_R.pdf</description>
</package>
</packages>
</library>
<library name="Teensy_3_and_LC_Series_Boards_v1.1">
<packages>
<package name="TEENSY3-ALL_PINS">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="wuerth-elektronik">
<description>&lt;BR&gt;WE eiSos -- EMC &amp; Inductive Solutions&lt;br&gt;&lt;Hr&gt;
&lt;BR&gt;&lt;BR&gt; 
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-400&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com"&gt;http://www.we-online.com&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:eisos@we-online.de"&gt;eisos@we-online.de&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither CadSoft nor WE-eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;&lt;BR&gt;&lt;br&gt;
&lt;hr&gt;
Version 4,   July 12th 2005
&lt;HR&gt;
Copyright: Würth Elektronik eiSos</description>
<packages>
<package name="0805">
<description>Multilayer SMD</description>
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="Diodes_Inc_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 14:20:03</description>
<packages>
<package name="SOT91P240X110-3N">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D2" library=" CvW" package="SOD-123W" value="PMEG3020">
<attribute name="VALUE"/>
</element>
<element name="D1" library=" CvW" package="SOD-123W" value="PMEG3020">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="CvW" package="POWERJACK2.0MM" value="PJ-102APTH"/>
<element name="U$5" library="CvW" package="WIRETERMINAL-3POS" value="WIRETERMINAL-3POS"/>
<element name="U$6" library="CvW" package="WIRETERMINAL-2POS" value="WIRETERMINAL-2POS"/>
<element name="LED3" library="SparkFun-LED" package="LED-1206-BOTTOM" value="">
<attribute name="VALUE" value="Green"/>
<attribute name="PROD_ID" value="DIO-11076"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0805" value="2k2">
<attribute name="VALUE"/>
</element>
<element name="LED4" library="SparkFun-LED" package="LED-1206-BOTTOM" value="">
<attribute name="VALUE" value="Green"/>
<attribute name="PROD_ID" value="DIO-11076"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0805" value="2k2">
<attribute name="VALUE"/>
</element>
<element name="C1" library="adafruit" package="C0805K" value="0.1uF">
<attribute name="VALUE"/>
</element>
<element name="C2" library="adafruit" package="C0805K" value="1nF">
<attribute name="VALUE"/>
</element>
<element name="C3" library="adafruit" package="B/3528-21R" value="47uF">
<attribute name="VALUE"/>
</element>
<element name="U$7" library="USB_Host" package="SPARKFUN_STAND-OFF" value=""/>
<element name="U$8" library="USB_Host" package="SPARKFUN_STAND-OFF" value=""/>
<element name="C4" library="adafruit" package="C0805K" value="0.1uF">
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="1X03" value=""/>
<element name="U$1" library="CvW" package="ACS712" value="ACS711">
<attribute name="VALUE"/>
</element>
<element name="OK1" library="CvW" package="DIL16-ROUND" value="LTV-844">
<attribute name="OC_NEWARK" value="58K1694"/>
<attribute name="MPN" value="ILQ620"/>
<attribute name="MF" value="VISHAY/TELEFUNKEN"/>
<attribute name="OC_FARNELL" value="1612470"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="2k2">
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="2k2">
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="2k2">
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="2k2">
<attribute name="VALUE"/>
</element>
<element name="U$9" library="CvW" package="MINI4G4B" value="DA4X106U0R"/>
<element name="U$10" library="CvW" package="MINI4G4B" value="DA4X106U0R">
<attribute name="VALUE"/>
</element>
<element name="U$11" library="CvW" package="MINI4G4B" value="DA4X106U0R"/>
<element name="U$12" library="CvW" package="MINI4G4B" value="DA4X106U0R"/>
<element name="C5" library="adafruit" package="C0805K" value="0.1uF">
<attribute name="VALUE"/>
</element>
<element name="C6" library="adafruit" package="C0805K" value="0.1uF">
<attribute name="VALUE"/>
</element>
<element name="C7" library="adafruit" package="C0805K" value="0.1uF">
<attribute name="VALUE"/>
</element>
<element name="C8" library="adafruit" package="C0805K" value="0.1uF">
<attribute name="VALUE"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="0805" value="10">
<attribute name="VALUE"/>
</element>
<element name="K1" library="relay" package="G2REA" value="G5RL-1A-E-HR DC5">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="K2" library="relay" package="G2REA" value="G5RL-1A-E-HR DC5">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="con-faston" package="62409-1" value="PIN262409-1">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="U$14" library="con-faston" package="62409-1" value="PIN262409-1">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="U$15" library="con-faston" package="62409-1" value="PIN262409-1">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X14" value="M14"/>
<element name="R5" library="SparkFun-Resistors" package="0805" value="100">
<attribute name="VALUE"/>
</element>
<element name="U$3" library="Teensy_3_and_LC_Series_Boards_v1.1" package="TEENSY3-ALL_PINS" value="TEENSY_LC_ALL_PINS"/>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23" value="BSS138">
<attribute name="PROD_ID" value="TRANS-00830"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="SOT23" value="BSS138">
<attribute name="PROD_ID" value="TRANS-00830"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library=" CvW" package="SOD-123W" value="PMEG3020">
<attribute name="VALUE"/>
</element>
<element name="D4" library=" CvW" package="SOD-123W" value="PMEG3020">
<attribute name="VALUE"/>
</element>
<element name="L1" library="wuerth-elektronik" package="0805" value="742792096">
<attribute name="VALUE"/>
</element>
<element name="C30" library="SparkFun" package="0805" value="1uF">
<attribute name="VALUE"/>
</element>
<element name="U1" library="Diodes_Inc_By_element14_Batch_1" package="SOT91P240X110-3N" value="BZX84C5V6">
<attribute name="PACKAGE" value="SOT-23-3"/>
<attribute name="OC_NEWARK" value="55T1793"/>
<attribute name="MPN" value="BZX84C5V6"/>
<attribute name="SUPPLIER" value="DIODES INC."/>
<attribute name="OC_FARNELL" value="1902459"/>
<attribute name="VALUE"/>
</element>
<element name="U$13" library="USB_Host" package="SPARKFUN_STAND-OFF" value=""/>
<element name="JP2" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
<element name="JP3" library="CvW" package="MOLEX-1X4_LOCK" value=""/>
<element name="R7" library="adafruit" package="R0805" value="220">
<attribute name="VALUE"/>
</element>
<element name="OK2" library="CvW" package="DIL16-ROUND" value="LTV-844">
<attribute name="OC_NEWARK" value="58K1694"/>
<attribute name="MPN" value="ILQ620"/>
<attribute name="MF" value="VISHAY/TELEFUNKEN"/>
<attribute name="OC_FARNELL" value="1612470"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="0805" value="420">
<attribute name="VALUE"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="0805" value="420">
<attribute name="VALUE"/>
</element>
<element name="R13" library="SparkFun-Resistors" package="0805" value="420">
<attribute name="VALUE"/>
</element>
<element name="R14" library="SparkFun-Resistors" package="0805" value="420">
<attribute name="VALUE"/>
</element>
<element name="R15" library="SparkFun-Resistors" package="0805" value="1k5">
<attribute name="VALUE"/>
</element>
<element name="R16" library="SparkFun-Resistors" package="0805" value="750">
<attribute name="VALUE"/>
</element>
<element name="R18" library="SparkFun-Resistors" package="0805" value="375">
<attribute name="VALUE"/>
</element>
<element name="R19" library="SparkFun-Resistors" package="0805" value="150">
<attribute name="VALUE"/>
</element>
<element name="U$16" library="CvW" package="WIRETERMINAL-2POS" value="WIRETERMINAL-2POS"/>
<element name="JP5" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="ACS711">
<contactref element="C2" pad="1"/>
<contactref element="U$1" pad="7"/>
<contactref element="U$3" pad="A10"/>
</signal>
<signal name="3.3V">
<contactref element="C3" pad="+"/>
<contactref element="C4" pad="1"/>
<contactref element="JP1" pad="4"/>
<contactref element="R5" pad="1"/>
<contactref element="U$3" pad="3.3V1"/>
<contactref element="U$3" pad="3.3V"/>
<contactref element="U$3" pad="3.3V1"/>
<contactref element="U$3" pad="3.3V"/>
<contactref element="L1" pad="1"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="24VAC-IN">
<contactref element="K2" pad="P@"/>
<contactref element="U$14" pad="A1"/>
<contactref element="U$14" pad="A2"/>
<contactref element="K2" pad="P"/>
<contactref element="U$1" pad="3&amp;4"/>
</signal>
<signal name="24VAC-OUT">
<contactref element="K1" pad="P@"/>
<contactref element="K1" pad="P"/>
<contactref element="U$1" pad="1&amp;2"/>
</signal>
<signal name="VUSB">
<contactref element="D2" pad="A"/>
<contactref element="U$3" pad="VUSB"/>
<contactref element="U$3" pad="VUSB"/>
</signal>
<signal name="VIN">
<contactref element="D2" pad="C"/>
<contactref element="D1" pad="C"/>
<contactref element="JP1" pad="1"/>
<contactref element="U$3" pad="VIN"/>
<contactref element="U$3" pad="VIN"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="GND">
<contactref element="U$2" pad="2"/>
<contactref element="LED3" pad="C"/>
<contactref element="LED4" pad="C"/>
<contactref element="C3" pad="-"/>
<contactref element="C4" pad="2"/>
<contactref element="JP4" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="U$3" pad="GND1"/>
<contactref element="U$3" pad="GND"/>
<contactref element="U$3" pad="AGND"/>
<contactref element="U$3" pad="GND1"/>
<contactref element="U$3" pad="GND"/>
<contactref element="U$3" pad="AGND"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U$1" pad="5"/>
<contactref element="Q2" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="C30" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="JP2" pad="2"/>
<contactref element="OK1" pad="15"/>
<contactref element="OK1" pad="13"/>
<contactref element="OK1" pad="9"/>
<contactref element="OK1" pad="11"/>
<contactref element="JP3" pad="4"/>
<contactref element="OK2" pad="8"/>
<contactref element="OK2" pad="6"/>
<contactref element="OK2" pad="4"/>
<contactref element="OK2" pad="2"/>
<contactref element="JP3" pad="3"/>
<contactref element="JP5" pad="3"/>
</signal>
<signal name="5V">
<contactref element="D1" pad="A"/>
<contactref element="U$2" pad="1"/>
<contactref element="K2" pad="1"/>
<contactref element="D3" pad="C"/>
<contactref element="K1" pad="1"/>
<contactref element="D4" pad="C"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="HUM2">
<contactref element="U$3" pad="4"/>
<contactref element="OK1" pad="14"/>
</signal>
<signal name="N$4">
<contactref element="R8" pad="1"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="R9" pad="1"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="HUM4">
<contactref element="U$3" pad="6"/>
<contactref element="OK1" pad="10"/>
</signal>
<signal name="HUM3">
<contactref element="U$3" pad="5"/>
<contactref element="OK1" pad="12"/>
</signal>
<signal name="HUM1">
<contactref element="U$3" pad="3"/>
<contactref element="OK1" pad="16"/>
</signal>
<signal name="AREF">
<contactref element="R11" pad="2"/>
<contactref element="U$3" pad="AREF"/>
<contactref element="U$3" pad="AREF"/>
<contactref element="L1" pad="2"/>
<contactref element="C30" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="OK1" pad="3"/>
<contactref element="R2" pad="2"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="OK1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="COMMON">
<contactref element="U$9" pad="2"/>
<contactref element="U$12" pad="2"/>
<contactref element="U$10" pad="2"/>
<contactref element="U$11" pad="2"/>
<contactref element="U$6" pad="2"/>
</signal>
<signal name="4-DC">
<contactref element="R3" pad="1"/>
<contactref element="U$10" pad="1"/>
</signal>
<signal name="2">
<contactref element="U$12" pad="4"/>
<contactref element="U$5" pad="5"/>
</signal>
<signal name="1">
<contactref element="U$9" pad="4"/>
<contactref element="U$5" pad="6"/>
</signal>
<signal name="2-DC">
<contactref element="R2" pad="1"/>
<contactref element="U$12" pad="1"/>
</signal>
<signal name="GND-2">
<contactref element="U$12" pad="3"/>
<contactref element="OK1" pad="4"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="GND-1">
<contactref element="U$9" pad="3"/>
<contactref element="OK1" pad="2"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="GND-3">
<contactref element="U$11" pad="3"/>
<contactref element="OK1" pad="6"/>
<contactref element="C8" pad="2"/>
</signal>
<signal name="1-DC">
<contactref element="R1" pad="1"/>
<contactref element="U$9" pad="1"/>
</signal>
<signal name="3">
<contactref element="U$11" pad="4"/>
<contactref element="U$5" pad="4"/>
</signal>
<signal name="4">
<contactref element="U$10" pad="4"/>
<contactref element="U$6" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R4" pad="2"/>
<contactref element="OK1" pad="5"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R3" pad="2"/>
<contactref element="OK1" pad="7"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="3-DC">
<contactref element="R4" pad="1"/>
<contactref element="U$11" pad="1"/>
</signal>
<signal name="GND-4">
<contactref element="U$10" pad="3"/>
<contactref element="OK1" pad="8"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="C1" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="DISP_CS">
<contactref element="JP1" pad="3"/>
<contactref element="U$3" pad="14/A0"/>
</signal>
<signal name="D/C">
<contactref element="JP1" pad="5"/>
<contactref element="U$3" pad="15/A1"/>
</signal>
<signal name="MOSI">
<contactref element="JP1" pad="6"/>
<contactref element="JP1" pad="12"/>
<contactref element="U$3" pad="11"/>
</signal>
<signal name="SCK">
<contactref element="JP1" pad="7"/>
<contactref element="JP1" pad="10"/>
<contactref element="U$3" pad="13"/>
</signal>
<signal name="LED">
<contactref element="JP1" pad="8"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="MISO">
<contactref element="JP1" pad="13"/>
<contactref element="JP1" pad="9"/>
<contactref element="U$3" pad="12"/>
</signal>
<signal name="T_CS">
<contactref element="JP1" pad="11"/>
<contactref element="U$3" pad="16/A2"/>
</signal>
<signal name="N$16">
<contactref element="K2" pad="2"/>
<contactref element="Q1" pad="3"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$17">
<contactref element="Q2" pad="3"/>
<contactref element="K1" pad="2"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="N$19">
<contactref element="K2" pad="S"/>
<contactref element="U$4" pad="A1"/>
<contactref element="U$4" pad="A2"/>
<contactref element="K2" pad="S@"/>
</signal>
<signal name="N$20">
<contactref element="K1" pad="S"/>
<contactref element="U$15" pad="A1"/>
<contactref element="U$15" pad="A2"/>
<contactref element="K1" pad="S@"/>
</signal>
<signal name="WATER_VALVE">
<contactref element="U$3" pad="10"/>
<contactref element="R9" pad="2"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="ULTRASONIC">
<contactref element="U$3" pad="9"/>
<contactref element="R8" pad="2"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="SSR">
<contactref element="JP2" pad="1"/>
<contactref element="U$3" pad="2"/>
</signal>
<signal name="DUCT_LED">
<contactref element="JP4" pad="3"/>
<contactref element="U$3" pad="VBAT"/>
</signal>
<signal name="WATER_LEVEL">
<contactref element="U$3" pad="RESET/DAC"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="OK2" pad="1"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="OK2" pad="3"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="OK2" pad="5"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="OK2" pad="7"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="R19" pad="1"/>
<contactref element="OK2" pad="9"/>
<contactref element="U$16" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="R19" pad="2"/>
<contactref element="R18" pad="1"/>
<contactref element="OK2" pad="11"/>
<contactref element="OK2" pad="10"/>
</signal>
<signal name="N$15">
<contactref element="R18" pad="2"/>
<contactref element="R16" pad="1"/>
<contactref element="OK2" pad="13"/>
<contactref element="OK2" pad="12"/>
</signal>
<signal name="N$18">
<contactref element="R16" pad="2"/>
<contactref element="R15" pad="1"/>
<contactref element="OK2" pad="15"/>
<contactref element="OK2" pad="14"/>
</signal>
<signal name="N$21">
<contactref element="R15" pad="2"/>
<contactref element="OK2" pad="16"/>
<contactref element="U$16" pad="1"/>
</signal>
<signal name="FAN1">
<contactref element="U$3" pad="18/A4"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="FAN2">
<contactref element="U$3" pad="19/A5"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="FAN3">
<contactref element="U$3" pad="20/A6"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="FAN4">
<contactref element="U$3" pad="21/A7"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="JP3" pad="2"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="RX1">
<contactref element="U$3" pad="0"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="TX1">
<contactref element="U$3" pad="1"/>
<contactref element="JP5" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
