<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="50" y2="0" width="0" layer="20"/>
<wire x1="50" y1="0" x2="50" y2="40" width="0" layer="20"/>
<wire x1="50" y1="40" x2="0" y2="40" width="0" layer="20"/>
<wire x1="0" y1="40" x2="0" y2="0" width="0" layer="20"/>
<text>MRL TinyTeRP 
Charging Board 
Rev1.1
9/18/2015</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01_LONGPAD">
</package>
<package name="1X04_LOCK">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B2,54">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="XYKlib">
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;SOT 23-5&lt;/b&gt;
&lt;br/&gt;
&lt;b&gt;TSOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="smd-special">
<description>&lt;b&gt;Special SMD Packages&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMS-003">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0402-CAP" value="1uF"/>
<element name="JP1" library="SparkFun-Connectors" package="1X01_LONGPAD" value="M01PTH_LONGPAD">
<attribute name="NAME"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X01_LONGPAD" value="M01PTH_LONGPAD">
<attribute name="NAME"/>
</element>
<element name="LED1" library="SparkFun-LED" package="LED-0603" value="Green"/>
<element name="LED2" library="SparkFun-LED" package="LED-0603" value="Blue"/>
<element name="R1" library="SparkFun-Passives" package="0402-RES" value="1k"/>
<element name="R2" library="SparkFun-Passives" package="0402-RES" value="5k"/>
<element name="R4" library="SparkFun-Passives" package="0402-RES" value="1k"/>
<element name="TP1" library="testpad" package="B2,54" value="TPB2,54">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP2" library="testpad" package="B2,54" value="TPB2,54">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="XYKlib" package="SOT23-5" value="LT4054ES5-4.2"/>
<element name="U2" library="XYKlib" package="SOT23-5" value="LT4054ES5-4.2"/>
<element name="R7" library="SparkFun-Passives" package="0402-RES" value="5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0402-CAP" value="1uF"/>
<element name="LED4" library="SparkFun-LED" package="LED-0603" value="Blue"/>
<element name="R8" library="SparkFun-Passives" package="0402-RES" value="1k"/>
<element name="TP3" library="testpad" package="B2,54" value="TPB2,54">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP4" library="testpad" package="B2,54" value="TPB2,54">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="LED5" library="SparkFun-LED" package="LED-0603" value="Green"/>
<element name="R9" library="SparkFun-Passives" package="0402-RES" value="1k"/>
<element name="JP3" library="SparkFun-Connectors" package="1X04_LOCK" value=""/>
<element name="JP4" library="SparkFun-Connectors" package="1X04_LOCK" value=""/>
<element name="S1" library="smd-special" package="SMS-003" value="SWS003"/>
<element name="S2" library="smd-special" package="SMS-003" value="SWS003"/>
<element name="R13" library="SparkFun-Passives" package="0402-RES" value="5k"/>
<element name="R14" library="SparkFun-Passives" package="0402-RES" value="5k"/>
<element name="R15" library="SparkFun-Passives" package="0402-RES" value="5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="SparkFun-Passives" package="0402-RES" value="5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$6">
<contactref element="LED2" pad="A"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="U2" pad="4"/>
<contactref element="C2" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="LED2" pad="C"/>
<contactref element="JP2" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="LED4" pad="C"/>
<contactref element="U2" pad="2"/>
<contactref element="JP3" pad="4"/>
<contactref element="JP4" pad="4"/>
<contactref element="R13" pad="1"/>
<contactref element="R14" pad="1"/>
<contactref element="R15" pad="1"/>
<contactref element="R16" pad="1"/>
<contactref element="TP4" pad="TP"/>
<contactref element="TP2" pad="TP"/>
</signal>
<signal name="N$3">
<contactref element="LED1" pad="A"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="CHRG1">
<contactref element="U1" pad="1"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="N$8">
<contactref element="LED4" pad="A"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="PROG2">
<contactref element="R7" pad="2"/>
<contactref element="S2" pad="4"/>
</signal>
<signal name="VBATT2">
<contactref element="TP3" pad="TP"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="LED5" pad="A"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="CHRG2">
<contactref element="U2" pad="1"/>
<contactref element="LED5" pad="C"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="5"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="2"/>
<contactref element="S1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="S1" pad="4"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="S1" pad="5"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="S1" pad="6"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="U2" pad="5"/>
<contactref element="S2" pad="3"/>
<contactref element="S2" pad="2"/>
<contactref element="S2" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="S2" pad="5"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="S2" pad="6"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="VBAT">
<contactref element="TP1" pad="TP"/>
<contactref element="U1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
