<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="35.56" width="0.2032" layer="20"/>
<wire x1="0" y1="35.56" x2="71.12" y2="35.56" width="0.2032" layer="20"/>
<wire x1="71.12" y1="35.56" x2="71.12" y2="0" width="0.2032" layer="20"/>
<wire x1="0" y1="0" x2="71.12" y2="0" width="0.2032" layer="20"/>
<text>Rain</text>
<text>Wind</text>
<text>Soil Moisture</text>
<text>Soil Temp</text>
<wire x1="5.08" y1="14.605" x2="5.08" y2="17.145" width="1.524" layer="46"/>
<wire x1="5.08" y1="17.145" x2="18.415" y2="17.145" width="1.524" layer="46"/>
<wire x1="5.08" y1="8.89" x2="5.08" y2="6.604" width="1.524" layer="46"/>
<wire x1="5.08" y1="6.604" x2="18.415" y2="6.604" width="1.524" layer="46"/>
<text>GND</text>
<text>SIG</text>
<text>D5</text>
<text>Humidity</text>
<text>Temp</text>
<text>Pressure</text>
<text>GND</text>
<text>SIG</text>
<text>VCC</text>
<text>GND</text>
<text>VCC</text>
<text>SDA</text>
<text>SCL</text>
<text>I2C Port</text>
<text>Soil Temp</text>
<text>GND</text>
<text>SIG</text>
<text>VCC</text>
<text>GND</text>
<text>VCC</text>
<text>SDA</text>
<text>SCL</text>
<text>I2C Port</text>
<text>Soil Moisture</text>
<text>GND</text>
<text>SIG</text>
<text>D5</text>
<text>Photon
Weather
Shield</text>
<text>I2C</text>
<text>PU</text>
<text>Photon</text>
<text>Weather</text>
<text>Shield</text>
<text>Power Select</text>
<text>RAW</text>
<text>P_VIN</text>
<text>VREG</text>
<text>Rain</text>
<text>Wind</text>
<text>Joel Bartlett</text>
<text>V10</text>
<text>+</text>
<text>-</text>
<text>+</text>
<text>-</text>
<text>3.3V Disable</text>
<wire x1="4.3942" y1="17.0942" x2="4.3942" y2="14.6304" width="0.2032" layer="20"/>
<wire x1="4.3942" y1="14.6304" x2="5.08" y2="13.9446" width="0.2032" layer="20" curve="90"/>
<wire x1="5.08" y1="13.9446" x2="5.7404" y2="14.605" width="0.2032" layer="20" curve="90"/>
<wire x1="5.7404" y1="14.605" x2="5.7404" y2="16.4592" width="0.2032" layer="20"/>
<wire x1="5.7404" y1="16.4592" x2="18.3642" y2="16.4592" width="0.2032" layer="20"/>
<wire x1="18.3642" y1="16.4592" x2="19.0754" y2="17.1704" width="0.2032" layer="20" curve="90"/>
<wire x1="19.0754" y1="17.1704" x2="18.4404" y2="17.8054" width="0.2032" layer="20" curve="90"/>
<wire x1="18.4404" y1="17.8054" x2="5.1054" y2="17.8054" width="0.2032" layer="20"/>
<wire x1="5.1054" y1="17.8054" x2="4.3942" y2="17.0942" width="0.2032" layer="20" curve="90"/>
<wire x1="4.4196" y1="6.6548" x2="4.4196" y2="8.8646" width="0.2032" layer="20"/>
<wire x1="4.4196" y1="8.8646" x2="5.1054" y2="9.5504" width="0.2032" layer="20" curve="-90"/>
<wire x1="5.1054" y1="9.5504" x2="5.7658" y2="8.8646" width="0.2032" layer="20" curve="-90"/>
<wire x1="5.7658" y1="8.8646" x2="5.7658" y2="7.2898" width="0.2032" layer="20"/>
<wire x1="5.7658" y1="7.2898" x2="18.3896" y2="7.2898" width="0.2032" layer="20"/>
<wire x1="18.3896" y1="7.2898" x2="19.1008" y2="6.5786" width="0.2032" layer="20" curve="-90"/>
<wire x1="19.1008" y1="6.5786" x2="18.4658" y2="5.9436" width="0.2032" layer="20" curve="-90"/>
<wire x1="18.4658" y1="5.9436" x2="5.1308" y2="5.9436" width="0.2032" layer="20"/>
<wire x1="5.1308" y1="5.9436" x2="4.4196" y2="6.6548" width="0.2032" layer="20" curve="-90"/>
<text>USART
Serial1</text>
<text>VCC</text>
<text>GND</text>
<text>RXI</text>
<text>TXO</text>
<text>VCC</text>
<text>GND</text>
<text>RXI</text>
<text>TXO</text>
<text>USART
Serial1</text>
<text>Route Out</text>
<text>Route Out</text>
</plain>
<libraries>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
<package name="SFE_LOGO_NAME_FLAME_.1">
</package>
<package name="FIDUCIAL-1X2">
</package>
<package name="SFE_LOGO_NAME_.1">
</package>
<package name="SFE_LOGO_FLAME_.1">
</package>
<package name="CREATIVE_COMMONS">
</package>
</packages>
</library>
<library name="template_temp">
<packages>
<package name="SPARK_PHOTON_TEMPLATE_WIDE_LOCKING">
</package>
</packages>
</library>
<library name="SparkFun-Sensors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LGA8">
<description>&lt;h4&gt;LGA8 Package&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt; 5.0x3.0x1.2mm&lt;/li&gt;
&lt;li&gt;8-pad&lt;/li&gt;&lt;br&gt;&lt;/ul&gt;
Used in MPL115A1 -</description>
</package>
<package name="HTU21D">
<description>&lt;b&gt;Description:&lt;/b&gt; HTU21D is a very small, low cost, I2C digital humidity and temperature sensor.</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PAD-JUMPER-3-3OF3_NC_BY_TRACE_YES_SILK_FULL_BOX">
</package>
<package name="PAD-JUMPER-3-2OF3_NC_BY_TRACE_YES_SILK_FULL_BOX">
</package>
<package name="PAD-JUMPER-2-NC_BY_TRACE_YES_SILK">
<description>Solder jumper, small, shorted with trace. No paste layer. Trace is cuttable.</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03">
</package>
<package name="1X04">
</package>
<package name="POWER_JACK_SMD">
</package>
<package name="SCREWTERMINAL-3.5MM-2">
</package>
<package name="RJ11-6">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOD-323">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
<package name="EIA3216">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C2" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="VALUE" value="0.1uF"/>
</element>
<element name="U1" library="SparkFun-PowerIC" package="SOT23-5" value="3.3V MIC5219">
<attribute name="PROD_ID" value="VREG-00822"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0603-CAP" value="1.0uF">
<attribute name="PROD_ID" value="CAP-00868"/>
<attribute name="VALUE" value="1.0uF"/>
</element>
<element name="U3" library="SparkFun-Sensors" package="LGA8" value="MPL3115A2LGA8">
<attribute name="PROD_ID" value="IC-10869"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="VALUE" value="0.1uF"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="VALUE" value="0.1uF"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="0603-CAP" value="1.0uF">
<attribute name="PROD_ID" value="CAP-00868"/>
<attribute name="VALUE" value="1.0uF"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="VALUE" value="0.1uF"/>
</element>
<element name="U2" library="SparkFun-Sensors" package="HTU21D" value="HTU21D">
<attribute name="PROD_ID" value="IC-11793"/>
</element>
<element name="C13" library="SparkFun-Capacitors" package="EIA3216" value="10uF">
<attribute name="PROD_ID" value="CAP-00811"/>
<attribute name="VALUE" value="10uF"/>
</element>
<element name="C14" library="SparkFun-Capacitors" package="EIA3216" value="10uF">
<attribute name="PROD_ID" value="CAP-00811"/>
<attribute name="VALUE" value="10uF"/>
</element>
<element name="JP8" library="SparkFun-Connectors" package="RJ11-6" value="RJ11">
<attribute name="PROD_ID" value="CONN-08590"/>
<attribute name="VALUE" value="RJ11"/>
</element>
<element name="JP7" library="SparkFun-Connectors" package="RJ11-6" value="RJ11">
<attribute name="PROD_ID" value="CONN-08590"/>
<attribute name="VALUE" value="RJ11"/>
</element>
<element name="R17" library="SparkFun-Resistors" package="0603-RES" value="4.7K">
<attribute name="PROD_ID" value="RES-07857"/>
<attribute name="VALUE" value="4.7K"/>
</element>
<element name="R14" library="SparkFun-Resistors" package="0603-RES" value="1K">
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE" value="1K"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="0603-RES" value="1K">
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE" value="1K"/>
</element>
<element name="R13" library="SparkFun-Resistors" package="0603-RES" value="1K">
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE" value="1K"/>
</element>
<element name="D9" library="SparkFun-DiscreteSemi" package="SOD-323" value="250mA/100V">
<attribute name="PROD_ID" value="DIO-09646"/>
<attribute name="VALUE" value="250mA/100V"/>
</element>
<element name="D10" library="SparkFun-DiscreteSemi" package="SOD-323" value="250mA/100V">
<attribute name="PROD_ID" value="DIO-09646"/>
<attribute name="VALUE" value="250mA/100V"/>
</element>
<element name="D7" library="SparkFun-DiscreteSemi" package="SOD-323" value="250mA/100V">
<attribute name="PROD_ID" value="DIO-09646"/>
<attribute name="VALUE" value="250mA/100V"/>
</element>
<element name="D8" library="SparkFun-DiscreteSemi" package="SOD-323" value="250mA/100V">
<attribute name="PROD_ID" value="DIO-09646"/>
<attribute name="VALUE" value="250mA/100V"/>
</element>
<element name="D5" library="SparkFun-DiscreteSemi" package="SOD-323" value="250mA/100V">
<attribute name="PROD_ID" value="DIO-09646"/>
<attribute name="VALUE" value="250mA/100V"/>
</element>
<element name="D6" library="SparkFun-DiscreteSemi" package="SOD-323" value="250mA/100V">
<attribute name="PROD_ID" value="DIO-09646"/>
<attribute name="VALUE" value="250mA/100V"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="0603-RES" value="1K">
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE" value="1K"/>
</element>
<element name="R15" library="SparkFun-Resistors" package="0603-RES" value="1K">
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE" value="1K"/>
</element>
<element name="R16" library="SparkFun-Resistors" package="0603-RES" value="1K">
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE" value="1K"/>
</element>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value="OSHW-LOGOM"/>
<element name="JP2" library="SparkFun-Connectors" package="1X03" value="Soil/Water Temp"/>
<element name="JP3" library="SparkFun-Connectors" package="1X03" value="Soil Moisture"/>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="4.7K">
<attribute name="PROD_ID" value="RES-07857"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X04" value="I2C Port"/>
<element name="SJ1" library="SparkFun-Passives" package="PAD-JUMPER-3-3OF3_NC_BY_TRACE_YES_SILK_FULL_BOX" value=""/>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="JP5-DNP" library="SparkFun-Connectors" package="POWER_JACK_SMD" value="5.5x2.1mm Barrel">
<attribute name="PROD_ID" value="CONN-08106"/>
<attribute name="SF_ID" value="PRT-12748"/>
</element>
<element name="JP6-DNP" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="PROD_ID" value="CONN-08399"/>
</element>
<element name="SJ2" library="SparkFun-Passives" package="PAD-JUMPER-3-2OF3_NC_BY_TRACE_YES_SILK_FULL_BOX" value=""/>
<element name="U$1" library="SparkFun-Aesthetics" package="SFE_LOGO_NAME_FLAME_.1" value=""/>
<element name="FID1" library="SparkFun-Aesthetics" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="FID2" library="SparkFun-Aesthetics" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="SJ3" library="SparkFun-Passives" package="PAD-JUMPER-2-NC_BY_TRACE_YES_SILK" value=""/>
<element name="JP4" library="SparkFun-Connectors" package="1X04" value="Serial1 Port"/>
<element name="U$3" library="SparkFun-Aesthetics" package="SFE_LOGO_FLAME_.1" value=""/>
<element name="JP9" library="template_temp" package="SPARK_PHOTON_TEMPLATE_WIDE_LOCKING" value="PHOTON_TEMPLATE_WIDE_LOCKING"/>
<element name="LOGO2" library="SparkFun-Aesthetics" package="SFE_LOGO_NAME_.1" value="SFE_LOGO_NAME.1_INCH"/>
<element name="FRAME1" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LETTER"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U3" pad="3"/>
<contactref element="U2" pad="GND"/>
<contactref element="U2" pad="7"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C13" pad="C"/>
<contactref element="C14" pad="C"/>
<contactref element="D10" pad="A"/>
<contactref element="D8" pad="A"/>
<contactref element="D6" pad="A"/>
<contactref element="R15" pad="2"/>
<contactref element="R16" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP1" pad="4"/>
<contactref element="JP5-DNP" pad="GND"/>
<contactref element="JP5-DNP" pad="P$4"/>
<contactref element="JP6-DNP" pad="1"/>
<contactref element="JP4" pad="3"/>
<contactref element="JP9" pad="2"/>
<contactref element="JP9" pad="GND@0"/>
<contactref element="JP9" pad="GND@2"/>
<contactref element="JP9" pad="21"/>
</signal>
<signal name="RAW">
<contactref element="JP5-DNP" pad="VIN0"/>
<contactref element="JP6-DNP" pad="2"/>
<contactref element="SJ2" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="U1" pad="5"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C14" pad="A"/>
<contactref element="U2" pad="VDD"/>
<contactref element="U3" pad="1"/>
<contactref element="U3" pad="4"/>
<contactref element="C8" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="JP2" pad="3"/>
<contactref element="R1" pad="1"/>
<contactref element="JP1" pad="3"/>
<contactref element="SJ1" pad="2"/>
<contactref element="D5" pad="C"/>
<contactref element="D7" pad="C"/>
<contactref element="D9" pad="C"/>
<contactref element="R17" pad="1"/>
<contactref element="SJ3" pad="2"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="SCL">
<contactref element="U3" pad="8"/>
<contactref element="U2" pad="SCK"/>
<contactref element="JP1" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="JP9" pad="14"/>
<contactref element="JP9" pad="D1"/>
</signal>
<signal name="SDA">
<contactref element="U3" pad="7"/>
<contactref element="U2" pad="DATA"/>
<contactref element="JP1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="JP9" pad="13"/>
<contactref element="JP9" pad="D0"/>
</signal>
<signal name="INT-PRESSURE">
<contactref element="U3" pad="6"/>
</signal>
<signal name="N$5">
<contactref element="U3" pad="2"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="RAIN">
<contactref element="R11" pad="1"/>
<contactref element="D5" pad="A"/>
<contactref element="D6" pad="C"/>
<contactref element="JP9" pad="D2"/>
<contactref element="JP9" pad="15"/>
</signal>
<signal name="WSPEED">
<contactref element="R14" pad="1"/>
<contactref element="D9" pad="A"/>
<contactref element="D10" pad="C"/>
<contactref element="JP9" pad="16"/>
<contactref element="JP9" pad="D3"/>
</signal>
<signal name="WDIR">
<contactref element="R17" pad="2"/>
<contactref element="R13" pad="1"/>
<contactref element="D7" pad="A"/>
<contactref element="D8" pad="C"/>
<contactref element="JP9" pad="12"/>
<contactref element="JP9" pad="A0"/>
</signal>
<signal name="RAIN2">
<contactref element="JP7" pad="2"/>
</signal>
<signal name="RAIN5">
<contactref element="JP7" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="JP8" pad="2"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="JP8" pad="3"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R11" pad="2"/>
<contactref element="JP7" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="JP7" pad="4"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="JP8" pad="5"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="JP8" pad="4"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="SOIL_TEMP">
<contactref element="JP2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="JP9" pad="17"/>
<contactref element="JP9" pad="D4"/>
</signal>
<signal name="SOIL_MOIST">
<contactref element="JP3" pad="2"/>
<contactref element="JP9" pad="A1"/>
<contactref element="JP9" pad="11"/>
</signal>
<signal name="N$3">
<contactref element="SJ1" pad="3"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R2" pad="2"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="SOIL_MOIST1">
</signal>
<signal name="PHOTON_VIN">
<contactref element="SJ2" pad="1"/>
<contactref element="JP9" pad="1"/>
<contactref element="JP9" pad="VIN"/>
</signal>
<signal name="VREG">
<contactref element="SJ2" pad="3"/>
<contactref element="C13" pad="A"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="SOIL_TEMP1">
</signal>
<signal name="SOIL_MOIST2">
</signal>
<signal name="N$7">
<contactref element="SJ3" pad="1"/>
<contactref element="JP9" pad="24"/>
<contactref element="JP9" pad="3V3"/>
</signal>
<signal name="SOIL_MOIST_POWER">
<contactref element="JP3" pad="3"/>
<contactref element="JP9" pad="18"/>
<contactref element="JP9" pad="D5"/>
</signal>
<signal name="TXO">
<contactref element="JP4" pad="1"/>
<contactref element="JP9" pad="3"/>
<contactref element="JP9" pad="TX"/>
</signal>
<signal name="RXI">
<contactref element="JP4" pad="2"/>
<contactref element="JP9" pad="RX"/>
<contactref element="JP9" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
