<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<board>
<plain>
<wire x1="21.6" y1="4.5" x2="42.2" y2="4.5" width="0.1524" layer="20"/>
<wire x1="42.2" y1="4.5" x2="42.2" y2="21.9" width="0.1524" layer="20"/>
<wire x1="42.2" y1="21.9" x2="21.6" y2="21.9" width="0.1524" layer="20"/>
<wire x1="21.6" y1="21.9" x2="21.6" y2="4.5" width="0.1524" layer="20"/>
<hole x="40.6" y="20.5" drill="2"/>
<hole x="40.5" y="5.8" drill="2"/>
<text>5v</text>
<text>GND</text>
<text>+</text>
<text>-</text>
<text>GingerOfOz - 2018</text>
<text>IC1</text>
<text>IC2</text>
</plain>
<libraries>
<library name="My Stuff">
<packages>
<package name="USBM_MULTIPLEXER">
</package>
<package name="DPDT_DIGITAL_SWITCH">
</package>
<package name="USBA">
<description>USB A female connector port.  Designed to work with https://www.digikey.com/products/en/connectors-interconnects/usb-dvi-hdmi-connectors/312?k=USB+A&amp;k=&amp;pkeyword=USB+A&amp;pv28=872&amp;FV=ffe00138&amp;mnonly=0&amp;ColumnSort=0&amp;page=1&amp;quantity=0&amp;ptm=0&amp;fid=0&amp;pageSize=25</description>
</package>
<package name="MICRO_USB">
</package>
<package name="1MM_PAD_SMD">
</package>
<package name="2MM_SMD_PAD">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R2" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="PROD_ID" value="RES-07856"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="PROD_ID" value="RES-07856"/>
</element>
<element name="U$1" library="My Stuff" package="USBM_MULTIPLEXER" value="USB_MULTIPLEXER"/>
<element name="U$2" library="My Stuff" package="DPDT_DIGITAL_SWITCH" value="DPDT_DIGITAL_SWITCH"/>
<element name="U$3" library="My Stuff" package="USBA" value="USB_A_FEMALEPTH"/>
<element name="U$4" library="My Stuff" package="MICRO_USB" value="MICRO_USB"/>
<element name="U$5" library="My Stuff" package="1MM_PAD_SMD" value="1MM_SMD_PAD"/>
<element name="U$6" library="My Stuff" package="1MM_PAD_SMD" value="1MM_SMD_PAD"/>
<element name="U$8" library="My Stuff" package="2MM_SMD_PAD" value="2MM_SMD_PAD"/>
<element name="WII_5V" library="My Stuff" package="2MM_SMD_PAD" value="2MM_SMD_PAD"/>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="PROD_ID" value="CAP-11625"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="PROD_ID" value="CAP-11625"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="PROD_ID" value="CAP-11625"/>
</element>
<element name="MIC_LED" library="SparkFun-Resistors" package="0603" value="">
<attribute name="PROD_ID" value="RES-07856"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="PROD_ID" value="RES-07856"/>
</element>
<element name="USB_LED" library="SparkFun-Resistors" package="0603" value="">
<attribute name="PROD_ID" value="RES-07856"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="PROD_ID" value="RES-07856"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$8" pad="PAD"/>
<contactref element="U$3" pad="SHIELDGND2"/>
<contactref element="U$3" pad="GND"/>
<contactref element="U$3" pad="SHIELDGND"/>
<contactref element="U$4" pad="GND4"/>
<contactref element="U$4" pad="GND2"/>
<contactref element="U$4" pad="GND"/>
<contactref element="U$4" pad="GND1"/>
<contactref element="U$4" pad="GND3"/>
<contactref element="U$2" pad="GND"/>
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="GND"/>
<contactref element="R2" pad="1"/>
<contactref element="U$1" pad="D0"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="MIC_LED" pad="2"/>
<contactref element="USB_LED" pad="2"/>
</signal>
<signal name="ILIM">
<contactref element="R2" pad="2"/>
<contactref element="U$1" pad="ILIM"/>
</signal>
<signal name="WII_5V">
<contactref element="U$1" pad="IN2"/>
<contactref element="WII_5V" pad="PAD"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="USB_5V">
<contactref element="U$1" pad="OUT"/>
<contactref element="U$3" pad="5V"/>
<contactref element="U$2" pad="VCC"/>
<contactref element="C1" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="MIC_5V">
<contactref element="U$1" pad="IN1"/>
<contactref element="U$4" pad="5V"/>
<contactref element="U$1" pad="D1"/>
<contactref element="U$2" pad="1OE"/>
<contactref element="R1" pad="2"/>
<contactref element="U$2" pad="2OE"/>
<contactref element="R3" pad="2"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="WII_DATA+">
<contactref element="U$2" pad="2A"/>
<contactref element="U$5" pad="PAD"/>
</signal>
<signal name="USB_D+">
<contactref element="U$3" pad="D+"/>
<contactref element="U$4" pad="D+"/>
<contactref element="U$2" pad="2B"/>
</signal>
<signal name="USB_D-">
<contactref element="U$3" pad="D-"/>
<contactref element="U$4" pad="D-"/>
<contactref element="U$2" pad="1B"/>
</signal>
<signal name="N$1">
<contactref element="R3" pad="1"/>
<contactref element="MIC_LED" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R4" pad="1"/>
<contactref element="USB_LED" pad="1"/>
</signal>
<signal name="WII_DATA-">
<contactref element="U$6" pad="PAD"/>
<contactref element="U$2" pad="1A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
