<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="25.38" y2="0" width="0" layer="20"/>
<wire x1="25.38" y1="0" x2="25.38" y2="25.07" width="0" layer="20"/>
<wire x1="25.38" y1="25.07" x2="0" y2="25.07" width="0" layer="20"/>
<wire x1="0" y1="25.07" x2="0" y2="0" width="0" layer="20"/>
<text>.</text>
<text>LT3032</text>
<text>+/- 15V
150 mA</text>
<text>20V
Max</text>
<text>-20V Max</text>
<text>+/- 15 Volt
Bi-polar supply</text>
<text>Max Input
+/- 20 Volt
+IP  -IN</text>
<text>Rev. 1.0</text>
<text>Greg Christenson
     2019</text>
<text>LT3032</text>
<text>Bat1 Bat2</text>
<text>Neg</text>
<text>Pos</text>
<text>Made on Earth
  by Humans</text>
</plain>
<libraries>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="cap-pan40">
<description>&lt;b&gt;Panasonic Electrolytic, Film and Tantalum Capacitors&lt;/b&gt;&lt;br&gt;

&lt;h4&gt;&lt;i&gt;Created by Bob Starr (rtzaudio@mindspring.com)&lt;br&gt;
Updated 01/08/2005&lt;/i&gt;&lt;/h4&gt;

&lt;p&gt;&lt;b&gt;The following Panasonic capactor types are supported by this library:&lt;/b&gt;
&lt;p&gt;M/NHG/FC/EB/KS/KG/TS/AA Series Radial Electrolytics&lt;br&gt;
  B/V/E/F Series Polyester Film&lt;br&gt;
  EF Series Tantalum Capacitors&lt;br&gt;
  CD/FD/H/S/UD/UE Series SMD Electrolytics&lt;br&gt;
  VV/TA/HD/VA/VS/HA/HB/FC/FK/EB SMD Electrolytics&lt;br&gt;&lt;br&gt;
 NOTE: All parts use .0125" grid spacing except where noted.&lt;/p&gt;
&lt;p&gt;&lt;h4&gt;All capacitors are grouped by the following naming conventions:&lt;/h4&gt;&lt;/p&gt;
&lt;table width="380" border="1" bordercolor="#000000"&gt;
  &lt;tr&gt; 
    &lt;td width="81" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Prefix&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
    &lt;td width="289" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Description&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;C-BP&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Bipolar Electrolytic Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;C-CA&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Chip Cap Array Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;C-NP&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Non-Polarized Film / Chip Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;C-PA&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Polarized Axial Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;C-PR&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Polarized Electrolytic/Tantalum Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
&lt;/table&gt;
&lt;p&gt;
&lt;small&gt;&lt;i&gt;Copyright (C) 2004, Bob Starr&lt;/i&gt;&lt;/small&gt;</description>
<packages>
<package name="TE-D-7343">
<description>&lt;b&gt;SMD TANTALUM&lt;/b&gt;&lt;p&gt; 
EIA Code 7343, Size D, 7.3 mm x 4.3 mm, grid 0.0125 inch</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="EIA3528">
</package>
</packages>
</library>
<library name="AWJLEagleLib">
<description>AWJ Logan Eagle Library v1.001</description>
<packages>
<package name="DFN14-4X3DE">
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2,54/1,1">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,2-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 3.2 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Passives" package="0805" value="0.01uF Film">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Passives" package="0805" value="0.01uF Film">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="cap-pan40" package="TE-D-7343" value="100uF 25V">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C4" library="cap-pan40" package="TE-D-7343" value="100uF 25V">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="EIA3528" value="4.7 25V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="EIA3528" value="4.7 25V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="AWJLEagleLib" package="DFN14-4X3DE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="+IP" library="wirepad" package="2,54/1,1" value="WIREPAD2,54/1,1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="-IN" library="wirepad" package="2,54/1,1" value="WIREPAD2,54/1,1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OP" library="wirepad" package="2,54/1,1" value="WIREPAD2,54/1,1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ON" library="wirepad" package="2,54/1,1" value="WIREPAD2,54/1,1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GNDOUT" library="wirepad" package="2,54/1,1" value="WIREPAD2,54/1,1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GNDIN" library="wirepad" package="2,54/1,1" value="WIREPAD2,54/1,1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SHDN" library="wirepad" package="2,54/1,1" value="WIREPAD2,54/1,1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H1" library="holes" package="3,2-PAD" value="MOUNT-PAD-ROUND3.2"/>
<element name="H2" library="holes" package="3,2-PAD" value="MOUNT-PAD-ROUND3.2"/>
<element name="IPS" library="wirepad" package="2,54/1,1" value="WIREPAD2,54/1,1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GNDIN1" library="wirepad" package="2,54/1,1" value="WIREPAD2,54/1,1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="C6" pad="A"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="5"/>
<contactref element="C3" pad="-"/>
<contactref element="C4" pad="+"/>
<contactref element="C5" pad="C"/>
<contactref element="GNDIN" pad="1"/>
<contactref element="GNDOUT" pad="1"/>
<contactref element="H1" pad="B3,2"/>
<contactref element="H2" pad="B3,2"/>
<contactref element="GNDIN1" pad="1"/>
</signal>
<signal name="IN">
<contactref element="C6" pad="C"/>
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="9"/>
<contactref element="-IN" pad="1"/>
</signal>
<signal name="IP">
<contactref element="C5" pad="A"/>
<contactref element="IC1" pad="14"/>
<contactref element="+IP" pad="1"/>
<contactref element="IPS" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="+"/>
<contactref element="OP" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="C1" pad="1"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="7"/>
<contactref element="C4" pad="-"/>
<contactref element="C2" pad="2"/>
<contactref element="ON" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="11"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="SHDN" pad="1"/>
<contactref element="IC1" pad="12"/>
<contactref element="IC1" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
