<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="30" y2="0" width="0" layer="20"/>
<wire x1="30" y1="0" x2="30" y2="15" width="0" layer="20"/>
<wire x1="30" y1="15" x2="0" y2="15" width="0" layer="20"/>
<wire x1="0" y1="15" x2="0" y2="0" width="0" layer="20"/>
<text>GDO2</text>
<text>MISO</text>
<text>SCLK</text>
<text>MOSI</text>
<text>GDO0</text>
<text>CSN</text>
<text>VCC</text>
<text>GND</text>
<text>Clemson University
Connor Bolton
04/2016</text>
<text>*</text>
<text>CC1101 v2a</text>
<text>GND</text>
<text>VCC</text>
<text>CSN</text>
<text>GDO0</text>
<text>GDO2</text>
<text>MISO</text>
<text>SCLK</text>
<text>MOSI</text>
</plain>
<libraries>
<library name="tiny_passives">
<packages>
<package name="0402">
</package>
</packages>
</library>
<library name="cc1101">
<packages>
<package name="QLP20">
</package>
<package name="XTAL-3.2X2.5">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
</packages>
</library>
<library name="johanson-baluns">
<packages>
<package name="XXXXBM15A0001">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="SMA_EDGELAUNCH">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="tiny_passives" package="0402" value="0.1uF">
<attribute name="MOUSER" value="581-530L104KT16T"/>
</element>
<element name="C10" library="tiny_passives" package="0402" value="0.01uF">
<attribute name="MOUSER" value="80-C0402T103K5RCL"/>
</element>
<element name="C11" library="tiny_passives" package="0402" value="12pF">
<attribute name="MOUSER" value="581-04025U120FAT2A"/>
</element>
<element name="C12" library="tiny_passives" package="0402" value="15pf">
<attribute name="MOUSER" value="80-CBR04C150F1GAC"/>
</element>
<element name="C2" library="tiny_passives" package="0402" value="220pF">
<attribute name="MOUSER" value="605-500X07W221MV4T"/>
</element>
<element name="C3" library="tiny_passives" package="0402" value="220pF">
<attribute name="MOUSER" value="605-500X07W221MV4T"/>
</element>
<element name="C4" library="tiny_passives" package="0402" value="220pF">
<attribute name="MOUSER" value="605-500X07W221MV4T"/>
</element>
<element name="C5" library="tiny_passives" package="0402" value="0.01uF">
<attribute name="MOUSER" value="80-C0402T103K5RCL"/>
</element>
<element name="C9" library="tiny_passives" package="0402" value="0.1uF">
<attribute name="MOUSER" value="581-530L104KT16T"/>
</element>
<element name="IC1" library="cc1101" package="QLP20" value="CC1101">
<attribute name="DIGIKEY" value="296-35718-1-ND"/>
<attribute name="MOUSER" value="595-CC1101RGPR"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="tiny_passives" package="0402" value="56k">
<attribute name="DIGIKEY" value="311-56KJRCT-ND"/>
<attribute name="MOUSER" value="603-RC0402JR-0756KL"/>
</element>
<element name="U4" library="johanson-baluns" package="XXXXBM15A0001" value="0896BM15A0001">
<attribute name="MOUSER" value="609-0433BM15A0001E"/>
</element>
<element name="X1" library="cc1101" package="XTAL-3.2X2.5" value="XTAL-3.2X2.5">
<attribute name="DIGIKEY" value="644-1261-1-ND"/>
</element>
<element name="X2" library="adafruit" package="SMA_EDGELAUNCH" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C12" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="IC1" pad="16"/>
<contactref element="IC1" pad="19"/>
<contactref element="IC1" pad="GND"/>
<contactref element="IC1" pad="GND1"/>
<contactref element="IC1" pad="GND2"/>
<contactref element="IC1" pad="GND3"/>
<contactref element="IC1" pad="GND4"/>
<contactref element="IC1" pad="GND5"/>
<contactref element="C9" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="U4" pad="2" route="any" routetag="G$1.GND"/>
<contactref element="U4" pad="5" route="any" routetag="G$1.GND"/>
<contactref element="U4" pad="6" route="any" routetag="G$1.GND"/>
<contactref element="J2" pad="4"/>
<contactref element="C10" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="X2" pad="GND@4"/>
<contactref element="X2" pad="GND@3"/>
<contactref element="X2" pad="GND@1"/>
<contactref element="X2" pad="GND@2"/>
</signal>
<signal name="R_VCC">
<contactref element="IC1" pad="14"/>
<contactref element="IC1" pad="9"/>
<contactref element="IC1" pad="11"/>
<contactref element="C3" pad="2"/>
<contactref element="IC1" pad="15"/>
<contactref element="IC1" pad="18"/>
<contactref element="C2" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="IC1" pad="4"/>
<contactref element="J2" pad="3"/>
<contactref element="C10" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="SCLK">
<contactref element="IC1" pad="1"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="MISO">
<contactref element="IC1" pad="2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="GDO2">
<contactref element="IC1" pad="3"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="IC1" pad="20"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="CSN">
<contactref element="IC1" pad="7"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="GDO0">
<contactref element="IC1" pad="6"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="17"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="X1" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="N$2">
<contactref element="C12" pad="2"/>
<contactref element="X1" pad="3"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="N$4">
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="U4" pad="4"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="N$5">
<contactref element="U4" pad="3"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="N$6">
<contactref element="X2" pad="P"/>
<contactref element="U4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
