<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="-0.762" y1="-1.143" x2="23.927" y2="-1.143" width="0" layer="20"/>
<wire x1="23.927" y1="-1.143" x2="24.054" y2="26.279" width="0" layer="20"/>
<wire x1="24.054" y1="26.279" x2="-0.762" y2="26.279" width="0" layer="20"/>
<wire x1="-0.762" y1="26.279" x2="-0.762" y2="-1.143" width="0" layer="20"/>
<text>5</text>
<text>12</text>
<text>TC649</text>
<text>ADJ</text>
<text>ERR</text>
<text>OUT</text>
<text>PWR</text>
<text>NTC 10K</text>
<text>FAN
CTRL</text>
<text>FAN(mA) RSENSE
50 ----  9.1
100 ---- 4.7
150 ---- 3.0
200 ---- 2.4
250 ---- 2.0
300 ---- 1.8
350 ---- 1.5
400 ---- 1.3
450 ---- 1.2
500 ---- 1.0</text>
</plain>
<libraries>
<library name="ic-package">
<description>&lt;b&gt;IC Packages an Sockets&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04_LOCK">
</package>
<package name="1X02_LOCK">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALL">
</package>
<package name="CAP-PTH-5MM">
</package>
<package name="CPOL-RADIAL-10UF-25V">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="1/6W-RES">
<description>1/6W Thru-hole Resistor - *UNPROVEN*</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TRIM_POT_PTH">
</package>
</packages>
</library>
<library name="dicons">
<description>&lt;b&gt;Silkscreen Icons, Legend Fields and Fiducials&lt;/b&gt;&lt;p&gt;
A collection of general purpose silkscreen icons, legends and label fields.
&lt;h4&gt;&lt;i&gt;Copyright (C) 2004, Bob Starr (rtzaudio@mindspring.com)&lt;br&gt;
Updated 01/08/2005&lt;/i&gt;&lt;/h4&gt;</description>
<packages>
<package name="ICON_MINUS">
<description>&lt;b&gt;ICON&lt;/b&gt;&lt;p&gt; Minus Symbol</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO35-7">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2 mm, horizontal, grid 7.62 mm</description>
</package>
</packages>
</library>
<library name="Lars2">
<packages>
<package name="8MOLOGO_TINY">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="ic-package" package="DIL08" value="">
<attribute name="VALUE"/>
</element>
<element name="IN" library="SparkFun-Connectors" package="1X04_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="FAULT" library="SparkFun-LED" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="C-BYPASS" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value=".01uF"/>
<element name="Q1" library="SparkFun-DiscreteSemi" package="TO-92" value="MOSFET-NCHANNEL2N7000"/>
<element name="R1" library="SparkFun-Resistors" package="1/6W-RES" value="20k">
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="1/6W-RES" value="3.9k">
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="1/6W-RES" value="33k">
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="1/6W-RES" value="18k">
<attribute name="VALUE"/>
</element>
<element name="R-SENSE" library="SparkFun-Resistors" package="AXIAL-0.4" value="SENSE">
<attribute name="VALUE"/>
</element>
<element name="R-BASE" library="SparkFun-Resistors" package="1/6W-RES" value="100">
<attribute name="VALUE"/>
</element>
<element name="C-BYPASS1" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value=".01uF"/>
<element name="JP1" library="SparkFun-Connectors" package="1X02_LOCK" value="M02LOCK"/>
<element name="C-VAS1" library="SparkFun-Capacitors" package="CAP-PTH-5MM" value=".1uf">
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="1/6W-RES" value="220">
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value="1uF">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X02_LOCK" value="M02LOCK"/>
<element name="C-VAS2" library="SparkFun-Capacitors" package="CAP-PTH-5MM" value=".1uf">
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="1/6W-RES" value="2k">
<attribute name="VALUE"/>
</element>
<element name="OUTPUT" library="SparkFun-LED" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="1/6W-RES" value="2k">
<attribute name="VALUE"/>
</element>
<element name="PWR" library="SparkFun-LED" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Electromechanical" package="TRIM_POT_PTH" value="TRIMPOTPTH"/>
<element name="U$2" library="dicons" package="ICON_MINUS" value=""/>
<element name="U$3" library="dicons" package="ICON_MINUS" value=""/>
<element name="U$4" library="dicons" package="ICON_MINUS" value=""/>
<element name="D1" library="diode" package="DO35-7" value="1N4148DO35-7"/>
<element name="U$1" library="Lars2" package="8MOLOGO_TINY" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="4"/>
<contactref element="IN" pad="3"/>
<contactref element="IN" pad="2"/>
<contactref element="C-BYPASS" pad="1"/>
<contactref element="R-SENSE" pad="P$2"/>
<contactref element="R2" pad="1"/>
<contactref element="C-BYPASS1" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C-VAS2" pad="1"/>
<contactref element="PWR" pad="K"/>
</signal>
<signal name="12V">
<contactref element="IN" pad="4"/>
<contactref element="JP1" pad="1"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="5V">
<contactref element="IN" pad="1"/>
<contactref element="C-BYPASS" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="IC1" pad="8"/>
<contactref element="JP2" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="7"/>
<contactref element="R-BASE" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="Q1" pad="3"/>
<contactref element="JP1" pad="2"/>
<contactref element="OUTPUT" pad="K"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="Q1" pad="2"/>
<contactref element="R-BASE" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="Q1" pad="1"/>
<contactref element="R-SENSE" pad="P$1"/>
<contactref element="C-VAS1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="C-BYPASS1" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="JP2" pad="2"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="IC1" pad="3"/>
<contactref element="C-VAS2" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="5"/>
<contactref element="C-VAS1" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="6"/>
<contactref element="FAULT" pad="K"/>
</signal>
<signal name="N$10">
<contactref element="FAULT" pad="A"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="R5" pad="1"/>
<contactref element="OUTPUT" pad="A"/>
</signal>
<signal name="N$12">
<contactref element="R7" pad="1"/>
<contactref element="PWR" pad="A"/>
</signal>
<signal name="N$13">
<contactref element="R1" pad="1"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="R2" pad="2"/>
<contactref element="R8" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
