<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.0.0">
<drawing>
<board>
<plain>
<wire x1="2.54" y1="0" x2="67.31" y2="0" width="0" layer="20"/>
<wire x1="69.85" y1="2.54" x2="69.85" y2="73.66" width="0" layer="20"/>
<wire x1="67.31" y1="76.2" x2="2.54" y2="76.2" width="0" layer="20"/>
<hole x="66.04" y="3.81" drill="3"/>
<hole x="66.04" y="72.39" drill="3"/>
<hole x="3.81" y="72.39" drill="3"/>
<wire x1="0" y1="73.66" x2="0" y2="2.54" width="0" layer="20"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0" layer="20"/>
<wire x1="67.31" y1="0" x2="69.85" y2="2.54" width="0" layer="20"/>
<wire x1="67.31" y1="76.2" x2="69.85" y2="73.66" width="0" layer="20"/>
<wire x1="0" y1="73.66" x2="2.54" y2="76.2" width="0" layer="20"/>
<text>+24IN</text>
<text>GND</text>
<text>GND</text>
<hole x="3.81" y="3.81" drill="3"/>
</plain>
<libraries>
<library name="Work">
<packages>
<package name="MGFW152415">
</package>
<package name="TEN5-2411">
</package>
<package name="CC6-2403SF-E">
</package>
</packages>
</library>
<library name="Richard">
<packages>
<package name="TERM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$2" library="Work" package="MGFW152415" value="MGFW152415"/>
<element name="U$3" library="Work" package="TEN5-2411" value="TEN5-2411"/>
<element name="U$1" library="Work" package="CC6-2403SF-E" value="CC6-2403SF-E"/>
<element name="POWER" library="Richard" package="TERM" value="TERM"/>
<element name="GND7" library="Richard" package="TERM" value="TERM"/>
<element name="GND8" library="Richard" package="TERM" value="TERM"/>
<element name="+3.3V" library="Richard" package="TERM" value="TERM">
<attribute name="NAME"/>
</element>
<element name="+5V" library="Richard" package="TERM" value="TERM">
<attribute name="NAME"/>
</element>
<element name="+15V" library="Richard" package="TERM" value="TERM">
<attribute name="NAME"/>
</element>
<element name="-15V" library="Richard" package="TERM" value="TERM">
<attribute name="NAME"/>
</element>
<element name="GND12" library="Richard" package="TERM" value="TERM"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$3" pad="-VIN"/>
<contactref element="U$3" pad="-VIN2"/>
<contactref element="U$2" pad="-VIN"/>
<contactref element="U$1" pad="-VIN"/>
<contactref element="U$1" pad="-VOUT"/>
<contactref element="U$3" pad="-VOUT"/>
<contactref element="U$1" pad="RC"/>
<contactref element="U$2" pad="COM"/>
<contactref element="U$1" pad="NC"/>
<contactref element="U$1" pad="TRM"/>
<contactref element="U$2" pad="RC"/>
<contactref element="U$3" pad="NC"/>
<contactref element="POWER" pad="A"/>
<contactref element="GND7" pad="A"/>
<contactref element="GND7" pad="B"/>
<contactref element="GND8" pad="B"/>
<contactref element="GND8" pad="A"/>
<contactref element="GND12" pad="A"/>
<contactref element="GND12" pad="B"/>
</signal>
<signal name="24V">
<contactref element="U$3" pad="+VIN"/>
<contactref element="U$3" pad="+VIN2"/>
<contactref element="U$2" pad="+VIN"/>
<contactref element="U$1" pad="+VIN"/>
<contactref element="POWER" pad="B"/>
</signal>
<signal name="3.3V">
<contactref element="U$1" pad="+VOUT"/>
<contactref element="+3.3V" pad="A"/>
<contactref element="+3.3V" pad="B"/>
</signal>
<signal name="-15V">
<contactref element="U$2" pad="-VOUT"/>
<contactref element="-15V" pad="B"/>
<contactref element="-15V" pad="A"/>
</signal>
<signal name="+15V">
<contactref element="U$2" pad="+VOUT"/>
<contactref element="+15V" pad="A"/>
<contactref element="+15V" pad="B"/>
</signal>
<signal name="5V">
<contactref element="U$3" pad="+VOUT"/>
<contactref element="+5V" pad="A"/>
<contactref element="+5V" pad="B"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
