<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="35.55" x2="0" y2="0" width="0" layer="20"/>
<hole x="2.54" y="33.02" drill="3.2"/>
<hole x="33.02" y="33.02" drill="3.2"/>
<hole x="33.02" y="2.54" drill="3.2"/>
<hole x="2.54" y="2.54" drill="3.2"/>
<text>Flimshaw Industries</text>
<text>Adjustable High Voltage Power Supply</text>
<text>Charlie Hoey 1.19.2016</text>
<text>REV1</text>
<text>6-12 volts DC in, 30-300V DC out</text>
<text>BC547</text>
<text>VOUT ADJ.</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALLEZ">
<description>This is the "EZ" version of the .1" spaced ceramic thru-hole cap.&lt;br&gt;
It has reduced top mask to make it harder to put the component on the wrong side of the board.</description>
</package>
<package name="0603-CAP">
</package>
<package name="CPOL-RADIAL-100UF-25V">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIODE-1N4148">
</package>
<package name="TO-92-AMMO">
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2,54/1,1">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="DIL08-ROUND">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="TO220V">
<description>&lt;b&gt;TO 200 vertical&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RLB0912">
</package>
<package name="AXIAL-0.3EZ">
<description>This is the "EZ" version of the standard .3" spaced resistor package.&lt;br&gt;
It has a reduced top mask to make it harder to install upside-down.</description>
</package>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="pot">
<description>&lt;b&gt;Potentiometers&lt;/b&gt;&lt;p&gt;
Beckman, Copal, Piher, Spectrol, Schukat&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="CA9H">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
distributor Schukat</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="CAP-PTH-SMALLEZ" value=""/>
<element name="C5" library="SparkFun-Capacitors" package="0603-CAP" value=""/>
<element name="D1" library="SparkFun-DiscreteSemi" package="DIODE-1N4148" value=""/>
<element name="HV" library="wirepad" package="2,54/1,1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="adafruit" package="DIL08-ROUND" value="LM555N">
<attribute name="VALUE"/>
</element>
<element name="L1" library="SparkFun-Passives" package="RLB0912" value=""/>
<element name="Q1" library="adafruit" package="TO220V" value=""/>
<element name="Q2" library="SparkFun-DiscreteSemi" package="TO-92-AMMO" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.3EZ" value="1K"/>
<element name="R2" library="SparkFun-Passives" package="AXIAL-0.3EZ" value="10K"/>
<element name="R3" library="pot" package="CA9H" value="1K"/>
<element name="R4" library="SparkFun-Passives" package="AXIAL-0.3EZ" value="220K"/>
<element name="R5" library="SparkFun-Passives" package="0603-RES" value="2.2k"/>
<element name="C2" library="SparkFun-Capacitors" package="CPOL-RADIAL-100UF-25V" value=""/>
<element name="C3" library="SparkFun-Capacitors" package="CPOL-RADIAL-100UF-25V" value=""/>
<element name="C4" library="SparkFun-Capacitors" package="CPOL-RADIAL-100UF-25V" value=""/>
<element name="GND" library="wirepad" package="2,54/1,1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="V+" library="wirepad" package="2,54/1,1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="V-" library="wirepad" package="2,54/1,1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="Q1" pad="3"/>
<contactref element="C5" pad="2"/>
<contactref element="Q2" pad="3"/>
<contactref element="R3" pad="E"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="GND" pad="1"/>
<contactref element="V-" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="8"/>
<contactref element="R1" pad="P$1"/>
<contactref element="L1" pad="1"/>
<contactref element="IC1" pad="4"/>
<contactref element="V+" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="R2" pad="P$1"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="7"/>
<contactref element="R2" pad="P$2"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="3"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="L1" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="D1" pad="C"/>
<contactref element="HV" pad="1"/>
<contactref element="R4" pad="P$2"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="Q2" pad="1"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="N$7">
<contactref element="Q2" pad="2"/>
<contactref element="R3" pad="S"/>
</signal>
<signal name="N$8">
<contactref element="R3" pad="A"/>
<contactref element="R4" pad="P$1"/>
</signal>
<signal name="N$9">
<contactref element="R5" pad="2"/>
<contactref element="C5" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
