<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="57.404" y1="48.26" x2="31.572" y2="48.26" width="0" layer="20"/>
<wire x1="31.572" y1="48.26" x2="31.572" y2="-0.244" width="0" layer="20"/>
<wire x1="31.572" y1="-0.244" x2="57.404" y2="0.01" width="0" layer="20"/>
<text>VCC</text>
<text>LED1</text>
<text>LED2</text>
<wire x1="57.404" y1="0.01" x2="57.404" y2="48.26" width="0" layer="20"/>
<text>A0</text>
<text>GND</text>
<text>D3/4</text>
<text>D3/4</text>
<text>GND</text>
<text>A0</text>
<text>LED2</text>
<text>LED1</text>
<text>VCC</text>
<text>GND</text>
<text>GND</text>
<text>D1</text>
<text>D2</text>
<text>GND</text>
<text>A</text>
<text>B</text>
<text>5V</text>
<text>DI</text>
<text>DE</text>
<text>RE</text>
<text>RO</text>
<text>toor camp 2016</text>
<text>control H</text>
<text>buckets</text>
<text>thomas hudson</text>
<text>RO</text>
<text>680</text>
<text>680</text>
<text>1MEG</text>
<text>120</text>
</plain>
<libraries>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-100UF-25V">
</package>
<package name="0805">
</package>
<package name="PAD-JUMPER-2-NC_BY_PASTE_YES_SILK">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-5MM-2">
</package>
<package name="1X01">
</package>
</packages>
</library>
<library name="ESP12E_DEVKIT">
<packages>
<package name="ESP12E_SHIELD">
</package>
</packages>
</library>
<library name="74AHCT125">
<packages>
<package name="SOIC14">
</package>
</packages>
</library>
<library name="graphics">
<packages>
<package name="BUCKETS2">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Passives" package="CPOL-RADIAL-100UF-25V" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="">
<attribute name="VALUE"/>
<attribute name="STOREFRONT_ID" value="PRT-08432"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="">
<attribute name="VALUE"/>
<attribute name="STOREFRONT_ID" value="PRT-08432"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0805" value="1 MEG">
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="0805" value="680">
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Passives" package="0805" value="680">
<attribute name="VALUE"/>
</element>
<element name="D7" library="SparkFun-Passives" package="PAD-JUMPER-2-NC_BY_PASTE_YES_SILK" value="JUMPER-PAD-2-NC_BY_PASTE">
<attribute name="NAME"/>
</element>
<element name="D8" library="SparkFun-Passives" package="PAD-JUMPER-2-NC_BY_PASTE_YES_SILK" value="JUMPER-PAD-2-NC_BY_PASTE">
<attribute name="NAME"/>
</element>
<element name="RX" library="SparkFun-Passives" package="PAD-JUMPER-2-NC_BY_PASTE_YES_SILK" value="JUMPER-PAD-2-NC_BY_PASTE">
<attribute name="NAME"/>
</element>
<element name="TX" library="SparkFun-Passives" package="PAD-JUMPER-2-NC_BY_PASTE_YES_SILK" value="JUMPER-PAD-2-NC_BY_PASTE">
<attribute name="NAME"/>
</element>
<element name="U$2" library="74AHCT125" package="SOIC14" value="74AHCT125">
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Passives" package="0805" value="120">
<attribute name="VALUE"/>
</element>
<element name="RO" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RE" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="DE" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="DI" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="5V" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="B" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="">
<attribute name="STOREFRONT_ID" value="PRT-08432"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="">
<attribute name="STOREFRONT_ID" value="PRT-08432"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="ESP12E_DEVKIT" package="ESP12E_SHIELD" value="ESP12E_SHIELD"/>
<element name="D1" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="graphics" package="BUCKETS2" value="BUCKET"/>
<element name="U$4" library="graphics" package="BUCKETS2" value="BUCKET"/>
<element name="U$5" library="graphics" package="BUCKETS2" value="BUCKET"/>
<element name="U$6" library="graphics" package="BUCKETS2" value="BUCKET"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$2" pad="7"/>
<contactref element="U$2" pad="1"/>
<contactref element="U$2" pad="4"/>
<contactref element="U$2" pad="13"/>
<contactref element="U$2" pad="12"/>
<contactref element="U$2" pad="10"/>
<contactref element="U$2" pad="9"/>
<contactref element="C1" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="GND" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="U$3" pad="GND@0"/>
<contactref element="U$3" pad="GND@1"/>
<contactref element="U$3" pad="GND@3"/>
<contactref element="U$3" pad="GND@2"/>
</signal>
<signal name="N$2">
<contactref element="U$2" pad="2"/>
<contactref element="U$3" pad="D1"/>
<contactref element="D1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U$2" pad="5"/>
<contactref element="U$3" pad="D2"/>
<contactref element="D2" pad="1"/>
</signal>
<signal name="5V">
<contactref element="U$2" pad="14"/>
<contactref element="C1" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="5V" pad="1"/>
<contactref element="U$3" pad="VIN"/>
</signal>
<signal name="N$5">
<contactref element="U$2" pad="3"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="6"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="U$3" pad="AD0"/>
</signal>
<signal name="D3">
<contactref element="JP5" pad="1"/>
<contactref element="U$3" pad="D3"/>
</signal>
<signal name="D4">
<contactref element="JP5" pad="2"/>
<contactref element="U$3" pad="D4"/>
</signal>
<signal name="N$6">
<contactref element="D7" pad="1"/>
<contactref element="RX" pad="1"/>
<contactref element="RO" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="D8" pad="1"/>
<contactref element="TX" pad="1"/>
<contactref element="DI" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="RE" pad="1"/>
<contactref element="DE" pad="1"/>
<contactref element="U$3" pad="D6"/>
</signal>
<signal name="N$9">
<contactref element="TX" pad="2"/>
<contactref element="U$3" pad="TX"/>
</signal>
<signal name="N$10">
<contactref element="RX" pad="2"/>
<contactref element="U$3" pad="RX"/>
</signal>
<signal name="N$11">
<contactref element="D8" pad="2"/>
<contactref element="U$3" pad="D8"/>
</signal>
<signal name="N$12">
<contactref element="D7" pad="2"/>
<contactref element="U$3" pad="D7"/>
</signal>
<signal name="N$13">
<contactref element="R2" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="A" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="B" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
