<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.7.1">
<drawing>
<board>
<plain>
<wire x1="37.084" y1="82.3" x2="37.084" y2="50.72" width="0" layer="20"/>
<wire x1="37.084" y1="50.72" x2="42.592" y2="45.72" width="0" layer="20" curve="90"/>
<wire x1="42.592" y1="45.72" x2="91.5" y2="45.72" width="0" layer="20"/>
<wire x1="91.5" y1="45.72" x2="96.5" y2="50.72" width="0" layer="20" curve="90"/>
<wire x1="96.5" y1="50.72" x2="96.5" y2="82.3" width="0" layer="20"/>
<wire x1="96.5" y1="82.3" x2="91.5" y2="87.3" width="0" layer="20" curve="90"/>
<wire x1="91.5" y1="87.3" x2="42.592" y2="87.3" width="0" layer="20"/>
<wire x1="42.592" y1="87.3" x2="37.084" y2="82.3" width="0" layer="20" curve="90"/>
<text>Transistor Array</text>
<text>S1</text>
<text>S2</text>
<text>S3</text>
<text>S4</text>
<text>S5</text>
<text>S6</text>
<text>S7</text>
<text>S8</text>
<text>Resistor Array</text>
<text>GND</text>
<text>5V</text>
<text>IN</text>
<text>OUT</text>
<text>QH</text>
<text>CLK</text>
<text>LD</text>
<text>CLK</text>
<text>5V</text>
<text>GND</text>
<text>74165D Shift-In</text>
<text>GND</text>
<text>QH</text>
<text>CLK</text>
<text>LD</text>
<text>5V</text>
<text>OMSI - Animations test brd
Shift Register with 8 reed switches
10K pullup resistors switches to GND
thomas hudson
06/02/18</text>
</plain>
<libraries>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RPACK-SIP-PTH-8">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X05">
</package>
<package name="1X01_NO_SILK">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="th_libraries">
<packages>
<package name="STANDOFF-ELECTRICAL">
<description>#8 screw hole, 170mill, 0.30 mask</description>
</package>
<package name="REED_SMD">
</package>
<package name="SOIC-18">
<description>0.02" wider for easy soldering to pads</description>
</package>
<package name="DIP16">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO16">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
</packages>
</library>
<library name="con-phoenix-508">
<description>&lt;b&gt;Phoenix Connectors&lt;/b&gt;&lt;p&gt;
Grid 5.08 mm&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;pho508a.lbr
&lt;li&gt;pho508b.lbr
&lt;li&gt;pho508c.lbr
&lt;li&gt;pho508d.lbr
&lt;li&gt;pho508e.lbr
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MSTBA5">
<description>&lt;b&gt;PHOENIX&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="4610X-1-103LF-ND" library="SparkFun-Resistors" package="RPACK-SIP-PTH-8" value="">
<attribute name="VALUE"/>
</element>
<element name="D10" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="VALUE"/>
</element>
<element name="D11" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="VALUE"/>
</element>
<element name="D5" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="VALUE"/>
</element>
<element name="D6" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="VALUE"/>
</element>
<element name="D7" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="VALUE"/>
</element>
<element name="D8" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="VALUE"/>
</element>
<element name="D9" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="VALUE"/>
</element>
<element name="IN" library="SparkFun-Connectors" package="1X05" value="">
<attribute name="VALUE"/>
</element>
<element name="J10" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J9" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="OUT" library="SparkFun-Connectors" package="1X05" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0805" value="1k"/>
<element name="S1" library="th_libraries" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="S2" library="th_libraries" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="S3" library="th_libraries" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="S4" library="th_libraries" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="U$1" library="SparkFun-DigitalIC" package="SO16" value="74165D">
<attribute name="VALUE"/>
</element>
<element name="U$10" library="th_libraries" package="REED_SMD" value="REED_SMD"/>
<element name="U$11" library="th_libraries" package="SOIC-18" value="ULN2803_DARLINGTON_ARRAY"/>
<element name="U$2" library="th_libraries" package="DIP16" value="ISOLATED_RESISTOR_ARRAY-8"/>
<element name="U$3" library="th_libraries" package="REED_SMD" value="REED_SMD"/>
<element name="U$4" library="th_libraries" package="REED_SMD" value="REED_SMD"/>
<element name="U$5" library="th_libraries" package="REED_SMD" value="REED_SMD"/>
<element name="U$6" library="th_libraries" package="REED_SMD" value="REED_SMD"/>
<element name="U$7" library="th_libraries" package="REED_SMD" value="REED_SMD"/>
<element name="U$8" library="th_libraries" package="REED_SMD" value="REED_SMD"/>
<element name="U$9" library="th_libraries" package="REED_SMD" value="REED_SMD"/>
<element name="X1" library="con-phoenix-508" package="MSTBA5" value="MSTBA5">
<attribute name="MF" value=""/>
<attribute name="MPN" value="1757271"/>
<attribute name="OC_FARNELL" value="3705201"/>
<attribute name="OC_NEWARK" value="71C4164"/>
</element>
</elements>
<signals>
<signal name="N$3">
<contactref element="U$1" pad="13"/>
<contactref element="4610X-1-103LF-ND" pad="P$7"/>
<contactref element="U$5" pad="3"/>
<contactref element="U$11" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="14"/>
<contactref element="4610X-1-103LF-ND" pad="P$6"/>
<contactref element="U$6" pad="3"/>
<contactref element="U$11" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="3"/>
<contactref element="4610X-1-103LF-ND" pad="P$5"/>
<contactref element="U$7" pad="3"/>
<contactref element="U$11" pad="8"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="4"/>
<contactref element="4610X-1-103LF-ND" pad="P$4"/>
<contactref element="U$8" pad="3"/>
<contactref element="U$11" pad="7"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="5"/>
<contactref element="4610X-1-103LF-ND" pad="P$3"/>
<contactref element="U$9" pad="3"/>
<contactref element="U$11" pad="6"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="6"/>
<contactref element="4610X-1-103LF-ND" pad="P$2"/>
<contactref element="U$10" pad="3"/>
<contactref element="U$11" pad="5"/>
</signal>
<signal name="QH">
<contactref element="U$1" pad="9"/>
<contactref element="IN" pad="2"/>
<contactref element="X1" pad="2"/>
</signal>
<signal name="LD">
<contactref element="U$1" pad="1"/>
<contactref element="IN" pad="4"/>
<contactref element="OUT" pad="4"/>
<contactref element="X1" pad="4"/>
</signal>
<signal name="CLK">
<contactref element="U$1" pad="2"/>
<contactref element="OUT" pad="3"/>
<contactref element="IN" pad="3"/>
<contactref element="X1" pad="3"/>
</signal>
<signal name="SER">
<contactref element="U$1" pad="10"/>
<contactref element="OUT" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="IN" pad="5"/>
<contactref element="OUT" pad="5"/>
<contactref element="U$1" pad="16"/>
<contactref element="J9" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="U$2" pad="9"/>
<contactref element="U$2" pad="11"/>
<contactref element="U$2" pad="10"/>
<contactref element="U$2" pad="12"/>
<contactref element="U$2" pad="13"/>
<contactref element="U$2" pad="14"/>
<contactref element="U$2" pad="15"/>
<contactref element="U$2" pad="16"/>
<contactref element="X1" pad="5"/>
</signal>
<signal name="GND">
<contactref element="4610X-1-103LF-ND" pad="P$1"/>
<contactref element="IN" pad="1"/>
<contactref element="OUT" pad="1"/>
<contactref element="U$1" pad="8"/>
<contactref element="U$1" pad="15"/>
<contactref element="J10" pad="1"/>
<contactref element="U$11" pad="10"/>
<contactref element="X1" pad="1"/>
<contactref element="S2" pad="P1"/>
<contactref element="S3" pad="P1"/>
<contactref element="S4" pad="P1"/>
<contactref element="S1" pad="P1"/>
</signal>
<signal name="N$9">
<contactref element="4610X-1-103LF-ND" pad="P$9"/>
<contactref element="U$1" pad="11"/>
<contactref element="U$3" pad="3"/>
<contactref element="U$11" pad="4"/>
</signal>
<signal name="N$13">
<contactref element="4610X-1-103LF-ND" pad="P$8"/>
<contactref element="U$1" pad="12"/>
<contactref element="U$4" pad="3"/>
<contactref element="U$11" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="U$3" pad="4"/>
<contactref element="U$4" pad="4"/>
<contactref element="U$5" pad="4"/>
<contactref element="U$6" pad="4"/>
<contactref element="U$7" pad="4"/>
<contactref element="U$8" pad="4"/>
<contactref element="U$9" pad="4"/>
<contactref element="U$10" pad="4"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="D10" pad="A"/>
<contactref element="U$2" pad="7"/>
</signal>
<signal name="N$20">
<contactref element="D11" pad="A"/>
<contactref element="U$2" pad="8"/>
</signal>
<signal name="N$29">
<contactref element="D7" pad="A"/>
<contactref element="U$2" pad="4"/>
</signal>
<signal name="N$30">
<contactref element="D6" pad="A"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="N$31">
<contactref element="D5" pad="A"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="N$32">
<contactref element="D2" pad="A"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="D8" pad="A"/>
<contactref element="U$2" pad="5"/>
</signal>
<signal name="N$34">
<contactref element="D9" pad="A"/>
<contactref element="U$2" pad="6"/>
</signal>
<signal name="N$1">
<contactref element="D11" pad="C"/>
<contactref element="U$11" pad="14"/>
</signal>
<signal name="N$2">
<contactref element="D2" pad="C"/>
<contactref element="U$11" pad="15"/>
</signal>
<signal name="N$11">
<contactref element="D5" pad="C"/>
<contactref element="U$11" pad="16"/>
</signal>
<signal name="N$14">
<contactref element="D6" pad="C"/>
<contactref element="U$11" pad="17"/>
</signal>
<signal name="N$18">
<contactref element="D7" pad="C"/>
<contactref element="U$11" pad="18"/>
</signal>
<signal name="N$19">
<contactref element="D8" pad="C"/>
<contactref element="U$11" pad="11"/>
</signal>
<signal name="N$21">
<contactref element="D9" pad="C"/>
<contactref element="U$11" pad="12"/>
</signal>
<signal name="N$23">
<contactref element="D10" pad="C"/>
<contactref element="U$11" pad="13"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
