<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="12.7" x2="12.7" y2="0" width="0" layer="20" curve="90"/>
<wire x1="12.7" y1="0" x2="25.4" y2="12.7" width="0" layer="20" curve="90"/>
<wire x1="25.4" y1="12.7" x2="12.7" y2="25.4" width="0" layer="20" curve="90"/>
<wire x1="12.7" y1="25.4" x2="0" y2="12.7" width="0" layer="20" curve="90"/>
<text>CuriousTech.net</text>
</plain>
<libraries>
<library name="microchip">
<packages>
<package name="SO-08">
<description>&lt;B&gt;Small Outline Narrow Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
150-mil body, package type SN</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PIC-ICSP-MINI">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BATTCON_12MM">
</package>
</packages>
</library>
<library name="CuriousTech">
<description>CuriousTech custom misc parts</description>
<packages>
<package name="TACTILE-SMD">
</package>
<package name="SMD-PAD3">
<description>SMD-PAD 0.15 x 0.0176</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="12F" library="microchip" package="SO-08" value="PIC12F675SN"/>
<element name="U$1" library="SparkFun" package="PIC-ICSP-MINI" value="PIC-ICSP-MINI"/>
<element name="R3" library="SparkFun-Passives" package="0805" value="470"/>
<element name="R2" library="SparkFun-Passives" package="0805" value="470"/>
<element name="1" library="led" package="CHIPLED_0805" value=""/>
<element name="2" library="led" package="CHIPLED_0805" value=""/>
<element name="4" library="led" package="CHIPLED_0805" value=""/>
<element name="R1" library="SparkFun-Passives" package="0805" value="470"/>
<element name="3" library="led" package="CHIPLED_0805" value=""/>
<element name="5" library="led" package="CHIPLED_0805" value=""/>
<element name="6" library="led" package="CHIPLED_0805" value=""/>
<element name="7" library="led" package="CHIPLED_0805" value=""/>
<element name="R4" library="SparkFun-Passives" package="0805" value="470"/>
<element name="8" library="led" package="CHIPLED_0805" value=""/>
<element name="9" library="led" package="CHIPLED_0805" value=""/>
<element name="10" library="led" package="CHIPLED_0805" value=""/>
<element name="11" library="led" package="CHIPLED_0805" value=""/>
<element name="12" library="led" package="CHIPLED_0805" value=""/>
<element name="R5" library="SparkFun-Passives" package="0805" value="470"/>
<element name="13" library="led" package="CHIPLED_0805" value=""/>
<element name="14" library="led" package="CHIPLED_0805" value=""/>
<element name="15" library="led" package="CHIPLED_0805" value=""/>
<element name="16" library="led" package="CHIPLED_0805" value=""/>
<element name="17" library="led" package="CHIPLED_0805" value=""/>
<element name="18" library="led" package="CHIPLED_0805" value=""/>
<element name="19" library="led" package="CHIPLED_0805" value=""/>
<element name="20" library="led" package="CHIPLED_0805" value=""/>
<element name="BAT1" library="SparkFun-Electromechanical" package="BATTCON_12MM" value="">
<attribute name="PROD_ID" value="BATT-08044"/>
</element>
<element name="U$2" library="CuriousTech" package="TACTILE-SMD" value="MOM-TACT"/>
<element name="GND" library="CuriousTech" package="SMD-PAD3" value="SMD-PAD-SM"/>
</elements>
<signals>
<signal name="GND">
<contactref element="12F" pad="8"/>
<contactref element="U$1" pad="3"/>
<contactref element="BAT1" pad="GND"/>
<contactref element="U$2" pad="2"/>
<contactref element="U$2" pad="1"/>
<contactref element="GND" pad="P$1"/>
</signal>
<signal name="VCC">
<contactref element="12F" pad="1"/>
<contactref element="U$1" pad="2"/>
<contactref element="BAT1" pad="PWR@1"/>
</signal>
<signal name="N$1">
<contactref element="12F" pad="7"/>
<contactref element="U$1" pad="4"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="12F" pad="3"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="12F" pad="6"/>
<contactref element="U$1" pad="5"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="4" pad="A"/>
<contactref element="1" pad="C"/>
<contactref element="R2" pad="2"/>
<contactref element="3" pad="C"/>
<contactref element="2" pad="A"/>
<contactref element="11" pad="A"/>
<contactref element="12" pad="C"/>
<contactref element="18" pad="C"/>
<contactref element="17" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="R3" pad="2"/>
<contactref element="4" pad="C"/>
<contactref element="5" pad="C"/>
<contactref element="6" pad="A"/>
<contactref element="3" pad="A"/>
<contactref element="7" pad="A"/>
<contactref element="8" pad="C"/>
<contactref element="16" pad="A"/>
<contactref element="15" pad="C"/>
</signal>
<signal name="N$10">
<contactref element="R1" pad="2"/>
<contactref element="5" pad="A"/>
<contactref element="6" pad="C"/>
<contactref element="2" pad="C"/>
<contactref element="1" pad="A"/>
<contactref element="9" pad="A"/>
<contactref element="10" pad="C"/>
<contactref element="19" pad="A"/>
<contactref element="20" pad="C"/>
</signal>
<signal name="N$6">
<contactref element="R4" pad="2"/>
<contactref element="7" pad="C"/>
<contactref element="8" pad="A"/>
<contactref element="9" pad="C"/>
<contactref element="10" pad="A"/>
<contactref element="11" pad="C"/>
<contactref element="12" pad="A"/>
<contactref element="13" pad="A"/>
<contactref element="14" pad="C"/>
</signal>
<signal name="N$11">
<contactref element="R1" pad="1"/>
<contactref element="12F" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="12F" pad="2"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R5" pad="2"/>
<contactref element="13" pad="C"/>
<contactref element="14" pad="A"/>
<contactref element="16" pad="C"/>
<contactref element="15" pad="A"/>
<contactref element="17" pad="C"/>
<contactref element="18" pad="A"/>
<contactref element="19" pad="C"/>
<contactref element="20" pad="A"/>
</signal>
<signal name="N$8">
<contactref element="U$2" pad="4"/>
<contactref element="12F" pad="4"/>
<contactref element="U$2" pad="3"/>
<contactref element="U$1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
