<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="53.61" y1="6.35" x2="2.27" y2="6.35" width="0.3048" layer="20"/>
<wire x1="0" y1="8.62" x2="0" y2="51.07" width="0.3048" layer="20"/>
<wire x1="0" y1="51.07" x2="2.27" y2="53.34" width="0.3048" layer="20" curve="-90"/>
<wire x1="2.27" y1="53.34" x2="53.61" y2="53.34" width="0.3048" layer="20"/>
<text>D:/SmartProjects/Snc/a4_bn_logo2.bmp</text>
<text>v1.4</text>
<wire x1="55.88" y1="8.62" x2="55.88" y2="51.07" width="0.3048" layer="20"/>
<wire x1="53.61" y1="53.34" x2="55.88" y2="51.07" width="0.3048" layer="20" curve="-90"/>
<wire x1="55.88" y1="8.62" x2="53.61" y2="6.35" width="0.3048" layer="20" curve="-90"/>
<hole x="2.54" y="8.89" drill="3.2"/>
<hole x="53.34" y="8.89" drill="3.2"/>
<hole x="2.54" y="50.8" drill="3.2"/>
<hole x="53.34" y="50.8" drill="3.2"/>
<wire x1="2.27" y1="6.35" x2="0" y2="8.62" width="0.3048" layer="20" curve="-90"/>
<text>Cerebro Charging Dock
v1.4</text>
<text>Cerebro 
Charging
Dock</text>
</plain>
<libraries>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Andy-library">
<packages>
<package name="HDSP-A">
<description>&lt;b&gt;LED DISPLAY&lt;/b&gt;&lt;p&gt;
 8-mm 1 character 7 segment, decimal point right</description>
</package>
<package name="SPDT_MOMENTRAY">
</package>
<package name="USB_VERT_MICRO_SMD">
</package>
<package name="LED_DUAL">
</package>
<package name="0805">
</package>
<package name="USB_HORZ_REINFORCED_MICRO">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIL14">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOD-123">
<description>100V/150mA 1N4148 - Super Cheap</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="DIS1" library="Andy-library" package="HDSP-A" value="HD-A1032DIGIT">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="U$1" library="Andy-library" package="SPDT_MOMENTRAY" value="SPDT_MOMENTARY"/>
<element name="U$2" library="SparkFun-DigitalIC" package="DIL14" value="ATTINY84ATTINY84-20PU"/>
<element name="U$3" library="Andy-library" package="SPDT_MOMENTRAY" value="SPDT_MOMENTARY"/>
<element name="U$4" library="Andy-library" package="SPDT_MOMENTRAY" value="SPDT_MOMENTARY"/>
<element name="U$5" library="Andy-library" package="SPDT_MOMENTRAY" value="SPDT_MOMENTARY"/>
<element name="U$6" library="Andy-library" package="USB_VERT_MICRO_SMD" value="USB_SOCKET_MICRO_VERT"/>
<element name="U$7" library="Andy-library" package="USB_VERT_MICRO_SMD" value="USB_SOCKET_MICRO_VERT"/>
<element name="U$8" library="Andy-library" package="USB_VERT_MICRO_SMD" value="USB_SOCKET_MICRO_VERT"/>
<element name="U$9" library="Andy-library" package="USB_VERT_MICRO_SMD" value="USB_SOCKET_MICRO_VERT"/>
<element name="U5" library="SparkFun-PowerIC" package="SOT23-5" value="MCP73831">
<attribute name="PROD_ID" value="IC-09995"/>
<attribute name="VALUE"/>
</element>
<element name="U$11" library="Andy-library" package="LED_DUAL" value="LED_DUAL"/>
<element name="R14" library="Andy-library" package="0805" value="100"/>
<element name="R15" library="Andy-library" package="0805" value="100">
<attribute name="VALUE"/>
</element>
<element name="R16" library="Andy-library" package="0805" value="27k">
<attribute name="VALUE"/>
</element>
<element name="C10" library="SparkFun-Capacitors" package="0805" value="4.7uF">
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="SparkFun-Capacitors" package="0805" value="4.7uF">
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun-PowerIC" package="SOT23-5" value="MCP73831">
<attribute name="PROD_ID" value="IC-09995"/>
<attribute name="VALUE"/>
</element>
<element name="U$12" library="Andy-library" package="LED_DUAL" value="LED_DUAL"/>
<element name="R1" library="Andy-library" package="0805" value="100">
<attribute name="VALUE"/>
</element>
<element name="R2" library="Andy-library" package="0805" value="100"/>
<element name="R3" library="Andy-library" package="0805" value="27k">
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="4.7uF">
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="4.7uF">
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="SparkFun-PowerIC" package="SOT23-5" value="MCP73831">
<attribute name="PROD_ID" value="IC-09995"/>
<attribute name="VALUE"/>
</element>
<element name="U$13" library="Andy-library" package="LED_DUAL" value="LED_DUAL"/>
<element name="R4" library="Andy-library" package="0805" value="100">
<attribute name="VALUE"/>
</element>
<element name="R5" library="Andy-library" package="0805" value="100"/>
<element name="R6" library="Andy-library" package="0805" value="27k">
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="4.7uF">
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="4.7uF">
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="SparkFun-PowerIC" package="SOT23-5" value="MCP73831">
<attribute name="PROD_ID" value="IC-09995"/>
<attribute name="VALUE"/>
</element>
<element name="U$14" library="Andy-library" package="LED_DUAL" value="LED_DUAL"/>
<element name="R7" library="Andy-library" package="0805" value="100">
<attribute name="VALUE"/>
</element>
<element name="R8" library="Andy-library" package="0805" value="100"/>
<element name="R9" library="Andy-library" package="0805" value="27k">
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="4.7uF">
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0805" value="4.7uF">
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="SparkFun-DiscreteSemi" package="SOD-123" value="">
<attribute name="VALUE"/>
</element>
<element name="D6" library="SparkFun-DiscreteSemi" package="SOD-123" value="">
<attribute name="VALUE"/>
</element>
<element name="D7" library="SparkFun-DiscreteSemi" package="SOD-123" value=""/>
<element name="D8" library="SparkFun-DiscreteSemi" package="SOD-123" value="">
<attribute name="VALUE"/>
</element>
<element name="R10" library="Andy-library" package="0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="0805" value="4.7uF">
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="VALUE"/>
</element>
<element name="U$15" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value=""/>
<element name="U$16" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value=""/>
<element name="U$17" library="Andy-library" package="USB_HORZ_REINFORCED_MICRO" value="USB_SOCKET_MICRO_VERTREINFORCED"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$2" pad="14"/>
<contactref element="U$7" pad="P4"/>
<contactref element="U$6" pad="P4"/>
<contactref element="U$8" pad="P4"/>
<contactref element="U$9" pad="P4"/>
<contactref element="U5" pad="2"/>
<contactref element="R16" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="U$11" pad="GC"/>
<contactref element="U1" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U$12" pad="GC"/>
<contactref element="U2" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="U$13" pad="GC"/>
<contactref element="U3" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="U$14" pad="GC"/>
<contactref element="R10" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="U$17" pad="P5"/>
<contactref element="U$17" pad="G1"/>
<contactref element="U$17" pad="G2"/>
<contactref element="U$17" pad="P$2"/>
<contactref element="U$17" pad="P$1"/>
</signal>
<signal name="5VDC">
<contactref element="U$2" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="U5" pad="4"/>
<contactref element="U$11" pad="RA"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="U$12" pad="RA"/>
<contactref element="C5" pad="1"/>
<contactref element="U2" pad="4"/>
<contactref element="U$13" pad="RA"/>
<contactref element="C7" pad="1"/>
<contactref element="U3" pad="4"/>
<contactref element="U$14" pad="RA"/>
<contactref element="C8" pad="2"/>
<contactref element="U$17" pad="P1"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="13"/>
<contactref element="DIS1" pad="10"/>
</signal>
<signal name="N$22">
<contactref element="DIS1" pad="8"/>
<contactref element="U$2" pad="12"/>
</signal>
<signal name="N$23">
<contactref element="DIS1" pad="1"/>
<contactref element="U$2" pad="11"/>
</signal>
<signal name="N$24">
<contactref element="DIS1" pad="5"/>
<contactref element="U$2" pad="10"/>
</signal>
<signal name="N$25">
<contactref element="DIS1" pad="3"/>
<contactref element="U$2" pad="9"/>
</signal>
<signal name="N$26">
<contactref element="DIS1" pad="6"/>
<contactref element="U$2" pad="8"/>
</signal>
<signal name="N$27">
<contactref element="DIS1" pad="7"/>
<contactref element="U$2" pad="6"/>
</signal>
<signal name="N$28">
<contactref element="DIS1" pad="9"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="N$31">
<contactref element="DIS1" pad="4"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="U$3" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="U$2" pad="5"/>
<contactref element="DIS1" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="U$3" pad="COMMON"/>
<contactref element="U$9" pad="P2"/>
</signal>
<signal name="N$32">
<contactref element="U$3" pad="2"/>
<contactref element="D6" pad="A"/>
</signal>
<signal name="N$33">
<contactref element="U$4" pad="COMMON"/>
<contactref element="U$8" pad="P2"/>
</signal>
<signal name="N$34">
<contactref element="U$4" pad="2"/>
<contactref element="D8" pad="A"/>
</signal>
<signal name="N$35">
<contactref element="U$1" pad="COMMON"/>
<contactref element="U$7" pad="P2"/>
</signal>
<signal name="N$36">
<contactref element="U$1" pad="2"/>
<contactref element="D5" pad="A"/>
</signal>
<signal name="N$37">
<contactref element="U$2" pad="7"/>
<contactref element="D5" pad="C"/>
<contactref element="D6" pad="C"/>
<contactref element="D8" pad="C"/>
<contactref element="D7" pad="C"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="U$5" pad="COMMON"/>
<contactref element="U$6" pad="P2"/>
</signal>
<signal name="N$39">
<contactref element="U$5" pad="2"/>
<contactref element="D7" pad="A"/>
</signal>
<signal name="N$40">
<contactref element="R16" pad="1"/>
<contactref element="U5" pad="5"/>
</signal>
<signal name="N$41">
<contactref element="U5" pad="3"/>
<contactref element="C10" pad="1"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$42">
<contactref element="R15" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="U5" pad="1"/>
</signal>
<signal name="N$43">
<contactref element="R14" pad="1"/>
<contactref element="U$11" pad="GA"/>
</signal>
<signal name="N$44">
<contactref element="U$11" pad="RC"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R3" pad="1"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="U$5" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R1" pad="1"/>
<contactref element="U$12" pad="GA"/>
</signal>
<signal name="N$6">
<contactref element="U$12" pad="RC"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R6" pad="1"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="N$8">
<contactref element="U2" pad="3"/>
<contactref element="C4" pad="1"/>
<contactref element="U$4" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R5" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R4" pad="1"/>
<contactref element="U$13" pad="GA"/>
</signal>
<signal name="N$12">
<contactref element="U$13" pad="RC"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="R9" pad="1"/>
<contactref element="U3" pad="5"/>
</signal>
<signal name="N$14">
<contactref element="U3" pad="3"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="R8" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="R7" pad="1"/>
<contactref element="U$14" pad="GA"/>
</signal>
<signal name="N$18">
<contactref element="U$14" pad="RC"/>
<contactref element="R8" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
