<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<board>
<plain>
<text>3v3</text>
<text>GND</text>
<text>CLK</text>
<text>MISO</text>
<text>MOSI</text>
<text>CS</text>
<text>SDN</text>
<text>GPIO-3</text>
<text>GPIO-2</text>
<text>GPIO-1</text>
<text>GPIO-0</text>
<text>SPSGRF-915
TEST BOARD
2017 - EEChi BOARDS</text>
<wire x1="2.54" y1="0" x2="27.94" y2="0" width="0" layer="20"/>
<wire x1="27.94" y1="0" x2="27.94" y2="20.32" width="0" layer="20"/>
<wire x1="27.94" y1="20.32" x2="2.54" y2="20.32" width="0" layer="20"/>
<wire x1="2.54" y1="20.32" x2="2.54" y2="0" width="0" layer="20"/>
<text>0,1u</text>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="1X07_LOCK">
</package>
<package name="1X04_LOCK">
</package>
</packages>
</library>
<library name="rajesh_kovvuri_eagle_library">
<description>My own library</description>
<packages>
<package name="ST_SPSGRFC">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun" package="0805" value=""/>
<element name="JP1" library="SparkFun" package="1X07_LOCK" value=""/>
<element name="JP2" library="SparkFun" package="1X04_LOCK" value=""/>
<element name="U$1" library="rajesh_kovvuri_eagle_library" package="ST_SPSGRFC" value="ST_SPSGRFC"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="P$6"/>
<contactref element="C1" pad="2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="P$5"/>
<contactref element="C1" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="P$4"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="P$3"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="P$2"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="P$1"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="CS">
<contactref element="U$1" pad="P$10"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="CK">
<contactref element="U$1" pad="P$7"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="MISO">
<contactref element="U$1" pad="P$8"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="MOSI">
<contactref element="U$1" pad="P$9"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="SDN">
<contactref element="U$1" pad="P$11"/>
<contactref element="JP1" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
