<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="-0.259" y1="-0.019" x2="19.581" y2="-0.035" width="0" layer="20"/>
<wire x1="19.581" y1="-0.035" x2="19.572" y2="15.199" width="0" layer="20"/>
<wire x1="19.572" y1="15.199" x2="-0.263" y2="15.198" width="0" layer="20"/>
<wire x1="-0.263" y1="15.198" x2="-0.259" y2="-0.019" width="0" layer="20"/>
<text>EZ-I2C MPU6050
IMU V2</text>
</plain>
<libraries>
<library name="SparkFun-Sensors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="QFN-24-NP">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="SJ_3_PASTE2&amp;3">
</package>
<package name="SJ_2S-TRACE">
<description>Solder jumper, small, shorted with trace. No paste layer. Trace is cuttable.</description>
</package>
</packages>
</library>
<library name="UniqueInteractionsLib">
<packages>
<package name="EZ-I2CHEADERV1">
</package>
</packages>
</library>
<library name="MiniWear_LOGO">
<packages>
<package name="LOGO2">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="SparkFun-Sensors" package="QFN-24-NP" value="MPU-9150">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="C1" library="SparkFun-Passives" package="0402-CAP" value="0.1uF">
<attribute name="OC_FARNELL" value="1657913RL"/>
<attribute name="MF" value="AVX"/>
<attribute name="MPN" value="02016D104KAT2A"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0402-RES" value="10k">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="0402-RES" value="10k">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Passives" package="0402-CAP" value="2.2nF">
<attribute name="OC_FARNELL" value="498592"/>
<attribute name="MF" value="AVX"/>
<attribute name="MPN" value="06035C222KAT2A"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Passives" package="0402-CAP" value="10nF">
<attribute name="OC_FARNELL" value="317433"/>
<attribute name="MF" value="AVX"/>
<attribute name="MPN" value="06035G103ZAT2A"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Passives" package="0402-CAP" value="0.1uF">
<attribute name="OC_FARNELL" value="1657913RL"/>
<attribute name="MF" value="AVX"/>
<attribute name="MPN" value="02016D104KAT2A"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="SparkFun-Passives" package="SJ_3_PASTE2&amp;3" value="">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="SJ2**" library="SparkFun-Passives" package="SJ_2S-TRACE" value="SOLDERJUMPERTRACE">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
</element>
<element name="SJ3**" library="SparkFun-Passives" package="SJ_2S-TRACE" value="SOLDERJUMPERTRACE">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
</element>
<element name="U$1" library="UniqueInteractionsLib" package="EZ-I2CHEADERV1" value="EZ-I2CHEADERV1"/>
<element name="U$2" library="MiniWear_LOGO" package="LOGO2" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="15"/>
<contactref element="U1" pad="17"/>
<contactref element="U1" pad="18"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="SJ1" pad="3"/>
<contactref element="SJ2**" pad="1"/>
<contactref element="SJ3**" pad="1"/>
<contactref element="U$1" pad="GND"/>
<contactref element="U$1" pad="GND1"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="13"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="8"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="SJ1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="U$1" pad="VCC"/>
<contactref element="U$1" pad="VCC1"/>
</signal>
<signal name="SDA">
<contactref element="U1" pad="24"/>
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="SDA"/>
<contactref element="U$1" pad="SDA1"/>
</signal>
<signal name="SCL">
<contactref element="U1" pad="23"/>
<contactref element="R2" pad="1"/>
<contactref element="U$1" pad="SCL"/>
<contactref element="U$1" pad="SCL1"/>
</signal>
<signal name="INT">
<contactref element="U1" pad="12"/>
</signal>
<signal name="AD0">
<contactref element="U1" pad="9"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="CLKOUT">
<contactref element="U1" pad="22"/>
</signal>
<signal name="ESC">
<contactref element="U1" pad="7"/>
</signal>
<signal name="ESD">
<contactref element="U1" pad="6"/>
</signal>
<signal name="CLKIN">
<contactref element="U1" pad="1"/>
<contactref element="SJ2**" pad="2"/>
</signal>
<signal name="FSYNC">
<contactref element="U1" pad="11"/>
<contactref element="SJ3**" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="20"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="10"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="BAT">
<contactref element="U$1" pad="BAT"/>
<contactref element="U$1" pad="BAT1"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="LPOW"/>
<contactref element="U$1" pad="LPOW1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
