<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="2.54" y1="-1.905" x2="48.26" y2="-1.905" width="0" layer="20"/>
<wire x1="48.26" y1="-1.905" x2="50.8" y2="0.635" width="0" layer="20" curve="90"/>
<wire x1="50.8" y1="0.635" x2="50.8" y2="22.225" width="0" layer="20"/>
<wire x1="50.8" y1="22.225" x2="48.26" y2="24.765" width="0" layer="20" curve="90"/>
<wire x1="48.26" y1="24.765" x2="2.54" y2="24.765" width="0" layer="20"/>
<wire x1="2.54" y1="24.765" x2="0" y2="22.225" width="0" layer="20" curve="90"/>
<wire x1="0" y1="22.225" x2="0" y2="0.635" width="0" layer="20"/>
<wire x1="0" y1="0.635" x2="2.54" y2="-1.905" width="0" layer="20" curve="90"/>
<text>By: Dan Watson
syncchannel.blogspot.com</text>
<text>PWR</text>
<hole x="48.5775" y="20.7645" drill="2.6"/>
<hole x="48.5775" y="2.0955" drill="2.6"/>
<text>C1</text>
<text>C2</text>
<text>R1</text>
<text>RN2903</text>
<text>RN2483/2903 FeatherWing
For Adafruit Feather</text>
<text>RN2483</text>
<text>R2</text>
<text>G10</text>
<text>RN Module ICSP</text>
<text>NODE ID</text>
<text>High Band Only</text>
<text>6/09/2016
Rev B</text>
<text>RN Module ICSP</text>
<text>LoRaWAN FeatherWing</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
<package name="SMA_EDGELAUNCH">
</package>
</packages>
</library>
<library name="adafruit2">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2,8-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 2.8 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-ConnectorsNEW">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06">
</package>
</packages>
</library>
<library name="SyncChannelCustom">
<packages>
<package name="RN2483/RN2903">
</package>
<package name="1X16_SMD_HEADER">
</package>
<package name="1X12_SMD_HEADER">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C2" library="adafruit" package="C0603" value="470nF"/>
<element name="U$1" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value=""/>
<element name="LED2" library="adafruit" package="CHIPLED_0805" value="GREEN"/>
<element name="R1" library="adafruit2" package="R0603" value="680"/>
<element name="H1" library="holes" package="2,8-PAD" value="MOUNT-PAD-ROUND2.8"/>
<element name="H2" library="holes" package="2,8-PAD" value="MOUNT-PAD-ROUND2.8"/>
<element name="C1" library="adafruit" package="C0603" value="1uF"/>
<element name="X1" library="adafruit" package="SMA_EDGELAUNCH" value="">
<attribute name="VALUE"/>
</element>
<element name="U1" library="SyncChannelCustom" package="RN2483/RN2903" value="">
<attribute name="VALUE"/>
</element>
<element name="LED1" library="adafruit" package="CHIPLED_0805" value="ORANGE"/>
<element name="R2" library="adafruit2" package="R0603" value="680"/>
<element name="J3" library="SparkFun-ConnectorsNEW" package="1X06" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SyncChannelCustom" package="1X12_SMD_HEADER" value=""/>
<element name="J1" library="SyncChannelCustom" package="1X16_SMD_HEADER" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="LED2" pad="C"/>
<contactref element="H2" pad="B2,8"/>
<contactref element="H1" pad="B2,8"/>
<contactref element="LED1" pad="C"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="X1" pad="GND@4"/>
<contactref element="X1" pad="GND@2"/>
<contactref element="X1" pad="GND@3"/>
<contactref element="X1" pad="GND@1"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="11"/>
<contactref element="U1" pad="20"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="22"/>
<contactref element="U1" pad="24"/>
<contactref element="U1" pad="26"/>
<contactref element="U1" pad="27"/>
<contactref element="U1" pad="28"/>
<contactref element="U1" pad="33"/>
<contactref element="U1" pad="47"/>
<contactref element="J3" pad="3"/>
<contactref element="J1" pad="4"/>
<contactref element="U1" pad="41"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="3V">
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="12"/>
<contactref element="U1" pad="34"/>
<contactref element="J3" pad="2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="LED2" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="LED1" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="GPIO10">
<contactref element="U1" pad="14"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="23"/>
<contactref element="X1" pad="P"/>
</signal>
<signal name="TX">
<contactref element="U1" pad="6"/>
<contactref element="J1" pad="14"/>
</signal>
<signal name="RX">
<contactref element="U1" pad="7"/>
<contactref element="J1" pad="15"/>
</signal>
<signal name="TEST0">
<contactref element="U1" pad="30"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="TEST1">
<contactref element="U1" pad="31"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="RESET">
<contactref element="U1" pad="32"/>
<contactref element="J3" pad="1"/>
<contactref element="J2" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
