<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="30" width="0.008" layer="20"/>
<wire x1="0" y1="30" x2="36" y2="30" width="0.008" layer="20"/>
<wire x1="36" y1="30" x2="36" y2="0" width="0.008" layer="20"/>
<wire x1="36" y1="0" x2="0" y2="0" width="0.008" layer="20"/>
<text>RIKKI A1200 LED</text>
<text>GND</text>
<text>3</text>
<text>2</text>
<text>1</text>
</plain>
<libraries>
<library name="a1200led">
<packages>
<package name="1X08">
<description>&lt;h3&gt;Plated Through Hole -8 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1206">
<description>&lt;p&gt;&lt;b&gt;Generic 3216 (1206) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Hardware">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
This library contains board components that are not electrical in nature, such as stand-offs, magnets, and Actobotics. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF">
<description>&lt;h3&gt;Standoff (#4 Screw)&lt;/h3&gt;
&lt;p&gt;This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components.&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;STAND-OFF&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DUMMY">
<description>&lt;h3&gt;Dummy Footprint&lt;/h3&gt;
&lt;p&gt;NOTHING HERE!!! For when you want a symbol with no package as an option against symbols with a package.&lt;/p&gt;

&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;BADGERHACK_LOGO&lt;/li&gt;
&lt;li&gt;FRAME-LETTER&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FLOPPY" library="a1200led" package="1X08" value="LTL-2450Y"/>
<element name="HDD" library="a1200led" package="1X08" value="LTL-2450Y"/>
<element name="J1" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
</element>
<element name="POWER" library="a1200led" package="1X08" value="LTL-2350HR"/>
<element name="R1" library="a1200led" package="1206" value="ERJ-8ENF51R0V"/>
<element name="R2" library="a1200led" package="1206" value="ERJ-8ENF51R0V"/>
<element name="R3" library="a1200led" package="1206" value="ERJ-8ENF40R2V"/>
<element name="R4" library="a1200led" package="1206" value="ERJ-8ENF40R2V"/>
<element name="R5" library="a1200led" package="1206" value="ERJ-8ENF40R2V"/>
<element name="R6" library="a1200led" package="1206" value="ERJ-8ENF40R2V"/>
<element name="H1" library="SparkFun-Hardware" package="STAND-OFF" value="STAND-OFF"/>
<element name="H2" library="SparkFun-Hardware" package="STAND-OFF" value="STAND-OFF"/>
<element name="FRAME1" library="SparkFun-Aesthetics" package="DUMMY" value="FRAME-LETTERNO_PACKAGE">
<attribute name="VERSION" value="v01"/>
<attribute name="DESIGNER" value="Nobody"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="POWER" pad="2"/>
<contactref element="POWER" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="POWER" pad="6"/>
<contactref element="POWER" pad="7"/>
</signal>
<signal name="N$3">
<contactref element="FLOPPY" pad="2"/>
<contactref element="FLOPPY" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="FLOPPY" pad="6"/>
<contactref element="FLOPPY" pad="7"/>
</signal>
<signal name="N$5">
<contactref element="HDD" pad="2"/>
<contactref element="HDD" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="HDD" pad="6"/>
<contactref element="HDD" pad="7"/>
</signal>
<signal name="GND">
<contactref element="HDD" pad="5"/>
<contactref element="HDD" pad="1"/>
<contactref element="FLOPPY" pad="5"/>
<contactref element="FLOPPY" pad="1"/>
<contactref element="POWER" pad="5"/>
<contactref element="POWER" pad="1"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="POWER_LED1">
<contactref element="R1" pad="1"/>
<contactref element="POWER" pad="4"/>
</signal>
<signal name="POWER_LED2">
<contactref element="R2" pad="1"/>
<contactref element="POWER" pad="8"/>
</signal>
<signal name="FLOPPY_LED1">
<contactref element="R3" pad="1"/>
<contactref element="FLOPPY" pad="4"/>
</signal>
<signal name="FLOPPY_LED2">
<contactref element="R4" pad="1"/>
<contactref element="FLOPPY" pad="8"/>
</signal>
<signal name="HDD_LED1">
<contactref element="R5" pad="1"/>
<contactref element="HDD" pad="4"/>
</signal>
<signal name="HDD_LED2">
<contactref element="R6" pad="1"/>
<contactref element="HDD" pad="8"/>
</signal>
<signal name="POWER_CONN">
<contactref element="J1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="FLOPPY_CONN">
<contactref element="J1" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="HDD_CONN">
<contactref element="J1" pad="3"/>
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
