<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="58.598" y2="0" width="0" layer="20"/>
<wire x1="58.598" y1="0" x2="58.42" y2="58.42" width="0" layer="20"/>
<wire x1="58.42" y1="58.42" x2="0" y2="58.42" width="0" layer="20"/>
<wire x1="0" y1="58.42" x2="0" y2="0" width="0" layer="20"/>
<text>C:/Users/bnold/Desktop/ResearchLogoFinal.bmp</text>
<text>C:/Users/bnold/Dropbox/Grad School/PurdueP.bmp</text>
<text>C:/Users/bnold/Dropbox/Grad School/PurdueP.bmp</text>
<text>Low Noise Switching Voltage Regulator
Designed by: Benjamin Nold
Radio Navigation Lab, Purdue University</text>
<text>GND</text>
<text>V In</text>
<text>GND</text>
<text>R2 and R3 are optional</text>
<text>GND</text>
<text>V Out</text>
<text>V Out</text>
</plain>
<libraries>
<library name="vRegPart">
<packages>
<package name="TZA07A">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1210">
<description>&lt;p&gt;&lt;b&gt;Generic 3225 (1210) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="CPOL-RADIAL-5MM-10MM">
<description>5 mm spaced PTHs in 10 mm diameter silk ring</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-5MM-2">
<description>&lt;h3&gt;Screw Terminal  5mm Pitch -2 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 5mm/197mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1210">
<description>&lt;p&gt;&lt;b&gt;Generic 3225 (1210) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Hardware">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
This library contains board components that are not electrical in nature, such as stand-offs, magnets, and Actobotics. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF">
<description>&lt;h3&gt;Standoff (#4 Screw)&lt;/h3&gt;
&lt;p&gt;This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components.&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;STAND-OFF&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="vRegPart" package="TZA07A" value="LMZ14202H_NDW_7">
<attribute name="DATASHEETURL" value="httpwww.ti.comlitdssymlinklmz14202h.pdf"/>
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="lmz14202h_ndw_7"/>
<attribute name="VENDOR" value="Texas Instruments"/>
<attribute name="BASEPN" value="LMZ14202"/>
<attribute name="NSC_PACKAGEREFERENCE" value="TZA07A"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="1210" value="4700 pF"/>
<element name="J1" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="VIn">
<attribute name="SF_SKU" value="PRT-08432"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="1210" value="C IN"/>
<element name="R1" library="SparkFun-Resistors" package="1210" value="R ON">
<attribute name="PROD_ID" value="RES-12374"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="1210" value="R ENB">
<attribute name="PROD_ID" value="RES-12374"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="1210" value="R ENT">
<attribute name="PROD_ID" value="RES-12374"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="1210" value="C FF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="1210" value="R FBT">
<attribute name="PROD_ID" value="RES-12374"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="1210" value="R FBB">
<attribute name="PROD_ID" value="RES-12374"/>
</element>
<element name="U$3" library="SparkFun-Hardware" package="STAND-OFF" value=""/>
<element name="C2" library="SparkFun-Capacitors" package="CPOL-RADIAL-5MM-10MM" value="Cout">
<attribute name="PROD_ID" value="CAP-09538"/>
</element>
<element name="U$1" library="SparkFun-Hardware" package="STAND-OFF" value=""/>
<element name="U$2" library="SparkFun-Hardware" package="STAND-OFF" value=""/>
<element name="U$4" library="SparkFun-Hardware" package="STAND-OFF" value=""/>
<element name="J2" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="VOut">
<attribute name="SF_SKU" value="PRT-08432"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="VOut">
<attribute name="SF_SKU" value="PRT-08432"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="U1" pad="8"/>
<contactref element="J1" pad="2"/>
<contactref element="C2" pad="-"/>
<contactref element="J2" pad="2"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="5"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="3"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="6"/>
<contactref element="C4" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="U1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="VOUT">
<contactref element="U1" pad="7"/>
<contactref element="R4" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C2" pad="+"/>
<contactref element="J2" pad="1"/>
<contactref element="J3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
