<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="1.0840125" y1="0" x2="57.44354375" y2="0" width="0.1524" layer="20"/>
<wire x1="57.44354375" y1="0" x2="58.598" y2="1.15445625" width="0.1524" layer="20" curve="90"/>
<wire x1="58.598" y1="1.15445625" x2="58.598" y2="15.131125" width="0.1524" layer="20"/>
<wire x1="58.598" y1="15.131125" x2="57.229125" y2="16.5" width="0.1524" layer="20" curve="90"/>
<wire x1="57.229125" y1="16.5" x2="1.283709375" y2="16.5" width="0.1524" layer="20"/>
<wire x1="1.283709375" y1="16.5" x2="0" y2="15.216290625" width="0.1524" layer="20" curve="90"/>
<wire x1="0" y1="15.216290625" x2="0" y2="1.0840125" width="0.1524" layer="20"/>
<wire x1="0" y1="1.0840125" x2="1.0840125" y2="0" width="0.1524" layer="20" curve="90"/>
<text>Thermostat
(Powered RJ11)</text>
<text>FAN
(Unpowered RJ11)</text>
<text>12V           GND</text>
<hole x="36.1315" y="8.128" drill="3.048"/>
<text>RV-Project.Com</text>
<text>RJ11 Power Board</text>
<text>V1.0   12/18/2018</text>
</plain>
<libraries>
<library name="a-lib">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="WURTHRJ11_RIGHTANGLE">
</package>
<package name="KF7.62CONNECTOR2">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="a-lib" package="WURTHRJ11_RIGHTANGLE" value="RJ11AMPHENOLRJ11RIGHTANGLE">
<attribute name="NAME"/>
<attribute name="PARTNUM" value="54601"/>
</element>
<element name="J2" library="a-lib" package="WURTHRJ11_RIGHTANGLE" value="RJ11AMPHENOLRJ11RIGHTANGLE">
<attribute name="PARTNUM" value="54601"/>
</element>
<element name="J3" library="a-lib" package="KF7.62CONNECTOR2" value="KF762-2CONNECTOR"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="J1" pad="P$5"/>
<contactref element="J2" pad="P$5"/>
</signal>
<signal name="N$2">
<contactref element="J2" pad="P$4"/>
<contactref element="J1" pad="P$4"/>
</signal>
<signal name="N$3">
<contactref element="J1" pad="P$3"/>
<contactref element="J2" pad="P$3"/>
</signal>
<signal name="N$4">
<contactref element="J2" pad="P$2"/>
<contactref element="J1" pad="P$2"/>
</signal>
<signal name="N$5">
<contactref element="J3" pad="2A"/>
<contactref element="J1" pad="P$1"/>
</signal>
<signal name="N$6">
<contactref element="J1" pad="P$6"/>
<contactref element="J3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
