<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="36.5" y2="0" width="0" layer="20"/>
<wire x1="36.5" y1="0" x2="36.5" y2="18.3" width="0" layer="20"/>
<wire x1="36.5" y1="18.3" x2="0" y2="18.3" width="0" layer="20"/>
<wire x1="0" y1="18.3" x2="0" y2="0" width="0" layer="20"/>
<text>HV
RELAY
ARRAY</text>
<text>Rev 1</text>
<text>OUT4</text>
<text>OUT3</text>
<text>OUT2</text>
<text>OUT1</text>
<text>AVCC</text>
<text>OUT5</text>
<text>OUT6</text>
<text>OUT7</text>
<text>OUT8</text>
<text>IN5</text>
<text>IN4</text>
<text>IN3</text>
<text>IN2</text>
<text>IN1</text>
<text>IN6</text>
<text>IN7</text>
<text>IN8</text>
<text>GND</text>
</plain>
<libraries>
<library name="_relay">
<packages>
<package name="SOP254P609X203-4">
<description>4-SOP, 2.54 mm pitch, 6.10 mm span, 4.09 X 3.81 X 2.03 mm body
&lt;p&gt;4-pin SOP package with 2.54 mm pitch, 6.10 mm span with body size 4.09 X 3.81 X 2.03 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="_resistors">
<packages>
<package name="RESC1005X35_SMD-0402">
<description>CHIP, 1 X 0.5 X 0.35 mm body
&lt;p&gt;CHIP package with body size 1 X 0.5 X 0.35 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="_connectors">
<packages>
<package name="HDRV9W64P254_1X9_2286X254X838B">
<description>Single-row, 9-pin Pin Header (Male) Straight, 2.54 mm (0.10 in) col pitch, 5.84 mm mating length, 22.86 X 2.54 X 8.38 mm body
&lt;p&gt;Single-row (1X9), 9-pin Pin Header (Male) Straight package with 2.54 mm (0.10 in) col pitch, 0.64 mm lead width, 3.05 mm tail length and 5.84 mm mating length with overall size 22.86 X 2.54 X 8.38 mm, pin pattern - zigzag from bottom left&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="RELAY1" library="_relay" package="SOP254P609X203-4" value="SPST-NO 170mA 250V">
<attribute name="DATASHEET" value="http://www.ixysic.com/home/pdfs.nsf/www/CPC1010N.pdf/$file/CPC1010N.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=CPC1010N-ND"/>
<attribute name="DISTPN" value="CPC1010N-ND"/>
<attribute name="MFR" value="IXYS Integrated Circuits Division"/>
<attribute name="MPN" value="CPC1010N"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RELAY2" library="_relay" package="SOP254P609X203-4" value="SPST-NO 170mA 250V">
<attribute name="DATASHEET" value="http://www.ixysic.com/home/pdfs.nsf/www/CPC1010N.pdf/$file/CPC1010N.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=CPC1010N-ND"/>
<attribute name="DISTPN" value="CPC1010N-ND"/>
<attribute name="MFR" value="IXYS Integrated Circuits Division"/>
<attribute name="MPN" value="CPC1010N"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RELAY3" library="_relay" package="SOP254P609X203-4" value="SPST-NO 170mA 250V">
<attribute name="DATASHEET" value="http://www.ixysic.com/home/pdfs.nsf/www/CPC1010N.pdf/$file/CPC1010N.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=CPC1010N-ND"/>
<attribute name="DISTPN" value="CPC1010N-ND"/>
<attribute name="MFR" value="IXYS Integrated Circuits Division"/>
<attribute name="MPN" value="CPC1010N"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RELAY4" library="_relay" package="SOP254P609X203-4" value="SPST-NO 170mA 250V">
<attribute name="DATASHEET" value="http://www.ixysic.com/home/pdfs.nsf/www/CPC1010N.pdf/$file/CPC1010N.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=CPC1010N-ND"/>
<attribute name="DISTPN" value="CPC1010N-ND"/>
<attribute name="MFR" value="IXYS Integrated Circuits Division"/>
<attribute name="MPN" value="CPC1010N"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RELAY5" library="_relay" package="SOP254P609X203-4" value="SPST-NO 170mA 250V">
<attribute name="DATASHEET" value="http://www.ixysic.com/home/pdfs.nsf/www/CPC1010N.pdf/$file/CPC1010N.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=CPC1010N-ND"/>
<attribute name="DISTPN" value="CPC1010N-ND"/>
<attribute name="MFR" value="IXYS Integrated Circuits Division"/>
<attribute name="MPN" value="CPC1010N"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RELAY6" library="_relay" package="SOP254P609X203-4" value="SPST-NO 170mA 250V">
<attribute name="DATASHEET" value="http://www.ixysic.com/home/pdfs.nsf/www/CPC1010N.pdf/$file/CPC1010N.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=CPC1010N-ND"/>
<attribute name="DISTPN" value="CPC1010N-ND"/>
<attribute name="MFR" value="IXYS Integrated Circuits Division"/>
<attribute name="MPN" value="CPC1010N"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="_resistors" package="RESC1005X35_SMD-0402" value="1K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-1.0KJRCT-ND"/>
<attribute name="DISTPN" value="311-1.0KJRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-071KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="_resistors" package="RESC1005X35_SMD-0402" value="1K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-1.0KJRCT-ND"/>
<attribute name="DISTPN" value="311-1.0KJRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-071KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="_resistors" package="RESC1005X35_SMD-0402" value="1K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-1.0KJRCT-ND"/>
<attribute name="DISTPN" value="311-1.0KJRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-071KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="_resistors" package="RESC1005X35_SMD-0402" value="1K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-1.0KJRCT-ND"/>
<attribute name="DISTPN" value="311-1.0KJRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-071KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="_resistors" package="RESC1005X35_SMD-0402" value="1K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-1.0KJRCT-ND"/>
<attribute name="DISTPN" value="311-1.0KJRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-071KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="_resistors" package="RESC1005X35_SMD-0402" value="1K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-1.0KJRCT-ND"/>
<attribute name="DISTPN" value="311-1.0KJRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-071KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RELAY7" library="_relay" package="SOP254P609X203-4" value="SPST-NO 170mA 250V">
<attribute name="DATASHEET" value="http://www.ixysic.com/home/pdfs.nsf/www/CPC1010N.pdf/$file/CPC1010N.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=CPC1010N-ND"/>
<attribute name="DISTPN" value="CPC1010N-ND"/>
<attribute name="MFR" value="IXYS Integrated Circuits Division"/>
<attribute name="MPN" value="CPC1010N"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RELAY8" library="_relay" package="SOP254P609X203-4" value="SPST-NO 170mA 250V">
<attribute name="DATASHEET" value="http://www.ixysic.com/home/pdfs.nsf/www/CPC1010N.pdf/$file/CPC1010N.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=CPC1010N-ND"/>
<attribute name="DISTPN" value="CPC1010N-ND"/>
<attribute name="MFR" value="IXYS Integrated Circuits Division"/>
<attribute name="MPN" value="CPC1010N"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="_resistors" package="RESC1005X35_SMD-0402" value="1K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-1.0KJRCT-ND"/>
<attribute name="DISTPN" value="311-1.0KJRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-071KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="_resistors" package="RESC1005X35_SMD-0402" value="1K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-1.0KJRCT-ND"/>
<attribute name="DISTPN" value="311-1.0KJRCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0402JR-071KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="_connectors" package="HDRV9W64P254_1X9_2286X254X838B" value="PTH VERT MALE">
<attribute name="DATASHEET" value="https://drawings-pdf.s3.amazonaws.com/C10436.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=S1012E-09-ND"/>
<attribute name="DISTPN" value="S1012E-09-ND"/>
<attribute name="MFR" value="Sullins Connector Solutions"/>
<attribute name="MPN" value="PEC09SAAN"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="_connectors" package="HDRV9W64P254_1X9_2286X254X838B" value="PTH VERT MALE">
<attribute name="DATASHEET" value="https://drawings-pdf.s3.amazonaws.com/C10436.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=S1012E-09-ND"/>
<attribute name="DISTPN" value="S1012E-09-ND"/>
<attribute name="MFR" value="Sullins Connector Solutions"/>
<attribute name="MPN" value="PEC09SAAN"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="J1" pad="9"/>
</signal>
<signal name="AVCC">
<contactref element="RELAY6" pad="4"/>
<contactref element="RELAY5" pad="4"/>
<contactref element="RELAY4" pad="4"/>
<contactref element="RELAY3" pad="4"/>
<contactref element="RELAY2" pad="4"/>
<contactref element="RELAY1" pad="4"/>
<contactref element="RELAY8" pad="4"/>
<contactref element="RELAY7" pad="4"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="RELAY1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="2"/>
<contactref element="RELAY2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="2"/>
<contactref element="RELAY3" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R4" pad="2"/>
<contactref element="RELAY4" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R5" pad="2"/>
<contactref element="RELAY5" pad="2"/>
</signal>
<signal name="IN4">
<contactref element="RELAY4" pad="1"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="IN3">
<contactref element="RELAY3" pad="1"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="IN2">
<contactref element="RELAY2" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="IN1">
<contactref element="RELAY1" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="OUT1">
<contactref element="RELAY1" pad="3"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="OUT2">
<contactref element="RELAY2" pad="3"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="OUT3">
<contactref element="RELAY3" pad="3"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="OUT4">
<contactref element="RELAY4" pad="3"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="N$18">
<contactref element="R6" pad="2"/>
<contactref element="RELAY6" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="R7" pad="2"/>
<contactref element="RELAY7" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="R8" pad="2"/>
<contactref element="RELAY8" pad="2"/>
</signal>
<signal name="IN5">
<contactref element="RELAY5" pad="1"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="IN6">
<contactref element="RELAY6" pad="1"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="IN7">
<contactref element="RELAY7" pad="1"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="IN8">
<contactref element="RELAY8" pad="1"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="OUT5">
<contactref element="RELAY5" pad="3"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="OUT6">
<contactref element="RELAY6" pad="3"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="OUT7">
<contactref element="RELAY7" pad="3"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="OUT8">
<contactref element="RELAY8" pad="3"/>
<contactref element="J2" pad="9"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
