<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="19.284" y2="0" width="0" layer="20"/>
<wire x1="19.284" y1="0" x2="19.284" y2="21.768" width="0" layer="20"/>
<wire x1="19.284" y1="21.768" x2="0" y2="21.768" width="0" layer="20"/>
<wire x1="0" y1="21.768" x2="0" y2="0" width="0" layer="20"/>
<text>VBATT</text>
</plain>
<libraries>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
<description>&lt;h3&gt;SOT23-3X&lt;/h3&gt;

&lt;ul&gt;
&lt;li&gt;Total Size: 3mm x 2.5mm&lt;/li&gt;
&lt;li&gt;Landing Pad Size: .8mm x .9mm&lt;/li&gt;
&lt;li&gt;Pitch: 2 (vertical) .95mm (horizontal)&lt;/li&gt;
&lt;li&gt;&lt;/li&gt;
&lt;li&gt;&lt;/li&gt;
&lt;li&gt;&lt;/li&gt;
&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
<description>SOT23-3</description>
</package>
<package name="SOD-323">
<description>SOD-323 (Small Outline Diode)</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08">
<description>&lt;h3&gt;Plated Through Hole -8 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X01">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23-3" value="220mA/50V/3.5Ω">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-00830"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="SOT23-3" value="220mA/50V/3.5Ω">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-00830"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="SparkFun-DiscreteSemi" package="SOT23-3" value="220mA/50V/3.5Ω">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-00830"/>
<attribute name="VALUE"/>
</element>
<element name="Q4" library="SparkFun-DiscreteSemi" package="SOT23-3" value="220mA/50V/3.5Ω">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-00830"/>
<attribute name="VALUE"/>
</element>
<element name="Q5" library="SparkFun-DiscreteSemi" package="SOT23-3" value="220mA/50V/3.5Ω">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-00830"/>
<attribute name="VALUE"/>
</element>
<element name="Q6" library="SparkFun-DiscreteSemi" package="SOT23-3" value="220mA/50V/3.5Ω">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-00830"/>
<attribute name="VALUE"/>
</element>
<element name="Q7" library="SparkFun-DiscreteSemi" package="SOT23-3" value="220mA/50V/3.5Ω">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-00830"/>
<attribute name="VALUE"/>
</element>
<element name="Q8" library="SparkFun-DiscreteSemi" package="SOT23-3" value="2.5A/30V/105mΩ">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-11308"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603" value="100k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07828"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-DiscreteSemi" package="SOD-323" value="1A/23V/620mV">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-11623"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="Q1" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="Q2" pad="1"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="Q3" pad="1"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="Q4" pad="1"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="Q5" pad="1"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="N$6">
<contactref element="Q6" pad="1"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="N$7">
<contactref element="Q7" pad="1"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="N$8">
<contactref element="Q1" pad="3"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="Q2" pad="3"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="Q3" pad="3"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="N$11">
<contactref element="Q4" pad="3"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="N$12">
<contactref element="Q5" pad="3"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="N$13">
<contactref element="Q6" pad="3"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="N$14">
<contactref element="Q7" pad="3"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="GND">
<contactref element="Q4" pad="2"/>
<contactref element="Q7" pad="2"/>
<contactref element="Q3" pad="2"/>
<contactref element="Q6" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="Q5" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="J3" pad="2"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="V_BATT">
<contactref element="Q8" pad="3"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="V_USB">
<contactref element="R1" pad="2"/>
<contactref element="Q8" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="VDD">
<contactref element="Q8" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="J3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
