<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="46.66" y2="0" width="0" layer="20"/>
<wire x1="46.66" y1="0" x2="46.66" y2="80" width="0" layer="20"/>
<wire x1="46.66" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="LilyPad-Wearables">
<packages>
<package name="SIMPLE_HOLE">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-3.5MM-2">
</package>
</packages>
</library>
<library name="matt-Teensy">
<packages>
<package name="TEENSY_3.0_BASIC">
</package>
</packages>
</library>
<library name="maxstream">
<description>&lt;b&gt;MaxSream&lt;/b&gt; XBee Products&lt;p&gt;
http://www.maxstream.net</description>
<packages>
<package name="XBEE-PRO">
<description>&lt;b&gt;XBEE Pro&lt;/b&gt;&lt;p&gt;
Source: http://www.maxstream.net/products/xbee/datasheet_XBee_OEM_RF-Modules.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="3VREG" library="linear" package="SOT223" value="MCP1703DB"/>
<element name="C1" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0603-CAP" value="4.7uF">
<attribute name="PROD_ID" value="CAP-08280"/>
</element>
<element name="GND" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="H1" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="H3" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="H4" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="H5" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="H6" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="BUTTON_0" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="M023.5MM"/>
<element name="TEENSY_3.0" library="matt-Teensy" package="TEENSY_3.0_BASIC" value="TEENSY_3.0_BASIC"/>
<element name="XB1" library="maxstream" package="XBEE-PRO" value="XBEE-PRO">
<attribute name="MF" value=""/>
<attribute name="MPN" value="XBP24-AWI-001"/>
<attribute name="OC_NEWARK" value="42M2667"/>
<attribute name="OC_FARNELL" value="1337916"/>
</element>
<element name="BUTTON_1" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="M023.5MM"/>
<element name="BUTTON_2" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="M023.5MM"/>
</elements>
<signals>
<signal name="AGND">
<contactref element="TEENSY_3.0" pad="AGND"/>
</signal>
<signal name="VBAT">
<contactref element="TEENSY_3.0" pad="VBAT"/>
</signal>
<signal name="GND">
<contactref element="TEENSY_3.0" pad="GND"/>
<contactref element="TEENSY_3.0" pad="GND1"/>
<contactref element="XB1" pad="10"/>
<contactref element="GND" pad="P$1"/>
<contactref element="H3" pad="P$1"/>
<contactref element="H4" pad="P$1"/>
<contactref element="H1" pad="P$1"/>
<contactref element="3VREG" pad="2"/>
<contactref element="H5" pad="P$1"/>
<contactref element="H6" pad="P$1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="BUTTON_0" pad="1"/>
<contactref element="BUTTON_1" pad="1"/>
<contactref element="BUTTON_2" pad="1"/>
</signal>
<signal name="5VDC">
<contactref element="TEENSY_3.0" pad="VIN"/>
<contactref element="3VREG" pad="1"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="XBEE_OUT">
<contactref element="XB1" pad="2"/>
<contactref element="TEENSY_3.0" pad="0"/>
</signal>
<signal name="3.3VDC">
<contactref element="XB1" pad="1"/>
<contactref element="3VREG" pad="3"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="T3.3">
<contactref element="TEENSY_3.0" pad="3.3V"/>
<contactref element="TEENSY_3.0" pad="3.3V1"/>
</signal>
<signal name="MEMCS">
<contactref element="TEENSY_3.0" pad="6"/>
</signal>
<signal name="MOSI">
<contactref element="TEENSY_3.0" pad="7"/>
</signal>
<signal name="BCLK">
<contactref element="TEENSY_3.0" pad="9"/>
</signal>
<signal name="SDCS">
<contactref element="TEENSY_3.0" pad="10"/>
</signal>
<signal name="MCLK">
<contactref element="TEENSY_3.0" pad="11"/>
</signal>
<signal name="MISO">
<contactref element="TEENSY_3.0" pad="12"/>
</signal>
<signal name="XBEE_IN">
<contactref element="TEENSY_3.0" pad="1"/>
<contactref element="XB1" pad="3"/>
</signal>
<signal name="BUTTON_0">
<contactref element="TEENSY_3.0" pad="2"/>
<contactref element="BUTTON_0" pad="2"/>
</signal>
<signal name="BUTTON_1">
<contactref element="TEENSY_3.0" pad="3"/>
<contactref element="BUTTON_1" pad="2"/>
</signal>
<signal name="BUTTON_2">
<contactref element="TEENSY_3.0" pad="4"/>
<contactref element="BUTTON_2" pad="2"/>
</signal>
<signal name="XBEE_IN_AUX">
<contactref element="TEENSY_3.0" pad="5"/>
</signal>
<signal name="XBEE_OUT_AUX">
<contactref element="TEENSY_3.0" pad="21/A7"/>
</signal>
<signal name="N$1">
<contactref element="TEENSY_3.0" pad="13"/>
</signal>
<signal name="N$2">
<contactref element="TEENSY_3.0" pad="14/A0"/>
</signal>
<signal name="N$3">
<contactref element="TEENSY_3.0" pad="15/A1"/>
</signal>
<signal name="N$4">
<contactref element="TEENSY_3.0" pad="18/A4"/>
</signal>
<signal name="N$5">
<contactref element="TEENSY_3.0" pad="19/A5"/>
</signal>
<signal name="N$7">
<contactref element="TEENSY_3.0" pad="22/A8"/>
</signal>
<signal name="N$8">
<contactref element="TEENSY_3.0" pad="23/A9"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
