<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.1">
<drawing>
<board>
<plain>
<wire x1="98.74" y1="80" x2="1.27" y2="80" width="0" layer="20"/>
<wire x1="1.27" y1="80" x2="0" y2="78.73" width="0" layer="20" curve="90"/>
<wire x1="0" y1="78.73" x2="0" y2="35.56" width="0" layer="20"/>
<wire x1="0" y1="35.56" x2="1.27" y2="34.29" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="34.29" x2="98.73" y2="34.29" width="0" layer="20"/>
<wire x1="98.73" y1="34.29" x2="100" y2="35.56" width="0" layer="20" curve="90"/>
<wire x1="100" y1="35.56" x2="100" y2="78.74" width="0" layer="20"/>
<wire x1="100" y1="78.74" x2="98.74" y2="80" width="0" layer="20" curve="90"/>
<text>Pins 0-13 inc</text>
<text>Pins 14 (A0) -&gt; 23 (A9)</text>
<text>Xbee Series 2</text>
<text>       Teensy LC / 3.2
Must not be USB powered!</text>
<text>DC 12V Max</text>
<text>3.3v</text>
<text>3.3v</text>
<text>5v</text>
<text>5v</text>
<text>GND</text>
<text>GND</text>
<text>JB (2018)</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-10UF-25V">
</package>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="POWER_JACK_PTH">
</package>
<package name="1X10">
<description>&lt;h3&gt;Plated Through Hole -10 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_10&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="AUDIO-JACK-KIT">
<description>&lt;h3&gt;3.5mm Stereo Audio Jack -Kit Version&lt;/h3&gt;
Reduced openings in tStop, pins spread a tiny bit out to hold part on PCB during assembly
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Audio-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Audio_Jack&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="RCA">
<description>&lt;h3&gt;RCA Jack - Plated Through-Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Connectors/RCA-Jack.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;RCA&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X05">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X4">
<description>&lt;h3&gt;Plated Through Hole - 2x4&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X14">
<description>&lt;h3&gt;Plated Through Hole -14 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:14&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_14&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TEENSY-3.1">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="SML0805">
<description>&lt;b&gt;SML0805-2CW-TR (0805 PROFILE)&lt;/b&gt; COOL WHITE&lt;p&gt;
Source: http://www.ledtronics.com/ds/smd-0603/Dstr0093.pdf</description>
</package>
</packages>
</library>
<library name="ST Microelctronics_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 15:32:30</description>
<packages>
<package name="TO254P450X1020X2000-3P">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-RF">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find things that send or receive RF- GPS, cellular modules, Bluetooth, WiFi, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="XBEE-SILK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value=""/>
<element name="C10" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value=""/>
<element name="C11" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value=""/>
<element name="C2" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value=""/>
<element name="C8" library="SparkFun-Capacitors" package="0805" value=""/>
<element name="C9" library="SparkFun-Capacitors" package="0805" value=""/>
<element name="J1" library="SparkFun-Connectors" package="POWER_JACK_PTH" value="POWER_JACKPTH">
<attribute name="PROD_ID" value="CONN-08197"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X10" value="">
<attribute name="PROD_ID" value="CONN-11563"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="2X4" value="">
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="AUDIO-JACK-KIT" value="AUDIO_JACK_3.5MM_KIT">
<attribute name="PROD_ID" value="CONN-08774"/>
<attribute name="SF_ID" value="PRT-08032"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="RCA" value="RCA">
<attribute name="PROD_ID" value="CONN-09081"/>
<attribute name="SF_ID" value="PRT-08631"/>
</element>
<element name="J6" library="SparkFun-Boards" package="TEENSY-3.1" value="TEENSY-3.2">
<attribute name="SF_ID" value="DEV-12646"/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="SparkFun-Connectors" package="1X05" value="">
<attribute name="VALUE"/>
</element>
<element name="J8" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="J9" library="SparkFun-Connectors" package="1X14" value=""/>
<element name="LED1" library="led" package="SML0805" value="RSSI">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="SML0805" value="ASSOC">
<attribute name="VALUE"/>
</element>
<element name="LED3" library="led" package="SML0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="led" package="SML0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="ST Microelctronics_By_element14_Batch_1" package="TO254P450X1020X2000-3P" value="LF50ABP">
<attribute name="MPN" value="LF50ABP"/>
<attribute name="OC_FARNELL" value="1087189"/>
<attribute name="OC_NEWARK" value="26M0234"/>
<attribute name="PACKAGE" value="TO-220"/>
<attribute name="SUPPLIER" value="STMicroelectronics"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0805" value=""/>
<element name="R10" library="SparkFun-Passives" package="0805" value="220"/>
<element name="R2" library="SparkFun-Passives" package="0805" value="1k"/>
<element name="R3" library="SparkFun-Passives" package="0805" value="220"/>
<element name="R4" library="SparkFun-Passives" package="0805" value="220"/>
<element name="R5" library="SparkFun-Passives" package="0805" value="220"/>
<element name="R6" library="SparkFun-Passives" package="0805" value="220"/>
<element name="R7" library="SparkFun-Passives" package="0805" value="220"/>
<element name="R8" library="SparkFun-Passives" package="0805" value="220"/>
<element name="R9" library="SparkFun-Passives" package="0805" value="220"/>
<element name="U$1" library="SparkFun-RF" package="XBEE-SILK" value="XBEE-1B2"/>
</elements>
<signals>
<signal name="GND">
<contactref element="Q2" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="U$1" pad="10"/>
<contactref element="LED1" pad="C"/>
<contactref element="LED2" pad="C"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="J1" pad="GND"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="LED3" pad="C"/>
<contactref element="LED4" pad="C"/>
<contactref element="J6" pad="GND1"/>
</signal>
<signal name="3.3V">
<contactref element="U$1" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="J6" pad="3.3V"/>
<contactref element="J3" pad="5"/>
<contactref element="J3" pad="6"/>
</signal>
<signal name="5V">
<contactref element="Q2" pad="3"/>
<contactref element="C10" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="J6" pad="VIN"/>
<contactref element="J3" pad="4"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="VIN">
<contactref element="Q2" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="J1" pad="PWR"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$19">
<contactref element="LED2" pad="A"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="R1" pad="2"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="N$21">
<contactref element="U$1" pad="15"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="U$1" pad="13"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R4" pad="2"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="3"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="R4" pad="1"/>
<contactref element="J6" pad="0"/>
<contactref element="J9" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="R3" pad="1"/>
<contactref element="J9" pad="2"/>
<contactref element="J6" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="R6" pad="1"/>
<contactref element="J6" pad="5"/>
<contactref element="J9" pad="6"/>
</signal>
<signal name="N$6">
<contactref element="R6" pad="2"/>
<contactref element="U$1" pad="9"/>
</signal>
<signal name="AGND">
<contactref element="J6" pad="AGND"/>
</signal>
<signal name="N$2">
<contactref element="R5" pad="2"/>
<contactref element="J6" pad="2"/>
<contactref element="J9" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="J6" pad="14"/>
<contactref element="J2" pad="10"/>
</signal>
<signal name="N$4">
<contactref element="J2" pad="9"/>
<contactref element="J6" pad="15"/>
</signal>
<signal name="N$9">
<contactref element="J6" pad="16"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="N$10">
<contactref element="J2" pad="7"/>
<contactref element="J6" pad="17"/>
</signal>
<signal name="N$11">
<contactref element="J2" pad="6"/>
<contactref element="J6" pad="18"/>
</signal>
<signal name="N$12">
<contactref element="J6" pad="19"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="N$13">
<contactref element="J2" pad="4"/>
<contactref element="J6" pad="20"/>
</signal>
<signal name="N$14">
<contactref element="J6" pad="21"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="J2" pad="2"/>
<contactref element="J6" pad="22"/>
</signal>
<signal name="N$16">
<contactref element="J6" pad="23"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="J6" pad="4"/>
<contactref element="J9" pad="5"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="J6" pad="7"/>
<contactref element="J9" pad="8"/>
</signal>
<signal name="N$26">
<contactref element="J6" pad="8"/>
<contactref element="J9" pad="9"/>
</signal>
<signal name="N$29">
<contactref element="J6" pad="10"/>
<contactref element="J9" pad="11"/>
</signal>
<signal name="N$31">
<contactref element="J6" pad="11"/>
<contactref element="J9" pad="12"/>
</signal>
<signal name="N$32">
<contactref element="J6" pad="12"/>
<contactref element="J9" pad="13"/>
</signal>
<signal name="N$33">
<contactref element="J6" pad="13"/>
<contactref element="J9" pad="14"/>
</signal>
<signal name="N$34">
<contactref element="J4" pad="SLEEVE"/>
<contactref element="J7" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="J7" pad="2"/>
<contactref element="J4" pad="RING"/>
</signal>
<signal name="N$37">
<contactref element="J4" pad="RSH"/>
<contactref element="J7" pad="3"/>
</signal>
<signal name="N$41">
<contactref element="J7" pad="4"/>
<contactref element="J4" pad="TSH"/>
</signal>
<signal name="N$42">
<contactref element="J4" pad="TIP"/>
<contactref element="J7" pad="5"/>
</signal>
<signal name="N$43">
<contactref element="J5" pad="PIN"/>
<contactref element="J8" pad="3"/>
</signal>
<signal name="N$44">
<contactref element="J8" pad="2"/>
<contactref element="J5" pad="SHELL"/>
</signal>
<signal name="N$45">
<contactref element="J5" pad="SWITCH"/>
<contactref element="J8" pad="1"/>
</signal>
<signal name="N$39">
<contactref element="J9" pad="4"/>
<contactref element="J6" pad="3"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$46">
<contactref element="J6" pad="6"/>
<contactref element="J9" pad="7"/>
</signal>
<signal name="N$24">
<contactref element="J9" pad="10"/>
<contactref element="J6" pad="9"/>
</signal>
<signal name="N$27">
<contactref element="U$1" pad="16"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$40">
<contactref element="R8" pad="1"/>
<contactref element="U$1" pad="12"/>
</signal>
<signal name="N$5">
<contactref element="J3" pad="7"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="R9" pad="1"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$36">
<contactref element="LED4" pad="A"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$38">
<contactref element="R10" pad="2"/>
<contactref element="J3" pad="8"/>
</signal>
<signal name="N$47">
</signal>
<signal name="N$48">
</signal>
<signal name="N$49">
</signal>
<signal name="N$51">
</signal>
<signal name="N$52">
<contactref element="J3" pad="1"/>
<contactref element="J6" pad="GND"/>
<contactref element="J3" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
