<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0.127" y1="0" x2="82.931" y2="0" width="0" layer="20"/>
<wire x1="82.931" y1="0" x2="82.931" y2="38.1762" width="0" layer="20"/>
<wire x1="82.931" y1="38.1762" x2="0.127" y2="38.1762" width="0" layer="20"/>
<wire x1="0.127" y1="38.1762" x2="0.127" y2="0" width="0" layer="20"/>
<text>Title: Padiddle
Rev: 1.2
Designer: Kevin J Dolan
Date: 1/2/2014</text>
<text>VCC</text>
<text>GND</text>
<hole x="62.484" y="36.068" drill="0.6"/>
<hole x="20.828" y="36.068" drill="0.6"/>
<text>Penalty</text>
<text>Score</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>14</text>
<hole x="1.778" y="1.778" drill="0.6"/>
<hole x="80.264" y="1.778" drill="0.6"/>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>14</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH-LED-12MM">
</package>
</packages>
</library>
<library name="SparkFun-Displays">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of display devices- LED displays, LCD displays, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="7-SEGMENT-1&quot;PTH">
<description>7 Segment display Storefront SKU#: COM-08546</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X14">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="L-SCORE" library="adafruit" package="LED5MM" value="Green">
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="L-P1" library="adafruit" package="LED5MM" value="Red">
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="L-P2" library="adafruit" package="LED5MM" value="Red">
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="R-P1" library="adafruit" package="LED5MM" value="Red">
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="R-P2" library="adafruit" package="LED5MM" value="Red">
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="R-SCORE" library="adafruit" package="LED5MM" value="Green">
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="BTN-SCORE" library="SparkFun-Electromechanical" package="TACTILE-PTH-LED-12MM" value="SWITCH-MOMENTARY-LEDPTH">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="BTN-PENALTY" library="SparkFun-Electromechanical" package="TACTILE-PTH-LED-12MM" value="SWITCH-MOMENTARY-LEDPTH">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="7SEG-L" library="SparkFun-Displays" package="7-SEGMENT-1&quot;PTH" value="7-SEGMENT-DISPLAY-1&quot;-RED">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="7SEG-R" library="SparkFun-Displays" package="7-SEGMENT-1&quot;PTH" value="7-SEGMENT-DISPLAY-1&quot;-RED">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="SR-A" library="SparkFun-DigitalIC" package="DIL16" value="74LS595N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="67K1099"/>
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="SN74LS595N"/>
</element>
<element name="SR-B" library="SparkFun-DigitalIC" package="DIL16" value="74LS595N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="67K1099"/>
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="SN74LS595N"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X14" value="M14">
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="R1" library="adafruit" package="R0805" value="200Ω">
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="11M7214"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="PFC-W0805LF-03-2000-B"/>
</element>
<element name="R3" library="adafruit" package="R0805" value="200Ω">
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="11M7214"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="PFC-W0805LF-03-2000-B"/>
</element>
<element name="R2" library="adafruit" package="R0805" value="200Ω">
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="11M7214"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="PFC-W0805LF-03-2000-B"/>
</element>
<element name="R5" library="adafruit" package="R0805" value="200Ω">
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="11M7214"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="PFC-W0805LF-03-2000-B"/>
</element>
<element name="R6" library="adafruit" package="R0805" value="200Ω">
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="11M7214"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="PFC-W0805LF-03-2000-B"/>
</element>
<element name="R7" library="adafruit" package="R0805" value="200Ω">
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="11M7214"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="PFC-W0805LF-03-2000-B"/>
</element>
<element name="R8" library="adafruit" package="R0805" value="200Ω">
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="11M7214"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="PFC-W0805LF-03-2000-B"/>
</element>
<element name="R9" library="adafruit" package="R0805" value="200Ω">
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="11M7214"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="PFC-W0805LF-03-2000-B"/>
</element>
<element name="R4" library="adafruit" package="R0805" value="200Ω">
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="11M7214"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="PFC-W0805LF-03-2000-B"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="SR-A" pad="8"/>
<contactref element="SR-A" pad="13"/>
<contactref element="SR-B" pad="8"/>
<contactref element="SR-B" pad="13"/>
<contactref element="JP1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="L-P1" pad="K"/>
<contactref element="L-P2" pad="K"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="L-SCORE" pad="K"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R-SCORE" pad="K"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R-P1" pad="K"/>
<contactref element="R-P2" pad="K"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="BTN_LED_NEG">
<contactref element="BTN-SCORE" pad="C"/>
<contactref element="BTN-PENALTY" pad="C"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="SRA-QA">
<contactref element="SR-A" pad="15"/>
<contactref element="7SEG-L" pad="5"/>
</signal>
<signal name="SRA-QB">
<contactref element="SR-A" pad="1"/>
<contactref element="7SEG-L" pad="10"/>
</signal>
<signal name="SRA-QC">
<contactref element="SR-A" pad="2"/>
<contactref element="7SEG-L" pad="9"/>
</signal>
<signal name="SRA-QD">
<contactref element="SR-A" pad="3"/>
<contactref element="7SEG-L" pad="1"/>
</signal>
<signal name="SRA-QE">
<contactref element="SR-A" pad="4"/>
<contactref element="7SEG-L" pad="2"/>
</signal>
<signal name="SRA-QF">
<contactref element="SR-A" pad="5"/>
<contactref element="7SEG-L" pad="4"/>
</signal>
<signal name="SRA-QG">
<contactref element="SR-A" pad="6"/>
<contactref element="7SEG-L" pad="6"/>
</signal>
<signal name="SRA-QH">
<contactref element="SR-A" pad="7"/>
<contactref element="7SEG-L" pad="7"/>
</signal>
<signal name="SRA-QH*">
<contactref element="SR-A" pad="9"/>
<contactref element="SR-B" pad="14"/>
</signal>
<signal name="SRB-QA">
<contactref element="SR-B" pad="15"/>
<contactref element="7SEG-R" pad="5"/>
</signal>
<signal name="SRB-QB">
<contactref element="SR-B" pad="1"/>
<contactref element="7SEG-R" pad="10"/>
</signal>
<signal name="SRB-QC">
<contactref element="SR-B" pad="2"/>
<contactref element="7SEG-R" pad="9"/>
</signal>
<signal name="SRB-QD">
<contactref element="SR-B" pad="3"/>
<contactref element="7SEG-R" pad="1"/>
</signal>
<signal name="SRB-QE">
<contactref element="SR-B" pad="4"/>
<contactref element="7SEG-R" pad="2"/>
</signal>
<signal name="SRB-QF">
<contactref element="SR-B" pad="5"/>
<contactref element="7SEG-R" pad="4"/>
</signal>
<signal name="SRB-QG">
<contactref element="SR-B" pad="6"/>
<contactref element="7SEG-R" pad="6"/>
</signal>
<signal name="SRB-QH">
<contactref element="SR-B" pad="7"/>
<contactref element="7SEG-R" pad="7"/>
</signal>
<signal name="SRB-QH*">
<contactref element="SR-B" pad="9"/>
</signal>
<signal name="N$4">
<contactref element="7SEG-L" pad="3"/>
<contactref element="7SEG-L" pad="8"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="BTN-PENALTY" pad="4"/>
<contactref element="BTN-SCORE" pad="4"/>
<contactref element="SR-B" pad="16"/>
<contactref element="SR-A" pad="16"/>
<contactref element="SR-A" pad="10"/>
<contactref element="SR-B" pad="10"/>
<contactref element="JP1" pad="14"/>
</signal>
<signal name="N$7">
<contactref element="7SEG-R" pad="8"/>
<contactref element="7SEG-R" pad="3"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="SER-IN">
<contactref element="SR-A" pad="14"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="CLK">
<contactref element="SR-A" pad="11"/>
<contactref element="SR-B" pad="11"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="LATCH">
<contactref element="SR-A" pad="12"/>
<contactref element="SR-B" pad="12"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="SCORE">
<contactref element="BTN-SCORE" pad="2"/>
<contactref element="JP1" pad="5"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="PENALTY">
<contactref element="BTN-PENALTY" pad="2"/>
<contactref element="JP1" pad="6"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="L-SCORE">
<contactref element="JP1" pad="7"/>
<contactref element="L-SCORE" pad="A"/>
</signal>
<signal name="L-P1">
<contactref element="JP1" pad="8"/>
<contactref element="L-P1" pad="A"/>
</signal>
<signal name="L-P2">
<contactref element="JP1" pad="9"/>
<contactref element="L-P2" pad="A"/>
</signal>
<signal name="R-SCORE">
<contactref element="JP1" pad="10"/>
<contactref element="R-SCORE" pad="A"/>
</signal>
<signal name="R-P1">
<contactref element="JP1" pad="11"/>
<contactref element="R-P1" pad="A"/>
</signal>
<signal name="R-P2">
<contactref element="JP1" pad="12"/>
<contactref element="R-P2" pad="A"/>
</signal>
<signal name="BTN-LED">
<contactref element="JP1" pad="13"/>
<contactref element="BTN-SCORE" pad="A"/>
<contactref element="BTN-PENALTY" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
