<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="2.54" x2="41.91" y2="2.54" width="0.2032" layer="20"/>
<wire x1="41.91" y1="2.54" x2="41.91" y2="49.53" width="0.2032" layer="20"/>
<wire x1="41.91" y1="49.53" x2="0" y2="49.53" width="0.2032" layer="20"/>
<wire x1="0" y1="49.53" x2="0" y2="2.54" width="0.2032" layer="20"/>
<text>BLK</text>
<text>EV SIM 2
ver 1.1</text>
</plain>
<libraries>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="TO220V">
<description>&lt;b&gt;TO 200 vertical&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
</package>
</packages>
</library>
<library name="special">
<description>&lt;b&gt;Special Devices&lt;/b&gt;&lt;p&gt;
7-segment displays, switches, heatsinks, crystals, transformers, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="EDG-04">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO35-7">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2 mm, horizontal, grid 7.62 mm</description>
</package>
<package name="DO41-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-3.5MM-2">
</package>
<package name="1X04">
</package>
<package name="2X3">
</package>
<package name="1X06">
</package>
<package name="POWER_JACK_PTH">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALL">
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="HC49U-V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="linear" package="DIL08" value="LM393N"/>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.3" value="3k"/>
<element name="SW1" library="special" package="EDG-04" value="PILOT"/>
<element name="D1" library="diode" package="DO35-7" value="1N4148"/>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="2.7k"/>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.3" value="330"/>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.3" value="1.3k"/>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k"/>
<element name="C3" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value=".1 uF"/>
<element name="C4" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value=".1 uF"/>
<element name="JP3" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="M023.5MM"/>
<element name="JP4" library="SparkFun-Connectors" package="1X04" value="I2C"/>
<element name="R6" library="SparkFun-Resistors" package="AXIAL-0.3" value="2k"/>
<element name="R7" library="SparkFun-Resistors" package="AXIAL-0.3" value="8.2k"/>
<element name="R8" library="SparkFun-Resistors" package="AXIAL-0.3" value="20k"/>
<element name="C5" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="22 pF"/>
<element name="C6" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="22 pF"/>
<element name="X1" library="crystal" package="HC49U-V" value="20 MHz">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1666969"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="2X3" value="AVR_SPI"/>
<element name="R9" library="SparkFun-Resistors" package="AXIAL-0.3" value="1K"/>
<element name="R10" library="SparkFun-Resistors" package="AXIAL-0.3" value="1K"/>
<element name="R11" library="SparkFun-Resistors" package="AXIAL-0.3" value="1K"/>
<element name="IC3" library="linear" package="TO220V" value="7805"/>
<element name="C1" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value=".1 uF"/>
<element name="C2" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value=".33 uF"/>
<element name="JP1" library="SparkFun-Connectors" package="1X06" value="FTDI"/>
<element name="D2" library="diode" package="DO35-7" value="1N4148"/>
<element name="J1" library="SparkFun-Connectors" package="POWER_JACK_PTH" value="POWER_JACKPTH"/>
<element name="IC2" library="atmel" package="DIL08" value="ATTiny85">
<attribute name="OC_NEWARK" value="96K6523"/>
<attribute name="MPN" value="ATTINY13V-10PU"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9171576"/>
</element>
<element name="U$1" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value=""/>
<element name="D3" library="diode" package="DO41-10" value="1N4004"/>
</elements>
<signals>
<signal name="PILOT_TTL">
<contactref element="IC1" pad="1"/>
<contactref element="R5" pad="P$1"/>
<contactref element="R11" pad="P$1"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="6"/>
<contactref element="SW1" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="IC1" pad="4"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="R6" pad="P$2"/>
<contactref element="R8" pad="P$2"/>
<contactref element="J2" pad="6"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="IC3" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="JP1" pad="6"/>
<contactref element="J1" pad="GNDBREAK"/>
<contactref element="J1" pad="GND"/>
<contactref element="IC2" pad="4"/>
<contactref element="IC2" pad="4"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="+5V">
<contactref element="R5" pad="P$2"/>
<contactref element="R1" pad="P$2"/>
<contactref element="IC1" pad="8"/>
<contactref element="C4" pad="1"/>
<contactref element="JP4" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="R7" pad="P$1"/>
<contactref element="J2" pad="2"/>
<contactref element="IC3" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="JP1" pad="4"/>
<contactref element="IC2" pad="8"/>
</signal>
<signal name="N$2">
<contactref element="SW1" pad="5"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="N$3">
<contactref element="SW1" pad="7"/>
<contactref element="R3" pad="P$2"/>
</signal>
<signal name="N$4">
<contactref element="R4" pad="P$2"/>
<contactref element="SW1" pad="6"/>
</signal>
<signal name="N$5">
<contactref element="R2" pad="P$1"/>
<contactref element="R3" pad="P$1"/>
<contactref element="R4" pad="P$1"/>
<contactref element="SW1" pad="8"/>
<contactref element="D1" pad="A2"/>
</signal>
<signal name="PILOT">
<contactref element="SW1" pad="2"/>
<contactref element="SW1" pad="4"/>
<contactref element="SW1" pad="3"/>
<contactref element="JP3" pad="2"/>
<contactref element="D2" pad="A2"/>
</signal>
<signal name="!RESET">
<contactref element="R1" pad="P$1"/>
<contactref element="J2" pad="5"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="JP4" pad="4"/>
<contactref element="R10" pad="P$2"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="JP4" pad="3"/>
<contactref element="R9" pad="P$2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="IC1" pad="2"/>
<contactref element="R7" pad="P$2"/>
<contactref element="R6" pad="P$1"/>
</signal>
<signal name="N$13">
<contactref element="IC1" pad="3"/>
<contactref element="R8" pad="P$1"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="MOSI">
<contactref element="J2" pad="4"/>
<contactref element="R10" pad="P$1"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="SCK">
<contactref element="J2" pad="3"/>
<contactref element="R9" pad="P$1"/>
<contactref element="IC2" pad="7"/>
</signal>
<signal name="MISO">
<contactref element="J2" pad="1"/>
<contactref element="R11" pad="P$2"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="N$6">
<contactref element="X1" pad="2"/>
<contactref element="X1" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="X1" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="IC3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="J1" pad="PWR"/>
<contactref element="D3" pad="C"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
