<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0.635" y1="2.032" x2="12.065" y2="2.032" width="0" layer="20"/>
<wire x1="12.065" y1="2.032" x2="12.065" y2="13.198" width="0" layer="20"/>
<wire x1="12.065" y1="13.198" x2="0.635" y2="13.198" width="0" layer="20"/>
<wire x1="0.635" y1="13.198" x2="0.635" y2="2.032" width="0" layer="20"/>
</plain>
<libraries>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Microchip_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 11:22:31</description>
<packages>
<package name="DFN492X599X100-9N">
</package>
</packages>
</library>
<library name="Spansion_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 25/07/2012 10:26:07</description>
<packages>
<package name="SOIC127P800X215-8N">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="pinhead" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="pinhead" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="U1" library="Microchip_By_element14_Batch_1" package="DFN492X599X100-9N" value="25AA1024-I/MF">
<attribute name="OC_FARNELL" value="1617312"/>
<attribute name="MPN" value="25AA1024-I/MF"/>
<attribute name="SUPPLIER" value="Microchip"/>
<attribute name="DESCRIPTION" value="EEPROM"/>
<attribute name="PACKAGE" value="DFN-8"/>
<attribute name="OC_NEWARK" value="89H3143"/>
</element>
<element name="U2" library="Spansion_By_element14_Batch_1" package="SOIC127P800X215-8N" value="S25FL064K0SMFI011">
<attribute name="OC_NEWARK" value="27T2974"/>
<attribute name="OC_FARNELL" value="1861631"/>
<attribute name="MPN" value="S25FL064K0SMFI011"/>
<attribute name="SUPPLIER" value="SPANSION"/>
<attribute name="PACKAGE" value="SOIC-8"/>
</element>
</elements>
<signals>
<signal name="N$2">
<contactref element="U1" pad="7"/>
<contactref element="JP1" pad="3"/>
<contactref element="U2" pad="7"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="6"/>
<contactref element="JP1" pad="2"/>
<contactref element="U2" pad="6"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="5"/>
<contactref element="JP1" pad="1"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="3"/>
<contactref element="JP2" pad="2"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="2"/>
<contactref element="JP2" pad="3"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="1"/>
<contactref element="JP2" pad="4"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="GND">
</signal>
<signal name="N$5">
<contactref element="U1" pad="8"/>
<contactref element="JP1" pad="4"/>
<contactref element="U2" pad="8"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="4"/>
<contactref element="JP2" pad="1"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="9"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
