<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.0">
<drawing>
<board>
<plain>
<wire x1="-60.96" y1="-44.45" x2="-33.04" y2="-44.45" width="0" layer="20"/>
<wire x1="-33.04" y1="-44.45" x2="-33.02" y2="78.74" width="0" layer="20"/>
<wire x1="-33.02" y1="78.74" x2="-60.96" y2="78.74" width="0" layer="20"/>
<wire x1="-60.96" y1="78.74" x2="-60.96" y2="-44.45" width="0" layer="20"/>
<text>Gnd</text>
<text>Gnd</text>
<text>Gnd</text>
<text>5v</text>
<text>5v</text>
<text>3v3</text>
<text>3v3</text>
<text>D4</text>
<text>D4</text>
<text>470</text>
<text>WLED</text>
<hole x="-46.99" y="10.16" drill="5.08"/>
<hole x="-46.99" y="68.58" drill="5.08"/>
<text>5v</text>
<text>5v</text>
<text>Gnd</text>
<text>Gnd</text>
<text>Sig</text>
<text>v0.1.0</text>
<text>5v</text>
<text>5v</text>
<text>5v</text>
<text>5v</text>
<text>Gnd</text>
<text>Gnd</text>
<text>Gnd</text>
<text>Gnd</text>
<text>Gnd</text>
<text>3v3</text>
<text>3v3</text>
<text>Sig</text>
<text>D4</text>
<text>D4</text>
<text>470</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>+</text>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
<package name="1X15">
</package>
<package name="1X06">
</package>
<package name="1X01_2MM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="470" library="SparkFun" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="ESP_L" library="SparkFun" package="1X15" value="M15"/>
<element name="ESP_R" library="SparkFun" package="1X15" value="M15"/>
<element name="LL_L" library="SparkFun" package="1X06" value="">
<attribute name="VALUE"/>
</element>
<element name="LL_R" library="SparkFun" package="1X06" value="">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun" package="1X01_2MM" value="M01PTH_2MM"/>
<element name="JP2" library="SparkFun" package="1X01_2MM" value="M01PTH_2MM"/>
<element name="JP3" library="SparkFun" package="1X01_2MM" value="M01PTH_2MM"/>
<element name="JP4" library="SparkFun" package="1X01_2MM" value="M01PTH_2MM"/>
<element name="JP5" library="SparkFun" package="1X01_2MM" value="M01PTH_2MM"/>
<element name="CAP+" library="SparkFun" package="1X01_2MM" value="M01PTH_2MM"/>
<element name="CAP-" library="SparkFun" package="1X01_2MM" value="M01PTH_2MM"/>
</elements>
<signals>
<signal name="3V3">
<contactref element="LL_L" pad="6"/>
<contactref element="ESP_R" pad="1"/>
</signal>
<signal name="5V">
<contactref element="LL_R" pad="6"/>
<contactref element="ESP_L" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP5" pad="1"/>
<contactref element="CAP+" pad="1"/>
</signal>
<signal name="D4">
<contactref element="LL_L" pad="4"/>
<contactref element="ESP_R" pad="11"/>
</signal>
<signal name="DOUT">
<contactref element="LL_R" pad="4"/>
<contactref element="470" pad="2"/>
</signal>
<signal name="GND">
<contactref element="LL_L" pad="5"/>
<contactref element="LL_R" pad="5"/>
<contactref element="ESP_R" pad="9"/>
<contactref element="ESP_L" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="CAP-" pad="1"/>
</signal>
<signal name="SIGNAL">
<contactref element="470" pad="1"/>
<contactref element="JP2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
