<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="1.27" y1="-1.27" x2="15.24" y2="-1.27" width="0" layer="20"/>
<wire x1="16.51" y1="0" x2="16.51" y2="27.94" width="0" layer="20"/>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>L2-</text>
<text>L1-</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>GND</text>
<text>VIN</text>
<wire x1="15.24" y1="29.21" x2="1.27" y2="29.21" width="0" layer="20"/>
<wire x1="0" y1="27.94" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="27.94" x2="1.27" y2="29.21" width="0" layer="20" curve="-90"/>
<wire x1="15.24" y1="29.21" x2="16.51" y2="27.94" width="0" layer="20" curve="-90"/>
<wire x1="15.24" y1="-1.27" x2="16.51" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="-1.27" x2="0" y2="0" width="0" layer="20" curve="-90"/>
<text>RJ45-LED</text>
<text>v1.0</text>
<text>Breakout</text>
<text>RJHSE-548x</text>
</plain>
<libraries>
<library name="LoganSmith-Connectors">
<packages>
<package name="RJ45-RJHSE">
<description>&lt;p&gt;RJHSE-548* footprint&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.digikey.com/product-detail/en/RJHSE-5481/RJHSE-5481-ND/1242705"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="SJ_2">
</package>
<package name="1X06_SQ1">
<description>&lt;p&gt;0.1" spaced header with silkscreen and square pin #1&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="LoganSmith-Resistors">
<packages>
<package name="0805-RES">
<description>&lt;b&gt;0805 Chip Resistor&lt;/b&gt;
&lt;p&gt;Follows standard set in &lt;a href="http://www.tortai-tech.com/upload/download/2011102023233369053.pdf"&gt;IPC-SM-782&lt;/a&gt;, section 8.1 "Chip Resistors", sub-section 5.0 "Land Pattern Dimensions", Figure 3, RLP 102A.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="LoganSmith-Connectors" package="RJ45-RJHSE" value="RJ45-RJHSE-5481">
<attribute name="LED1_COLOR" value="GRN"/>
<attribute name="LED2_COLOR" value="YEL"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="LoganSmith-Resistors" package="0805-RES" value="1k">
<attribute name="MFR" value="Panasonic Electronic Components"/>
<attribute name="MPN" value="ERJ-6GEYJ102V"/>
<attribute name="DIGIKEY_OC" value="P1.0KACT-ND"/>
<attribute name="POWER" value="0.125W"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R2" library="LoganSmith-Resistors" package="0805-RES" value="1k">
<attribute name="MFR" value="Panasonic Electronic Components"/>
<attribute name="MPN" value="ERJ-6GEYJ102V"/>
<attribute name="DIGIKEY_OC" value="P1.0KACT-ND"/>
<attribute name="POWER" value="0.125W"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="SJ1" library="LoganSmith-Connectors" package="SJ_2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ2" library="LoganSmith-Connectors" package="SJ_2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="LoganSmith-Connectors" package="1X06_SQ1" value="">
<attribute name="VALUE"/>
</element>
<element name="J3" library="LoganSmith-Connectors" package="1X06_SQ1" value="">
<attribute name="VALUE"/>
</element>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value="OSHW-LOGOM"/>
</elements>
<signals>
<signal name="N$5">
<contactref element="J1" pad="4"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="J1" pad="3"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="J1" pad="2"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="J1" pad="1"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="LED2+">
<contactref element="J1" pad="LED2+"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="LED1+">
<contactref element="J1" pad="LED1+"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="VIN">
<contactref element="R1" pad="P$2"/>
<contactref element="R2" pad="P$2"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="LED2-">
<contactref element="J1" pad="LED2-"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="LED1-">
<contactref element="J1" pad="LE1D-"/>
<contactref element="J3" pad="6"/>
</signal>
<signal name="GND">
<contactref element="SJ1" pad="2"/>
<contactref element="SJ2" pad="2"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="N$11">
<contactref element="SJ1" pad="1"/>
<contactref element="J1" pad="SHIELD@0"/>
</signal>
<signal name="N$12">
<contactref element="J1" pad="SHEILD@1"/>
<contactref element="SJ2" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="J2" pad="1"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="J2" pad="2"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="J2" pad="3"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="N$4">
<contactref element="J2" pad="4"/>
<contactref element="J1" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
