<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="50.8" y1="3.81" x2="50.8" y2="25.4" width="0" layer="20"/>
<wire x1="0" y1="25.4" x2="0" y2="3.81" width="0" layer="20"/>
<wire x1="0" y1="25.4" x2="50.8" y2="25.4" width="0" layer="20" curve="-40"/>
<wire x1="0" y1="3.81" x2="50.8" y2="3.81" width="0" layer="20" curve="40"/>
<text>Happy</text>
<text>Birth</text>
<text>Day!!!</text>
<text>Pretty
Candles!</text>
<text>Yum, cake!</text>
<text>Mmm frosting...</text>
</plain>
<libraries>
<library name="Texas Instruments_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 17:45:58</description>
<packages>
<package name="SOIC127P600X175-14N">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="Nick">
<packages>
<package name="CR2032_HOLDER">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="1206">
<description>&lt;b&gt;CHICAGO MINIATURE LAMP, INC.&lt;/b&gt;&lt;p&gt;
7022X Series SMT LEDs 1206 Package Size</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="556" library="Texas Instruments_By_element14_Batch_1" package="SOIC127P600X175-14N" value="TLC556CD">
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="OC_NEWARK" value="08F9146"/>
<attribute name="MPN" value="TLC556CD"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
<attribute name="OC_FARNELL" value="1103187"/>
</element>
<element name="R2-2" library="SparkFun-Passives" package="0805" value="47k"/>
<element name="R2-1" library="SparkFun-Passives" package="0805" value="100k"/>
<element name="R1-1" library="SparkFun-Passives" package="0805" value="1k"/>
<element name="R1-2" library="SparkFun-Passives" package="0805" value="1k"/>
<element name="C10" library="SparkFun-Passives" package="0805" value="0.1uF"/>
<element name="C1" library="SparkFun-Passives" package="0805" value="10uF"/>
<element name="C2" library="SparkFun-Passives" package="0805" value="10uF"/>
<element name="BAT1" library="Nick" package="CR2032_HOLDER" value="20mm coincell"/>
<element name="RED" library="adafruit" package="1206" value="">
<attribute name="VALUE"/>
</element>
<element name="YELLOW" library="adafruit" package="1206" value="">
<attribute name="VALUE"/>
</element>
<element name="GREEN" library="adafruit" package="1206" value="">
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Passives" package="0805" value="1.5k"/>
<element name="R7" library="SparkFun-Passives" package="0805" value="1.5k"/>
<element name="R8" library="SparkFun-Passives" package="0805" value="1k"/>
</elements>
<signals>
<signal name="GND">
<contactref element="BAT1" pad="CENTER"/>
<contactref element="556" pad="7"/>
<contactref element="C10" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="RED" pad="C"/>
<contactref element="YELLOW" pad="C"/>
<contactref element="GREEN" pad="C"/>
</signal>
<signal name="VDD">
<contactref element="BAT1" pad="VDD1"/>
<contactref element="556" pad="14"/>
<contactref element="R1-1" pad="2"/>
<contactref element="R1-2" pad="2"/>
<contactref element="BAT1" pad="VDD2"/>
<contactref element="556" pad="4"/>
<contactref element="556" pad="10"/>
</signal>
<signal name="CONT">
<contactref element="C10" pad="2"/>
<contactref element="556" pad="3"/>
<contactref element="556" pad="11"/>
</signal>
<signal name="1TRIGTHRESH">
<contactref element="556" pad="6"/>
<contactref element="556" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="R2-1" pad="2"/>
</signal>
<signal name="2TRIGTHRESH">
<contactref element="556" pad="8"/>
<contactref element="556" pad="12"/>
<contactref element="C2" pad="2"/>
<contactref element="R2-2" pad="2"/>
</signal>
<signal name="1DISCH">
<contactref element="R2-1" pad="1"/>
<contactref element="556" pad="1"/>
<contactref element="R1-1" pad="1"/>
</signal>
<signal name="2DISCH">
<contactref element="R2-2" pad="1"/>
<contactref element="556" pad="13"/>
<contactref element="R1-2" pad="1"/>
</signal>
<signal name="1OUT">
<contactref element="556" pad="5"/>
<contactref element="R6" pad="1"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="2OUT">
<contactref element="556" pad="9"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R6" pad="2"/>
<contactref element="RED" pad="A"/>
</signal>
<signal name="N$10">
<contactref element="R7" pad="2"/>
<contactref element="YELLOW" pad="A"/>
</signal>
<signal name="N$11">
<contactref element="R8" pad="2"/>
<contactref element="GREEN" pad="A"/>
</signal>
<signal name="N$13">
</signal>
<signal name="N$12">
</signal>
</signals>
</board>
</drawing>
</eagle>
