<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="-1.27" y1="0" x2="66.02" y2="0" width="0" layer="20"/>
<wire x1="66.02" y1="0" x2="66.02" y2="69.52" width="0" layer="20"/>
<wire x1="66.02" y1="69.52" x2="-1.27" y2="69.52" width="0" layer="20"/>
<wire x1="-1.27" y1="69.52" x2="-1.27" y2="0" width="0" layer="20"/>
<text>Pool Controller</text>
<text>Roof Temp</text>
<text>Pool Temp</text>
<text>Solar Temp</text>
<text>Solar Monitor</text>
<text>by Jerad Jacob</text>
<text>Display</text>
<text>Stop</text>
<text>Clean</text>
<text>Resume</text>
<text>5vDC 500mA</text>
<text>African Black-footed penguins, although they
cannot fly, can swim up to 25 miles per hour
which is faster than the Atlantic Bottlenosed
dolphin, which can attain speeds of 18-23 mph.</text>
<text>github.com/Here-Be-Dragons</text>
<text>v2.1</text>
<text>P1 P2 P3 P4 P5 P6</text>
<text>Relay pinout on back</text>
<text>RELAY PINOUT:
P1 GND
P2 Solar
P3 Pump Relay 3
P4 Pump Relay 2
P5 Pump Relay 1
P6 VCC (5V)</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="POWER_JACK_PTH">
</package>
<package name="SCREWTERMINAL-5MM-2">
</package>
<package name="1X06">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
</package>
</packages>
</library>
<library name="SparkFun-Sensors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PHOTOCELL">
</package>
</packages>
</library>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are no longer used in our catalog.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Spark">
<packages>
<package name="PHOTON">
</package>
</packages>
</library>
<library name="tft_1.8_1.44_oled_0.96">
<packages>
<package name="OLED_0.96_I2C">
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,0">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.0 mm with drill center</description>
</package>
<package name="2,8">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 2.8 mm with drill center</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="POWER_JACK_PTH" value="POWER_JACKPTH">
<attribute name="PROD_ID" value="CONN-08197"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="Temp_Pool">
<attribute name="STOREFRONT_ID" value="PRT-08432"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="Solar_Mon">
<attribute name="STOREFRONT_ID" value="PRT-08432"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="Temp_Solar">
<attribute name="STOREFRONT_ID" value="PRT-08432"/>
</element>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.3" value="1kΩ"/>
<element name="R10" library="SparkFun-Passives" package="AXIAL-0.3" value="22kΩ"/>
<element name="R12" library="SparkFun-Passives" package="AXIAL-0.3" value="10kΩ"/>
<element name="R14" library="SparkFun-Passives" package="AXIAL-0.3" value="10kΩ"/>
<element name="R2" library="SparkFun-Passives" package="AXIAL-0.3" value="2kΩ"/>
<element name="R3" library="SparkFun-Passives" package="AXIAL-0.3" value="10kΩ"/>
<element name="R4" library="SparkFun-Sensors" package="PHOTOCELL" value="PHOTOCELL"/>
<element name="R5" library="SparkFun-Passives" package="AXIAL-0.3" value="10kΩ"/>
<element name="R6" library="SparkFun-Passives" package="AXIAL-0.3" value="10kΩ"/>
<element name="R7" library="SparkFun-Passives" package="AXIAL-0.3" value="47kΩ"/>
<element name="R8" library="SparkFun-Passives" package="AXIAL-0.3" value="68kΩ"/>
<element name="R9" library="SparkFun-Passives" package="AXIAL-0.3" value="100kΩ"/>
<element name="S1" library="SparkFun-Retired" package="TACTILE-PTH" value="Resume"/>
<element name="S2" library="SparkFun-Retired" package="TACTILE-PTH" value="Clean"/>
<element name="S3" library="SparkFun-Retired" package="TACTILE-PTH" value="Stop"/>
<element name="S4" library="SparkFun-Retired" package="TACTILE-PTH" value="Display Step"/>
<element name="PHOTON" library="Spark" package="PHOTON" value=""/>
<element name="U$2" library="tft_1.8_1.44_oled_0.96" package="OLED_0.96_I2C" value="OLED_0.96_I2C"/>
<element name="U$3" library="holes" package="3,0" value=""/>
<element name="U$4" library="holes" package="3,0" value=""/>
<element name="U$5" library="holes" package="3,0" value=""/>
<element name="U$6" library="holes" package="3,0" value=""/>
<element name="U$1" library="holes" package="2,8" value=""/>
<element name="U$7" library="holes" package="2,8" value=""/>
<element name="J6" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="Temp_Roof">
<attribute name="STOREFRONT_ID" value="PRT-08432"/>
</element>
<element name="R11" library="SparkFun-Passives" package="AXIAL-0.3" value="10kΩ"/>
</elements>
<signals>
<signal name="VIN">
<contactref element="PHOTON" pad="1"/>
</signal>
<signal name="VBAT">
<contactref element="PHOTON" pad="22"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="GNDBREAK"/>
<contactref element="J1" pad="GND"/>
<contactref element="R2" pad="P$2"/>
<contactref element="PHOTON" pad="21"/>
<contactref element="R9" pad="P$2"/>
<contactref element="J3" pad="1"/>
<contactref element="R12" pad="P$1"/>
<contactref element="U$2" pad="GND"/>
<contactref element="PHOTON" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="J5" pad="2"/>
<contactref element="R5" pad="P$1"/>
<contactref element="J6" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="PHOTON" pad="13"/>
<contactref element="U$2" pad="SDA"/>
</signal>
<signal name="N$4">
<contactref element="PHOTON" pad="14"/>
<contactref element="U$2" pad="SCL"/>
</signal>
<signal name="N$5">
<contactref element="R4" pad="2"/>
<contactref element="R5" pad="P$2"/>
<contactref element="PHOTON" pad="12"/>
</signal>
<signal name="5V">
<contactref element="J1" pad="PWR"/>
<contactref element="R1" pad="P$2"/>
<contactref element="U$2" pad="VCC"/>
<contactref element="J3" pad="6"/>
</signal>
<signal name="N$1">
<contactref element="PHOTON" pad="15"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="PHOTON" pad="16"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="N$7">
<contactref element="PHOTON" pad="18"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="PHOTON" pad="19"/>
<contactref element="J4" pad="2"/>
<contactref element="R12" pad="P$2"/>
</signal>
<signal name="N$8">
<contactref element="R7" pad="P$2"/>
<contactref element="S3" pad="4"/>
<contactref element="S3" pad="3"/>
</signal>
<signal name="N$14">
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="S2" pad="1"/>
<contactref element="S2" pad="2"/>
<contactref element="S4" pad="2"/>
<contactref element="S4" pad="1"/>
<contactref element="S3" pad="2"/>
<contactref element="S3" pad="1"/>
<contactref element="R9" pad="P$1"/>
<contactref element="PHOTON" pad="11"/>
</signal>
<signal name="N$6">
<contactref element="J3" pad="3"/>
<contactref element="PHOTON" pad="17"/>
</signal>
<signal name="N$11">
<contactref element="J5" pad="1"/>
<contactref element="R14" pad="P$2"/>
<contactref element="PHOTON" pad="10"/>
</signal>
<signal name="N$12">
<contactref element="PHOTON" pad="9"/>
<contactref element="J2" pad="1"/>
<contactref element="R3" pad="P$2"/>
</signal>
<signal name="3.3V">
<contactref element="R6" pad="P$1"/>
<contactref element="R7" pad="P$1"/>
<contactref element="R8" pad="P$1"/>
<contactref element="R10" pad="P$1"/>
<contactref element="R2" pad="P$1"/>
<contactref element="R1" pad="P$1"/>
<contactref element="PHOTON" pad="24"/>
<contactref element="J4" pad="1"/>
<contactref element="R3" pad="P$1"/>
<contactref element="R14" pad="P$1"/>
<contactref element="R11" pad="P$1"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="R6" pad="P$2"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
</signal>
<signal name="N$10">
<contactref element="R10" pad="P$2"/>
<contactref element="S2" pad="3"/>
<contactref element="S2" pad="4"/>
</signal>
<signal name="N$13">
<contactref element="R8" pad="P$2"/>
<contactref element="S4" pad="3"/>
<contactref element="S4" pad="4"/>
</signal>
<signal name="N$17">
<contactref element="PHOTON" pad="8"/>
<contactref element="J6" pad="1"/>
<contactref element="R11" pad="P$2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
