<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="10.16" x2="23.8" y2="10.16" width="0" layer="20"/>
<wire x1="23.8" y1="10.16" x2="23.8" y2="48.25" width="0" layer="20"/>
<wire x1="23.8" y1="48.25" x2="0" y2="48.25" width="0" layer="20"/>
<wire x1="0" y1="48.25" x2="0" y2="10.16" width="0" layer="20"/>
<text>ILI9341 Touch Connector
roger-parkinson.com
(c) 2016</text>
<text>VCC</text>
<text>GND</text>
<text>CS</text>
<text>RESET</text>
<text>D/C (RS)</text>
<text>SDI (MOSI)</text>
<text>SCK</text>
<text>LED</text>
<text>SDO (MISO)</text>
<text>T_CLK</text>
<text>T_CS</text>
<text>T_DIN</text>
<text>T_DO</text>
<text>T_IRQ</text>
<text>TFT_GND</text>
<text>TFT_YP</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>14</text>
<text>15</text>
<text>16</text>
<text>17</text>
<text>18</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X14">
</package>
</packages>
</library>
<library name="XPT2046-TSSOP-16">
<description>A library for the XPT2046 Touch Controller</description>
<packages>
<package name="TSSOP16-EXPOSED_PAD_MINIMAL">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 16&lt;/b&gt;&lt;p&gt;
MAX3223-MAX3243.pdf</description>
</package>
</packages>
</library>
<library name="TFT18PIN">
<description>TFT ribbon connector with 18 pads
14 pads for the screen and 4 for the touch controller</description>
<packages>
<package name="TFT_18PIN">
</package>
</packages>
</library>
<library name="RT9169">
<description>A library for the RT9169</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
reflow soldering</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP2" library="SparkFun-Connectors" package="1X14" value="">
<attribute name="VALUE"/>
</element>
<element name="XPT2046" library="XPT2046-TSSOP-16" package="TSSOP16-EXPOSED_PAD_MINIMAL" value="XPT2046">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="adafruit" package="R0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="adafruit" package="C0805K" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="TFT18PIN" package="TFT_18PIN" value="TFT_18PIN"/>
<element name="R1" library="adafruit" package="R0805" value="3.9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="adafruit" package="C0805K" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="RT9169" package="SOT23" value="RT9169">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="JP2" pad="2"/>
<contactref element="XPT2046" pad="6"/>
<contactref element="C1" pad="1"/>
<contactref element="U$4" pad="TFT_GND5"/>
<contactref element="U$4" pad="TFT_GND4"/>
<contactref element="U$4" pad="TFT_GND3"/>
<contactref element="U$4" pad="TFT_GND2"/>
<contactref element="U$4" pad="TFT_GND"/>
<contactref element="U$4" pad="TFT_GND1"/>
<contactref element="C2" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="JP2" pad="1"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="TFT_RESET">
<contactref element="JP2" pad="4"/>
<contactref element="U$4" pad="TFT_RESET"/>
</signal>
<signal name="TFT_RS">
<contactref element="JP2" pad="5"/>
<contactref element="U$4" pad="TFT_RS"/>
</signal>
<signal name="TFT_CS">
<contactref element="JP2" pad="3"/>
<contactref element="U$4" pad="TFT_CS"/>
</signal>
<signal name="TFT_SDI">
<contactref element="JP2" pad="6"/>
<contactref element="U$4" pad="TFT_SDI"/>
</signal>
<signal name="TFT_SDO">
<contactref element="JP2" pad="9"/>
<contactref element="U$4" pad="TFT_SDO"/>
</signal>
<signal name="YP">
<contactref element="XPT2046" pad="3"/>
<contactref element="U$4" pad="YP"/>
</signal>
<signal name="TFT_SCK">
<contactref element="JP2" pad="7"/>
<contactref element="U$4" pad="TFT_SCK"/>
</signal>
<signal name="T_CLK">
<contactref element="JP2" pad="10"/>
<contactref element="XPT2046" pad="16"/>
</signal>
<signal name="T_CS">
<contactref element="JP2" pad="11"/>
<contactref element="XPT2046" pad="15"/>
</signal>
<signal name="T_DIN">
<contactref element="JP2" pad="12"/>
<contactref element="XPT2046" pad="14"/>
</signal>
<signal name="T_DO">
<contactref element="JP2" pad="13"/>
<contactref element="XPT2046" pad="12"/>
</signal>
<signal name="T_IRQ">
<contactref element="JP2" pad="14"/>
<contactref element="XPT2046" pad="11"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="XP">
<contactref element="XPT2046" pad="2"/>
<contactref element="U$4" pad="XP"/>
</signal>
<signal name="XN">
<contactref element="XPT2046" pad="4"/>
<contactref element="U$4" pad="XN"/>
</signal>
<signal name="YN">
<contactref element="XPT2046" pad="5"/>
<contactref element="U$4" pad="YN"/>
</signal>
<signal name="VCC3V">
<contactref element="C1" pad="2"/>
<contactref element="XPT2046" pad="1"/>
<contactref element="U$4" pad="VIN3V"/>
<contactref element="XPT2046" pad="9"/>
<contactref element="XPT2046" pad="10"/>
<contactref element="R6" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U$4" pad="LED"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="TFT_LED">
<contactref element="JP2" pad="8"/>
<contactref element="R1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
