<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="50.8" y2="0" width="0" layer="20"/>
<wire x1="50.8" y1="0" x2="50.8" y2="46.0375" width="0" layer="20"/>
<wire x1="50.8" y1="46.0375" x2="0" y2="46.0375" width="0" layer="20"/>
<wire x1="0" y1="46.0375" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="esp8266modules">
<packages>
<package name="ESP12">
<description>ESP8266 Module 12</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CREATIVE_COMMONS">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="POWER_JACK_PTH">
</package>
</packages>
</library>
<library name="Microchip_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 11:22:31</description>
<packages>
<package name="TO170P482X1024X3124-5P">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-10UF-25V">
</package>
</packages>
</library>
<library name="SSR-Board-v10">
<description>Generated from &lt;b&gt;SSR-Board-v10.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="RELAY-S108T02">
</package>
<package name="1X02_LOCK">
</package>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="1X03_LONGPADS">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.1">
</package>
<package name="AXIAL-0.3">
</package>
</packages>
</library>
<library name="furnace_monitor">
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ESP-12" library="esp8266modules" package="ESP12" value="ESP12"/>
<element name="FRAME1" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LETTER"/>
<element name="JP1" library="SparkFun-Connectors" package="POWER_JACK_PTH" value="POWER_JACKPTH">
<attribute name="PROD_ID" value="CONN-08197"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value="4.7uF"/>
<element name="C2" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value="1uF"/>
<element name="SSR1" library="SSR-Board-v10" package="RELAY-S108T02" value=""/>
<element name="HV2" library="SSR-Board-v10" package="1X02_LOCK" value=""/>
<element name="HV1" library="SSR-Board-v10" package="1X02_LOCK" value=""/>
<element name="SSR2" library="SSR-Board-v10" package="RELAY-S108T02" value=""/>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="470">
<attribute name="PROD_ID" value="RES-12183"/>
<attribute name="VALUE" value="10k"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="470">
<attribute name="PROD_ID" value="RES-12183"/>
<attribute name="VALUE" value="10k"/>
</element>
<element name="SERIAL" library="SSR-Board-v10" package="1X03_LONGPADS" value=""/>
<element name="R4" library="SSR-Board-v10" package="AXIAL-0.4" value="11K"/>
<element name="HV_MON1" library="furnace_monitor" package="DIL08" value="MID400"/>
<element name="HV_MON2" library="furnace_monitor" package="DIL08" value="MID400"/>
<element name="R6" library="SparkFun-Resistors" package="AXIAL-0.3" value="5.6k">
<attribute name="PROD_ID" value="RES-12183"/>
<attribute name="VALUE" value="10k"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="AXIAL-0.3" value="5.6k">
<attribute name="PROD_ID" value="RES-12183"/>
<attribute name="VALUE" value="10k"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="AXIAL-0.3" value="4.7k">
<attribute name="PROD_ID" value="RES-12183"/>
<attribute name="VALUE" value="10k"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="AXIAL-0.3" value="4.7k">
<attribute name="PROD_ID" value="RES-12183"/>
<attribute name="VALUE" value="10k"/>
</element>
<element name="C3_1UF" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value=""/>
<element name="SLEEP" library="SSR-Board-v10" package="1X02_LOCK" value="JP2"/>
<element name="POWERREG" library="Microchip_By_element14_Batch_1" package="TO170P482X1024X3124-5P" value="MCP1827">
<attribute name="OC_NEWARK" value="88K5598"/>
<attribute name="PACKAGE" value="TO-220-5"/>
<attribute name="SUPPLIER" value="Microchip"/>
<attribute name="MPN" value="MCP1827-5002E/AT"/>
<attribute name="OC_FARNELL" value="1840847"/>
</element>
<element name="PROG" library="SSR-Board-v10" package="1X02_LOCK" value="JP2"/>
<element name="THERMISTOR1" library="SparkFun-Resistors" package="AXIAL-0.1" value="100K"/>
<element name="JP3" library="SSR-Board-v10" package="1X02_LOCK" value=""/>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-12183"/>
<attribute name="VALUE" value="10k"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-12183"/>
<attribute name="VALUE" value="10k"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-12183"/>
<attribute name="VALUE" value="10k"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-12183"/>
<attribute name="VALUE" value="10k"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="JP1" pad="GNDBREAK"/>
<contactref element="JP1" pad="GND"/>
<contactref element="C1" pad="2"/>
<contactref element="POWERREG" pad="3"/>
<contactref element="C2" pad="2"/>
<contactref element="HV_MON2" pad="5"/>
<contactref element="SSR2" pad="4"/>
<contactref element="SSR1" pad="4"/>
<contactref element="ESP-12" pad="GND"/>
<contactref element="SERIAL" pad="3"/>
<contactref element="R4" pad="P$2"/>
<contactref element="HV_MON1" pad="5"/>
<contactref element="R3" pad="P$1"/>
<contactref element="R5" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="SSR2" pad="2"/>
<contactref element="HV2" pad="1"/>
<contactref element="R6" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="SSR2" pad="1"/>
<contactref element="HV2" pad="2"/>
<contactref element="HV_MON2" pad="3"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="SSR1" pad="2"/>
<contactref element="HV1" pad="1"/>
<contactref element="R7" pad="P$1"/>
</signal>
<signal name="N$7">
<contactref element="SSR1" pad="1"/>
<contactref element="HV1" pad="2"/>
<contactref element="HV_MON1" pad="3"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="SSR1" pad="3"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="N$10">
<contactref element="SSR2" pad="3"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="N$13">
<contactref element="R2" pad="P$1"/>
<contactref element="ESP-12" pad="GPIO4"/>
</signal>
<signal name="N$16">
<contactref element="SERIAL" pad="1"/>
<contactref element="ESP-12" pad="TX"/>
</signal>
<signal name="N$17">
<contactref element="SERIAL" pad="2"/>
<contactref element="ESP-12" pad="RX"/>
</signal>
<signal name="N$11">
<contactref element="ESP-12" pad="GPIO0"/>
<contactref element="PROG" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="R4" pad="P$1"/>
<contactref element="ESP-12" pad="ADC"/>
<contactref element="THERMISTOR1" pad="P$1"/>
</signal>
<signal name="N$22">
<contactref element="HV_MON2" pad="1"/>
<contactref element="R6" pad="P$2"/>
</signal>
<signal name="N$23">
<contactref element="HV_MON1" pad="1"/>
<contactref element="R7" pad="P$2"/>
</signal>
<signal name="N$25">
<contactref element="HV_MON2" pad="6"/>
<contactref element="R9" pad="P$1"/>
<contactref element="ESP-12" pad="GPIO12"/>
</signal>
<signal name="N$26">
<contactref element="HV_MON1" pad="6"/>
<contactref element="R10" pad="P$1"/>
<contactref element="ESP-12" pad="GPIO13"/>
</signal>
<signal name="N$27">
<contactref element="C1" pad="1"/>
<contactref element="JP1" pad="PWR"/>
<contactref element="POWERREG" pad="2"/>
<contactref element="POWERREG" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="ESP-12" pad="RESET"/>
<contactref element="SLEEP" pad="2"/>
</signal>
<signal name="N$28">
<contactref element="ESP-12" pad="GPIO16"/>
<contactref element="C3_1UF" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="C3_1UF" pad="2"/>
<contactref element="SLEEP" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="ESP-12" pad="GPIO14"/>
<contactref element="THERMISTOR1" pad="P$2"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="P$1"/>
<contactref element="ESP-12" pad="GPIO5"/>
</signal>
<signal name="+3V3">
<contactref element="POWERREG" pad="4"/>
<contactref element="C2" pad="1"/>
<contactref element="ESP-12" pad="VCC"/>
<contactref element="R9" pad="P$2"/>
<contactref element="HV_MON2" pad="8"/>
<contactref element="HV_MON1" pad="8"/>
<contactref element="R10" pad="P$2"/>
<contactref element="R8" pad="P$1"/>
<contactref element="R11" pad="P$2"/>
</signal>
<signal name="N$9">
<contactref element="ESP-12" pad="GPIO15"/>
<contactref element="R3" pad="P$2"/>
</signal>
<signal name="N$12">
<contactref element="PROG" pad="1"/>
<contactref element="R5" pad="P$2"/>
</signal>
<signal name="N$14">
<contactref element="ESP-12" pad="GPIO2"/>
<contactref element="R8" pad="P$2"/>
</signal>
<signal name="N$15">
<contactref element="R11" pad="P$1"/>
<contactref element="ESP-12" pad="CH_PD"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
