<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="6.35" y1="12.065" x2="6.35" y2="20.955" width="0" layer="20"/>
<wire x1="6.35" y1="20.955" x2="5.715" y2="21.59" width="0" layer="20" curve="90"/>
<wire x1="5.715" y1="21.59" x2="3.175" y2="21.59" width="0" layer="20"/>
<wire x1="2.54" y1="34.925" x2="3.175" y2="35.56" width="0" layer="20" curve="-90"/>
<wire x1="3.175" y1="35.56" x2="19.685" y2="35.56" width="0" layer="20"/>
<wire x1="19.685" y1="35.56" x2="20.32" y2="34.925" width="0" layer="20" curve="-90"/>
<wire x1="20.32" y1="34.925" x2="20.32" y2="22.225" width="0" layer="20"/>
<wire x1="19.685" y1="21.59" x2="17.145" y2="21.59" width="0" layer="20"/>
<wire x1="17.145" y1="21.59" x2="16.51" y2="20.955" width="0" layer="20" curve="90"/>
<wire x1="16.51" y1="20.955" x2="16.51" y2="12.065" width="0" layer="20"/>
<wire x1="16.51" y1="12.065" x2="15.875" y2="11.43" width="0" layer="20" curve="-90"/>
<wire x1="15.875" y1="11.43" x2="6.985" y2="11.43" width="0" layer="20"/>
<wire x1="6.985" y1="11.43" x2="6.35" y2="12.065" width="0" layer="20" curve="-90"/>
<wire x1="2.54" y1="34.925" x2="2.54" y2="22.225" width="0" layer="20"/>
<wire x1="2.54" y1="22.225" x2="3.175" y2="21.59" width="0" layer="20" curve="90"/>
<wire x1="19.685" y1="21.59" x2="20.32" y2="22.225" width="0" layer="20" curve="90"/>
<text>RESET</text>
<text>TX</text>
<text>RX</text>
<text>CONN</text>
<text>3.3V</text>
<text>GND</text>
<text>XTAL1</text>
<text>XTAL2</text>
<text>BG312L</text>
<text>BG312L 
Bluetooth Low Energy
v1.0 @joewalnes</text>
</plain>
<libraries>
<library name="BLE">
<packages>
<package name="BG312L">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
</packages>
</library>
<library name="E-test-solutions (11)">
<packages>
<package name="LOGO-10MM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="BLE" package="BG312L" value="BG213L"/>
<element name="JP2" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="E-test-solutions (11)" package="LOGO-10MM" value=""/>
</elements>
<signals>
<signal name="RX">
<contactref element="U$1" pad="P1_7/RX"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="TX">
<contactref element="U$1" pad="P1_6/TX"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="RESET">
<contactref element="U$1" pad="RESET"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="VDD">
<contactref element="U$1" pad="VDD_1"/>
<contactref element="U$1" pad="VDD_2"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="OSC2">
<contactref element="U$1" pad="X_OSC2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="OSC1">
<contactref element="U$1" pad="X_OSC1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="GND_1"/>
<contactref element="U$1" pad="GND_2"/>
<contactref element="U$1" pad="GND_3"/>
<contactref element="U$1" pad="GND_4"/>
<contactref element="U$1" pad="GND_5"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="CONNECTED">
<contactref element="U$1" pad="P0_7"/>
<contactref element="JP2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
