<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<board>
<plain>
<wire x1="38.735" y1="70.485" x2="38.735" y2="26.3525" width="0" layer="20"/>
<wire x1="38.735" y1="26.3525" x2="17.78" y2="26.3525" width="0" layer="20"/>
<wire x1="17.78" y1="26.3525" x2="17.78" y2="70.485" width="0" layer="20"/>
<wire x1="17.78" y1="70.485" x2="38.735" y2="70.485" width="0" layer="20"/>
</plain>
<libraries>
<library name="con-harting-ml">
<description>&lt;b&gt;Harting  &amp; 3M Connectors&lt;/b&gt;&lt;p&gt;
Low profile connectors, straight&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="ML26">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-3m-skt-header">
<description>&lt;h1 align=center&gt;&lt;b&gt;3M PCB Sockets (Reverse of standard Plugs)&lt;/b&gt;&lt;/h1&gt;
&lt;h2 align=center&gt;Reverse IDC connectors&lt;/h2&gt;
&lt;p align=right&gt;Version 1.1 - &amp;nbsp; 3&lt;sup&gt;rd&lt;/sup&gt; August 2012&lt;/p&gt;
&lt;p&gt;Created by Paul Carpenter of &lt;B&gt;PC Services&lt;/B&gt;, Reading, UK., updates to this library can also be obtained from the PC Services website
&lt;a href="http://www.pcserviceselectronics.co.uk/"&gt;www.pcserviceselectronics.co.uk&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;These sockets are the 3M &lt;b&gt;Series 5100 (horizontal) and 8500 (vertical) sockets;&lt;/b&gt; PCB sockets on 0.1in pitch double row for mating with standard centrebump polarised 0.1in pitch, double row ribbon cable connectors.&lt;/p&gt;
&lt;center&gt;
&lt;TABLE BORDER=1 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;caption align=center&gt;&lt;b&gt;Part Number and Library Name&lt;/b&gt;&lt;/caption&gt;
  &lt;TR align=center bgcolor=yellow&gt;
    &lt;td rowspan=2 valign=bottom&gt;Pins&lt;/td&gt;
    &lt;TD colspan=2&gt;Vertical&lt;/td&gt;
    &lt;TD colspan=2&gt;Horizontal&lt;/td&gt;
  &lt;/TR&gt;
  &lt;tr align=center bgcolor=cyan&gt;
    &lt;TD&gt;Part Number&lt;/td&gt;
    &lt;TD&gt;Library Name&lt;/td&gt;
    &lt;TD&gt;Part Number&lt;/td&gt;
    &lt;TD&gt;Library Name&lt;/td&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;10&lt;/td&gt;
    &lt;TD bgcolor=cyan&gt;8510-4500&lt;/td&gt;
    &lt;TD&gt;SKT10V&lt;/td&gt;
    &lt;TD&gt; - &lt;/td&gt;
    &lt;TD&gt; - &lt;/td&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;16&lt;/td&gt;
    &lt;TD bgcolor=cyan&gt;8516-4500&lt;/td&gt;
    &lt;TD&gt;SKT16V&lt;/td&gt;
    &lt;TD&gt; - &lt;/td&gt;
    &lt;TD&gt; - &lt;/td&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;20&lt;/td&gt;
    &lt;TD bgcolor=cyan&gt;8520-4500&lt;/td&gt;
    &lt;TD&gt;SKT20V&lt;/td&gt;
    &lt;TD bgcolor=cyan&gt;5120-B7A2&lt;/td&gt;
    &lt;TD&gt;SKT20H&lt;/td&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;26&lt;/td&gt;
    &lt;TD bgcolor=cyan&gt;8526-4500&lt;/td&gt;
    &lt;TD&gt;SKT26V&lt;/td&gt;
    &lt;TD bgcolor=cyan&gt;5126-B7A2&lt;/td&gt;
    &lt;TD&gt;SKT26H&lt;/td&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;30&lt;/td&gt;
    &lt;TD&gt; - &lt;/td&gt;
    &lt;TD&gt; - &lt;/td&gt;
    &lt;TD bgcolor=cyan&gt;5130-B7A2&lt;/td&gt;
    &lt;TD&gt;SKT30H&lt;/td&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;34&lt;/td&gt;
    &lt;TD bgcolor=cyan&gt;8534-4500&lt;/td&gt;
    &lt;TD&gt;SKT34V&lt;/td&gt;
    &lt;TD bgcolor=cyan&gt;5134-B7A2&lt;/td&gt;
    &lt;TD&gt;SKT34H&lt;/td&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;40&lt;/td&gt;
    &lt;TD bgcolor=cyan&gt;8540-4500&lt;/td&gt;
    &lt;TD&gt;SKT40V&lt;/td&gt;
    &lt;TD bgcolor=cyan&gt;5140-B7A2&lt;/td&gt;
    &lt;TD&gt;SKT40H&lt;/td&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;50&lt;/td&gt;
    &lt;TD bgcolor=cyan&gt;8550-4500&lt;/td&gt;
    &lt;TD&gt;SKT50V&lt;/td&gt;
    &lt;TD bgcolor=cyan&gt;5150-B7A2&lt;/td&gt;
    &lt;TD&gt;SKT50H&lt;/td&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;60&lt;/td&gt;
    &lt;TD bgcolor=cyan&gt;8560-4500&lt;/td&gt;
    &lt;TD&gt;SKT60V&lt;/td&gt;
    &lt;TD bgcolor=cyan&gt;5160-B7A2&lt;/td&gt;
    &lt;TD&gt;SKT60H&lt;/td&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;64&lt;/td&gt;
    &lt;TD bgcolor=cyan&gt;8564-4500&lt;/td&gt;
    &lt;TD&gt;SKT64V&lt;/td&gt;
    &lt;TD bgcolor=cyan&gt;5164-B7A2&lt;/td&gt;
    &lt;TD&gt;SKT64H&lt;/td&gt;
  &lt;/TR&gt;
&lt;/table&gt;</description>
<packages>
<package name="S26V">
<description>26 pin Vertical PCB Socket 8526-xxxxx</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="SV1" library="con-3m-skt-header" package="S26V" value="SCSI Controller"/>
<element name="SV3" library="con-harting-ml" package="ML26" value="Mega ST DMA">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="SV1" pad="2"/>
<contactref element="SV1" pad="6"/>
<contactref element="SV1" pad="10"/>
<contactref element="SV1" pad="14"/>
<contactref element="SV3" pad="20"/>
<contactref element="SV3" pad="1"/>
<contactref element="SV3" pad="5"/>
<contactref element="SV3" pad="7"/>
<contactref element="SV3" pad="9"/>
<contactref element="SV3" pad="13"/>
<contactref element="SV3" pad="15"/>
<contactref element="SV3" pad="17"/>
<contactref element="SV3" pad="21"/>
</signal>
<signal name="CS">
<contactref element="SV1" pad="17"/>
<contactref element="SV3" pad="18"/>
</signal>
<signal name="IRQ">
<contactref element="SV1" pad="19"/>
<contactref element="SV3" pad="24"/>
</signal>
<signal name="RESET">
<contactref element="SV1" pad="4"/>
<contactref element="SV3" pad="3"/>
</signal>
<signal name="ACK">
<contactref element="SV1" pad="8"/>
<contactref element="SV3" pad="11"/>
</signal>
<signal name="A1">
<contactref element="SV1" pad="12"/>
<contactref element="SV3" pad="19"/>
</signal>
<signal name="RW">
<contactref element="SV1" pad="16"/>
<contactref element="SV3" pad="22"/>
</signal>
<signal name="DRQ">
<contactref element="SV1" pad="18"/>
<contactref element="SV3" pad="23"/>
</signal>
<signal name="D7">
<contactref element="SV1" pad="15"/>
<contactref element="SV3" pad="16"/>
</signal>
<signal name="D6">
<contactref element="SV1" pad="13"/>
<contactref element="SV3" pad="14"/>
</signal>
<signal name="D5">
<contactref element="SV1" pad="11"/>
<contactref element="SV3" pad="12"/>
</signal>
<signal name="D4">
<contactref element="SV1" pad="9"/>
<contactref element="SV3" pad="10"/>
</signal>
<signal name="D3">
<contactref element="SV1" pad="7"/>
<contactref element="SV3" pad="8"/>
</signal>
<signal name="D2">
<contactref element="SV1" pad="5"/>
<contactref element="SV3" pad="6"/>
</signal>
<signal name="D1">
<contactref element="SV1" pad="3"/>
<contactref element="SV3" pad="4"/>
</signal>
<signal name="D0">
<contactref element="SV1" pad="1"/>
<contactref element="SV3" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
