<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<board>
<plain>
<wire x1="-1.524" y1="27.686" x2="54.915" y2="27.686" width="0" layer="20"/>
<wire x1="54.915" y1="27.686" x2="54.915" y2="71.364" width="0" layer="20"/>
<wire x1="54.915" y1="71.364" x2="-1.524" y2="71.364" width="0" layer="20"/>
<wire x1="-1.524" y1="71.364" x2="-1.524" y2="27.686" width="0" layer="20"/>
<text>GND</text>
<text>REF</text>
<text>REF</text>
<text>GND</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>14</text>
<text>15</text>
<text>16</text>
<text>17</text>
<text>18</text>
<text>19</text>
<text>20</text>
<text>21</text>
<text>22</text>
<text>23</text>
<text>24</text>
<text>25</text>
<text>26</text>
<text>27</text>
<text>28</text>
<text>29</text>
<text>30</text>
<text>31</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>Intan RHD2132 breakout</text>
<text>v2   10/2017</text>
<text>evan_matteson@brown.edu</text>
</plain>
<libraries>
<library name="open-ephys">
<packages>
<package name="NPD-36-VV-GS">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="open-ephys" package="NPD-36-VV-GS" value="NPD-36-VV-GS"/>
<element name="J1" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J7" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J8" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J9" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J10" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J11" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J12" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J13" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J14" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J15" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J16" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J17" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J18" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J19" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J20" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J21" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J22" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J23" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J24" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J25" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J26" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J27" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J28" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J29" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J30" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J31" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J32" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J33" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J34" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J35" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J36" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$2">
<contactref element="U$1" pad="P$2"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="P$3"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="P$4"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="P$5"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="P$6"/>
<contactref element="J6" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="P$7"/>
<contactref element="J7" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="P$8"/>
<contactref element="J8" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="P$9"/>
<contactref element="J9" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="U$1" pad="P$10"/>
<contactref element="J10" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="P$11"/>
<contactref element="J11" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="U$1" pad="P$12"/>
<contactref element="J12" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="U$1" pad="P$13"/>
<contactref element="J13" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="U$1" pad="P$14"/>
<contactref element="J14" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="U$1" pad="P$15"/>
<contactref element="J15" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="U$1" pad="P$16"/>
<contactref element="J16" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="U$1" pad="P$17"/>
<contactref element="J17" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="U$1" pad="P$18"/>
<contactref element="J18" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="U$1" pad="P$36"/>
<contactref element="J36" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="U$1" pad="P$35"/>
<contactref element="J35" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="U$1" pad="P$34"/>
<contactref element="J34" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="U$1" pad="P$33"/>
<contactref element="J33" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="U$1" pad="P$32"/>
<contactref element="J32" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="U$1" pad="P$31"/>
<contactref element="J31" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="U$1" pad="P$30"/>
<contactref element="J30" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="U$1" pad="P$29"/>
<contactref element="J29" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="U$1" pad="P$28"/>
<contactref element="J28" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="U$1" pad="P$27"/>
<contactref element="J27" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="U$1" pad="P$26"/>
<contactref element="J26" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="U$1" pad="P$25"/>
<contactref element="J25" pad="1"/>
</signal>
<signal name="N$31">
<contactref element="U$1" pad="P$24"/>
<contactref element="J24" pad="1"/>
</signal>
<signal name="N$32">
<contactref element="U$1" pad="P$23"/>
<contactref element="J23" pad="1"/>
</signal>
<signal name="N$33">
<contactref element="U$1" pad="P$22"/>
<contactref element="J22" pad="1"/>
</signal>
<signal name="N$34">
<contactref element="U$1" pad="P$21"/>
<contactref element="J21" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="U$1" pad="P$20"/>
<contactref element="J20" pad="1"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="1"/>
<contactref element="U$1" pad="P$1"/>
<contactref element="U$1" pad="P$19"/>
<contactref element="J19" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
