<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="14" width="0" layer="20"/>
<wire x1="100" y1="14" x2="0" y2="14" width="0" layer="20"/>
<wire x1="0" y1="14" x2="0" y2="0" width="0" layer="20"/>
<text>Geppetto
Electronics</text>
<text>+</text>
<text>+</text>
<text>Magic Trackpad
Plugger</text>
<text>-</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="SOT23-5L">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;&lt;p&gt;
package type OT</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01">
</package>
<package name="1X02">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="adafruit" package="SOT23-5L" value="LP298XS"/>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="1 µF"/>
<element name="C2" library="SparkFun-Capacitors" package="0805" value=".01 µF"/>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="2.2 µF"/>
<element name="JP1" library="SparkFun-Connectors" package="1X01" value="+OUT"/>
<element name="JP2" library="SparkFun-Connectors" package="1X01" value="GND"/>
<element name="JP3" library="SparkFun-Connectors" package="1X02" value="USB POWER">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="C1" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="C2" pad="1"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="5"/>
<contactref element="C3" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
