<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="53.34" y2="0" width="0.2032" layer="20"/>
<wire x1="53.34" y1="0" x2="53.34" y2="70.612" width="0.2032" layer="20"/>
<wire x1="53.34" y1="70.612" x2="0" y2="70.612" width="0.2032" layer="20"/>
<wire x1="0" y1="70.612" x2="0" y2="0" width="0.2032" layer="20"/>
<text>+</text>
<text>+5v</text>
<text>+3v3</text>
<text>A14/DAC</text>
<text>Vbat</text>
<text>24</text>
<text>25</text>
<text>26</text>
<text>27</text>
<text>28</text>
<text>29</text>
<text>30</text>
<text>31</text>
<text>32</text>
<text>33</text>
<text>A12</text>
<text>A13</text>
<text>A10</text>
<text>A11</text>
<text>Aref</text>
<text>VUSB</text>
<text>A7</text>
<text>A9</text>
<text>A8</text>
<text>A0</text>
<text>A1</text>
<text>A2</text>
<text>A3</text>
<text>A4</text>
<text>A5</text>
<text>A6</text>
<text>0</text>
<text>1</text>
<text>Vin</text>
<text>Agnd</text>
<text>InfoGauge</text>
<text>Controlled
Surrouncings 
Inc.</text>
<text>c '16</text>
<text>O</text>
<text>v.048gb</text>
<text>Controlled Surroundings Inc.</text>
<text>Dash Lts.</text>
<text>1Wire</text>
<text>Bat1</text>
<text>Bat2</text>
<text>Gnd</text>
<text>+5v</text>
<text>+</text>
<text>c  '16</text>
<text>O</text>
<text>REMOVE</text>
<text>RE</text>
<text>RE</text>
<text>RE</text>
<text>RE</text>
<text>RE</text>
<text>RE</text>
<text>RE</text>
<text>RE</text>
<text>RE</text>
<text>RE</text>
<text>RE</text>
<text>RE</text>
<text>RE</text>
<text>RE</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="FIDUCIAL-1X2">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
<package name="SOD-323F">
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="microbuilder">
<packages>
<package name="MOUNTINGHOLE_2.0_PLATED">
</package>
<package name="_0805">
<description>&lt;b&gt;0805&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Z_adafruit">
<packages>
<package name="1X2-3.5MM">
</package>
<package name="SMADIODE">
<description>&lt;b&gt;SMA Surface Mount Diode&lt;/b&gt;</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-3.5MM-3">
</package>
<package name="1X01">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BUZZER-CCV">
</package>
</packages>
</library>
<library name="Z_MAR">
<packages>
<package name="RJ45-8">
</package>
<package name="SMA">
</package>
<package name="SOT-363">
</package>
</packages>
</library>
<library name="Teensy3.0">
<packages>
<package name="TEENSY_3.2_BITES_NORESET">
</package>
</packages>
</library>
<library name="Z_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X12_LOCK_LONGPADS">
</package>
<package name="ARDUINO-BD-2.8LCD">
</package>
<package name="1X07_LOCK">
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP4" library="SparkFun" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="JP6" library="SparkFun" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="C1" library="adafruit" package="C0805K" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="adafruit" package="C0805K" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="R0805" value="22k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="R0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="adafruit" package="R0805" value="22k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="adafruit" package="R0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="Z_adafruit" package="1X2-3.5MM" value="1X2-3.5MM">
<attribute name="NAME"/>
</element>
<element name="D3" library="adafruit" package="SOD-323F" value="1n4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="adafruit" package="SOD-323F" value="1n4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$9" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0"/>
<element name="U$10" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0"/>
<element name="JP7" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="adafruit" package="C0805K" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="adafruit" package="C0805K" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="microbuilder" package="_0805" value="0.01µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="microbuilder" package="_0805" value="0.01µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SG1" library="SparkFun-Electromechanical" package="BUZZER-CCV" value="BUZZERSMD2"/>
<element name="J2" library="Z_adafruit" package="1X2-3.5MM" value="1X2-3.5MM">
<attribute name="NAME"/>
</element>
<element name="R7" library="adafruit" package="R0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="Z_MAR" package="RJ45-8" value="RJ45-8"/>
<element name="R1" library="adafruit" package="R0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="Teensy3.0" package="TEENSY_3.2_BITES_NORESET" value="TEENSY_3.1-3.23.2_NO-RESET"/>
<element name="JP12" library="Z_SparkFun" package="1X12_LOCK_LONGPADS" value="M12LOCK_LONGPADS">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R39" library="adafruit" package="R0805" value="1.8k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R40" library="adafruit" package="R0805" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R41" library="adafruit" package="R0805" value="1.8k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R42" library="adafruit" package="R0805" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R43" library="adafruit" package="R0805" value="1.8k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R44" library="adafruit" package="R0805" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R45" library="adafruit" package="R0805" value="1.8k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R46" library="adafruit" package="R0805" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R47" library="adafruit" package="R0805" value="1.8k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R48" library="adafruit" package="R0805" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R49" library="adafruit" package="R0805" value="1.8k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R50" library="adafruit" package="R0805" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R51" library="adafruit" package="R0805" value="1.8k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R52" library="adafruit" package="R0805" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R53" library="adafruit" package="R0805" value="1.8k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R54" library="adafruit" package="R0805" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R55" library="adafruit" package="R0805" value="1.8k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R56" library="adafruit" package="R0805" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R57" library="adafruit" package="R0805" value="1.8k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R58" library="adafruit" package="R0805" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R59" library="adafruit" package="R0805" value="1.8k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R60" library="adafruit" package="R0805" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R61" library="adafruit" package="R0805" value="1.8k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R62" library="adafruit" package="R0805" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R63" library="adafruit" package="R0805" value="1.8k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R64" library="adafruit" package="R0805" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R65" library="adafruit" package="R0805" value="1.8k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R66" library="adafruit" package="R0805" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="R0805" value="1.8k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="adafruit" package="R0805" value="3.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="adafruit" package="R0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X01" value="M01PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ZD4" library="Z_MAR" package="SMA" value="3.3vZ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ZD6" library="Z_MAR" package="SMA" value="3.3vZ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D18" library="Z_adafruit" package="SMADIODE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D19" library="Z_adafruit" package="SMADIODE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="Z_adafruit" package="R1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F2" library="Z_adafruit" package="R1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$11" library="Z_SparkFun" package="ARDUINO-BD-2.8LCD" value="ARDUINO-2.8LCD"/>
<element name="JP2" library="Z_SparkFun" package="1X07_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="Z_SparkFun" package="1X07_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$13" library="Z_MAR" package="SOT-363" value="DIOD_3X_SD103"/>
<element name="U$14" library="Z_MAR" package="SOT-363" value="DIOD_3X_SD103"/>
<element name="U$15" library="Z_MAR" package="SOT-363" value="DIOD_3X_SD103"/>
<element name="U$16" library="Z_MAR" package="SOT-363" value="DIOD_3X_SD103"/>
<element name="U$17" library="Z_MAR" package="SOT-363" value="DIOD_3X_SD103"/>
<element name="U$18" library="Z_MAR" package="SOT-363" value="DIOD_3X_SD103"/>
<element name="U$19" library="Z_MAR" package="SOT-363" value="DIOD_3X_SD103"/>
<element name="U$20" library="Z_MAR" package="SOT-363" value="DIOD_3X_SD103"/>
<element name="U$21" library="Z_MAR" package="SOT-363" value="DIOD_3X_SD103"/>
<element name="U$22" library="Z_MAR" package="SOT-363" value="DIOD_3X_SD103"/>
<element name="JP5" library="SparkFun-Connectors" package="1X01" value="M01PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP8" library="SparkFun-Connectors" package="1X01" value="M01PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="Z_SparkFun" package="SOT23" value="MMBT2222">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="adafruit" package="R0805" value="180r">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="5V_REG" library="Z_SparkFun" package="SOT223" value="V_REG_MIC2920"/>
<element name="3.3VREG" library="Z_SparkFun" package="SOT223" value="V_REG_MIC2920"/>
</elements>
<signals>
<signal name="GND">
<contactref element="R4" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="U$1" pad="5"/>
<contactref element="JP7" pad="3"/>
<contactref element="U$2" pad="GND"/>
<contactref element="U$2" pad="GND"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="R54" pad="2"/>
<contactref element="R56" pad="2"/>
<contactref element="R58" pad="2"/>
<contactref element="R60" pad="2"/>
<contactref element="R62" pad="2"/>
<contactref element="R64" pad="2"/>
<contactref element="R66" pad="2"/>
<contactref element="R40" pad="2"/>
<contactref element="R42" pad="2"/>
<contactref element="R44" pad="2"/>
<contactref element="R46" pad="2"/>
<contactref element="R48" pad="2"/>
<contactref element="R50" pad="2"/>
<contactref element="R52" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="ZD6" pad="A"/>
<contactref element="ZD4" pad="A"/>
<contactref element="U$11" pad="GND@1"/>
<contactref element="U$11" pad="GND@0"/>
<contactref element="U$11" pad="GND@2"/>
<contactref element="U$13" pad="4"/>
<contactref element="U$14" pad="6"/>
<contactref element="U$14" pad="5"/>
<contactref element="U$14" pad="4"/>
<contactref element="U$13" pad="6"/>
<contactref element="U$13" pad="5"/>
<contactref element="U$16" pad="4"/>
<contactref element="U$15" pad="6"/>
<contactref element="U$15" pad="5"/>
<contactref element="U$15" pad="4"/>
<contactref element="U$17" pad="6"/>
<contactref element="U$17" pad="5"/>
<contactref element="U$17" pad="4"/>
<contactref element="U$16" pad="6"/>
<contactref element="U$16" pad="5"/>
<contactref element="Q2" pad="2"/>
<contactref element="5V_REG" pad="2"/>
<contactref element="5V_REG" pad="4"/>
<contactref element="3.3VREG" pad="2"/>
<contactref element="3.3VREG" pad="4"/>
</signal>
<signal name="1WIRE">
<contactref element="U$2" pad="2"/>
<contactref element="JP7" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="LTS">
<contactref element="R7" pad="2"/>
<contactref element="U$2" pad="6"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="+3V3">
<contactref element="U$2" pad="3.3V"/>
<contactref element="C2" pad="1"/>
<contactref element="ZD4" pad="K"/>
<contactref element="U$11" pad="3.3V"/>
<contactref element="U$19" pad="1"/>
<contactref element="U$18" pad="3"/>
<contactref element="U$18" pad="2"/>
<contactref element="U$18" pad="1"/>
<contactref element="U$19" pad="3"/>
<contactref element="U$19" pad="2"/>
<contactref element="U$22" pad="1"/>
<contactref element="U$22" pad="2"/>
<contactref element="U$22" pad="3"/>
<contactref element="U$21" pad="1"/>
<contactref element="U$21" pad="2"/>
<contactref element="U$21" pad="3"/>
<contactref element="U$20" pad="1"/>
<contactref element="U$20" pad="2"/>
<contactref element="U$20" pad="3"/>
<contactref element="SG1" pad="+"/>
<contactref element="3.3VREG" pad="3"/>
</signal>
<signal name="+5V">
<contactref element="D4" pad="C"/>
<contactref element="D3" pad="C"/>
<contactref element="JP7" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="ZD6" pad="K"/>
<contactref element="U$11" pad="5V"/>
<contactref element="U$2" pad="VIN"/>
<contactref element="5V_REG" pad="3"/>
<contactref element="3.3VREG" pad="1"/>
</signal>
<signal name="D5">
<contactref element="U$2" pad="5"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R7" pad="1"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="BAT2">
<contactref element="R3" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="D19" pad="C"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="D7">
<contactref element="U$2" pad="7"/>
<contactref element="R8" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="U$17" pad="3"/>
<contactref element="U$21" pad="4"/>
</signal>
<signal name="AGND">
<contactref element="U$2" pad="AGND"/>
</signal>
<signal name="AREF">
<contactref element="U$2" pad="AREF"/>
</signal>
<signal name="VUSB">
<contactref element="U$2" pad="VUSB"/>
</signal>
<signal name="D3">
<contactref element="U$2" pad="3"/>
<contactref element="U$11" pad="D3"/>
</signal>
<signal name="D4">
<contactref element="U$2" pad="4"/>
<contactref element="U$11" pad="D4"/>
</signal>
<signal name="D8">
<contactref element="U$2" pad="8"/>
<contactref element="U$11" pad="D8"/>
</signal>
<signal name="D9">
<contactref element="U$2" pad="9"/>
<contactref element="U$11" pad="D9"/>
</signal>
<signal name="D10">
<contactref element="U$2" pad="10"/>
<contactref element="U$11" pad="D10"/>
</signal>
<signal name="D11">
<contactref element="U$2" pad="11"/>
<contactref element="U$11" pad="D11"/>
</signal>
<signal name="D12">
<contactref element="U$2" pad="12"/>
<contactref element="U$11" pad="D12"/>
</signal>
<signal name="D13">
<contactref element="U$2" pad="13"/>
<contactref element="U$11" pad="D13"/>
</signal>
<signal name="D31">
<contactref element="U$2" pad="31"/>
<contactref element="JP12" pad="9"/>
</signal>
<signal name="D30">
<contactref element="U$2" pad="30"/>
<contactref element="JP12" pad="10"/>
</signal>
<signal name="D29">
<contactref element="U$2" pad="29"/>
<contactref element="JP12" pad="11"/>
</signal>
<signal name="D28">
<contactref element="U$2" pad="28"/>
<contactref element="JP12" pad="12"/>
</signal>
<signal name="D27">
<contactref element="U$2" pad="27"/>
<contactref element="JP12" pad="6"/>
</signal>
<signal name="D26">
<contactref element="U$2" pad="26"/>
<contactref element="JP12" pad="5"/>
</signal>
<signal name="D25">
<contactref element="U$2" pad="25"/>
<contactref element="JP12" pad="4"/>
</signal>
<signal name="D24">
<contactref element="U$2" pad="24"/>
<contactref element="JP12" pad="3"/>
</signal>
<signal name="VCC">
<contactref element="D18" pad="C"/>
<contactref element="R5" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="5V_REG" pad="1"/>
</signal>
<signal name="D33">
<contactref element="U$2" pad="33"/>
<contactref element="JP12" pad="7"/>
</signal>
<signal name="D1">
<contactref element="U$2" pad="1"/>
<contactref element="JP12" pad="2"/>
</signal>
<signal name="A6">
<contactref element="R40" pad="1"/>
<contactref element="R39" pad="2"/>
<contactref element="U$2" pad="20/A6"/>
<contactref element="U$16" pad="1"/>
<contactref element="U$20" pad="6"/>
</signal>
<signal name="A5">
<contactref element="R42" pad="1"/>
<contactref element="R41" pad="2"/>
<contactref element="U$2" pad="19/A5"/>
<contactref element="U$16" pad="2"/>
<contactref element="U$20" pad="5"/>
</signal>
<signal name="A4">
<contactref element="R44" pad="1"/>
<contactref element="R43" pad="2"/>
<contactref element="U$2" pad="18/A4"/>
<contactref element="U$16" pad="3"/>
<contactref element="U$20" pad="4"/>
</signal>
<signal name="A3">
<contactref element="R46" pad="1"/>
<contactref element="R45" pad="2"/>
<contactref element="U$2" pad="17/A3"/>
<contactref element="U$15" pad="1"/>
<contactref element="U$22" pad="6"/>
</signal>
<signal name="A2">
<contactref element="R48" pad="1"/>
<contactref element="R47" pad="2"/>
<contactref element="U$2" pad="16/A2"/>
<contactref element="U$15" pad="2"/>
<contactref element="U$22" pad="5"/>
</signal>
<signal name="A1">
<contactref element="R50" pad="1"/>
<contactref element="R49" pad="2"/>
<contactref element="U$2" pad="15/A1"/>
<contactref element="U$17" pad="1"/>
<contactref element="U$21" pad="6"/>
</signal>
<signal name="A0">
<contactref element="R52" pad="1"/>
<contactref element="R51" pad="2"/>
<contactref element="U$2" pad="14/A0"/>
<contactref element="U$17" pad="2"/>
<contactref element="U$21" pad="5"/>
</signal>
<signal name="A13">
<contactref element="R54" pad="1"/>
<contactref element="R53" pad="2"/>
<contactref element="U$2" pad="A13"/>
<contactref element="U$13" pad="2"/>
<contactref element="U$18" pad="5"/>
</signal>
<signal name="A12">
<contactref element="R56" pad="1"/>
<contactref element="R55" pad="2"/>
<contactref element="U$2" pad="A12"/>
<contactref element="U$13" pad="3"/>
<contactref element="U$18" pad="4"/>
</signal>
<signal name="A11">
<contactref element="R58" pad="1"/>
<contactref element="R57" pad="2"/>
<contactref element="U$2" pad="A11"/>
<contactref element="U$13" pad="1"/>
<contactref element="U$18" pad="6"/>
</signal>
<signal name="A10">
<contactref element="R60" pad="1"/>
<contactref element="R59" pad="2"/>
<contactref element="U$2" pad="A10"/>
<contactref element="U$14" pad="3"/>
<contactref element="U$19" pad="4"/>
</signal>
<signal name="A9">
<contactref element="R62" pad="1"/>
<contactref element="R61" pad="2"/>
<contactref element="U$2" pad="23/A9"/>
<contactref element="U$14" pad="1"/>
<contactref element="U$19" pad="6"/>
</signal>
<signal name="A8">
<contactref element="R64" pad="1"/>
<contactref element="R63" pad="2"/>
<contactref element="U$2" pad="22/A8"/>
<contactref element="U$14" pad="2"/>
<contactref element="U$19" pad="5"/>
</signal>
<signal name="N$77">
<contactref element="R51" pad="1"/>
<contactref element="U$1" pad="1"/>
<contactref element="U$11" pad="A3"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$78">
<contactref element="R49" pad="1"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$11" pad="A2"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$79">
<contactref element="R47" pad="1"/>
<contactref element="U$1" pad="3"/>
<contactref element="U$11" pad="A1"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="N$80">
<contactref element="R45" pad="1"/>
<contactref element="U$11" pad="A0"/>
<contactref element="JP2" pad="4"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="N$81">
<contactref element="R43" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="D4" pad="A"/>
<contactref element="U$11" pad="A4"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="N$82">
<contactref element="R41" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="D3" pad="A"/>
<contactref element="U$11" pad="A5"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="N$83">
<contactref element="R39" pad="1"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="N$86">
<contactref element="R55" pad="1"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$87">
<contactref element="R61" pad="1"/>
<contactref element="JP3" pad="7"/>
</signal>
<signal name="N$88">
<contactref element="R59" pad="1"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="D32">
<contactref element="U$2" pad="32"/>
<contactref element="JP12" pad="8"/>
</signal>
<signal name="D0">
<contactref element="JP12" pad="1"/>
<contactref element="U$2" pad="0"/>
</signal>
<signal name="N$5">
<contactref element="R63" pad="1"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="N$6">
<contactref element="R53" pad="1"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="R65" pad="1"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="R57" pad="1"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="N$22">
<contactref element="U$1" pad="8"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="J2" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="D19" pad="A"/>
<contactref element="F2" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="F1" pad="2"/>
<contactref element="D18" pad="A"/>
</signal>
<signal name="BAT1">
<contactref element="F1" pad="1"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="J4" pad="2"/>
<contactref element="F2" pad="1"/>
</signal>
<signal name="A7">
<contactref element="R66" pad="1"/>
<contactref element="R65" pad="2"/>
<contactref element="U$2" pad="21/A7"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="A14/DAC"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="VBAT">
<contactref element="JP8" pad="1"/>
<contactref element="U$2" pad="VBAT"/>
</signal>
<signal name="N$4">
<contactref element="Q2" pad="3"/>
<contactref element="SG1" pad="-"/>
</signal>
<signal name="N$11">
<contactref element="R10" pad="1"/>
<contactref element="Q2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
